Natural Global Buffer Pool Manager Messages

#### Search Results

Search

# Natural Global Buffer Pool Manager Messages

This section contains the informational and error messages issued by the Natural Global buffer pool manager under z/OS.

All messages have the format:

`GBPnnnn xxxxxxxx: message text`

- where:

- nnnn is the message number.

- xxxxxxxx is the job name, under which the Natural global buffer pool is running.

For ease of use, the job name message portion has been omitted in the following list of messages. Notation in italics indicates a variable message portion.

The following topics are covered below:

- Natural Global Buffer Pool Manager Syntax Error Messages

- Natural Global Buffer Pool Manager Run-Time Messages

- Natural Global Buffer Pool Manager Driver Messages

## Natural Global Buffer Pool Manager Syntax Error Messages

The Natural global buffer pool manager syntax error messages are self-explanatory with xxxx being the invalid command or parameter.

For appropriate command and parameter syntax, refer to Natural Global buffer pool manager under z/OS in the Operations documentation of Natural for Mainframes.

Message Number | Message Text
--- | ---
GBP0001 | Invalid command: xxxx
GBP0002 | More than one command specified
GBP0003 | Invalid parameter keyword: xxxx
GBP0004 | Buffer pool name parameter missing
GBP0005 | Invalid buffer pool name: xxxx
GBP0006 | Leading parenthesis missing in NATBUFFER
GBP0007 | Ending parenthesis missing in NATBUFFER
GBP0008 | Buffer pool size not numeric: xxxx
GBP0009 | Buffer pool size less than 100K: xxxx
GBP0010 | Buffer pool size too large: xxxx
GBP0011 | Invalid MODE specified: xxxx
GBP0012 | Text block size not numeric: xxxx
GBP0013 | Text block size must be 1,2,4,8,12 or 16, not xxxx
GBP0014 | Invalid buffer pool type: xxxx
GBP0015 | Invalid preload list name: xxxx
GBP0016 | Invalid sub-system ID: xxxx
GBP0017 | IDLE time not numeric: xxxx
GBP0018 | IDLE time out of valid range: xxxx
GBP0019 | Buffer pool cache size not numeric: xxxx
GBP0020 | Buffer pool cache size out of valid range: xxxx
GBP0021 | RESIDENT must be Y or N or A, not xxxx
GBP0022 | METHOD must be S or N, not xxxx
GBP0023 | CONFIRM must be Y or N, not xxxx
GBP0024 | PLUGIN must be BP or NOBP, not xxxx
GBP0025 | REGISTER must be Y or N, not xxxx
GBP0026 | NAT buffer pool size less than 256K: xxxx
GBP0029 | CC must be Y or N, not xxxx

## Natural Global Buffer Pool Manager Run-Time Messages

In the following table, error-info format is:

failing function (macro), sub-function, request return (RC) or cancel code (CC), request failure reason code

Please see the relevant IBM documentation for an explanation of the return or abend codes of the relevant IBM request macro.

Message Number | Message Text
--- | ---
GBP0000 | xxxx (dummy message consisting only of a variable message part)
GBP0098 | Parameter module missing or invalid: pgm-name
GBP0099 | Message text module missing or invalid: pgm-name
GBP0100 | No parameters specified
GBP0101 | Specified parms: xxxx
GBP0102 | Operator input: xxxx
GBP0103 | Input from file: xxxx
GBP0104 | Mandatory module missing or invalid: pgm-name
GBP0105 | Storage could not be obtained: xxxx
GBP0106 | FREEMAIN not successful
GBP0107 | NAME/TOKEN service failure: error-info
GBP0108 | Buffer pool manager module incompatible: pgm-name
GBP0109 | Pool (de)allocation failure: error-info
GBP0110 | GBP not active: gbp-name/subsid
GBP0111 | GBP active: gbp-name/subsid - DIR=dir-addr ADDR=gbp-addr
GBP0112 | GBP refreshed: gbp-name/subsid - DIR=dir-addr ADDR=gbp-addr
GBP0113 | GBP stopped: gbp-name/subsid - DIR=dir-addr ADDR=gbp-addr
GBP0114 | GBP already active: gbp-name/subsid - DIR=dir-addr ADDR=gbp-addr
GBP0115 | GBP still in use: gbp-name/subsid - DIR=dir-addr ADDR=gbp-addr
GBP0116 | Associated GBP has been lost gbp-name/subsid
GBP0117 | Shutdown forced for GBP gbp-name/subsid
GBP0118 | Reply Y to force shutdown of GBP gbp-name/subsid
GBP0119 | Shutdown aborted, reply was x
GBP0120 | Creating cache for GBP: gbp-name/subsid
GBP0121 | Deleting cache for GBP: gbp-name/subsid
GBP0122 | GBP cache creation failure: error-info
GBP0123 | GBP cache deletion failure: error-info
GBP0124 | Data Space: GBP cache created: cache-name, cache-token, cache-ALET, KEY Memory Object (above the bar): GBP cache created: MEMOBJ, address, cache-token, size, KEY
GBP0125 | Data Space: GBP cache deleted: cache-name, cache-token, cache-ALET Memory Object (above the bar): GBP cache deleted: MEMOBJ, address
GBP0126 | ALET stack overflow. Cannot create GBP cache
GBP0127 | Cache already exists for GBP: gbp-name/subsid
GBP0128 | No cache available for GBP: gbp-name/subsid
GBP0129 | GBP cache not owned by job job-name
GBP0130 | No global buffer pool available for SUBSID: subsid
GBP0131 | List of all global buffer pools with SUBSID: subsid
GBP0132 | BP-Name/SUBSID Size(KB) A(GBP) A(DIR) Cache-ALET/ADDR----- Size-Owner--- Key
GBP0133 | About to shutdown the following global buffer pools
GBP0134 | Reply Y to continue shutdown of global buffer pools
GBP0135 | No global buffer pool matching selection criteria
GBP0136 | Job does not own GBP cache(s)
GBP0137 | GBP cache(s) owned by job job-name
GBP0138 | Data space cache not supported in non-ESA environment
GBP0139 | GBP(s) owned by job: job-name
GBP0140 | RESIDENT=N ignored due to owning GBP cache(s):
GBP0141 | TERMINATE aborted due to owning GBP cache(s):
GBP0142 | RESIDENT=N ignored due to owning GBP(s):
GBP0143 | TERMINATE aborted due to owning GBP(s):
GBP0144 | GBP not allocated due to user key pool not possible
GBP0145 | Global parameter settings: xxxx
GBP0149 | Service request failure: service, error-info
GBP0150 | Formatted dump
GBP0151 | Formatted dump for GBP gbp-name/subsid
GBP0154 | Global buffer pool manager not operational
GBP0158 | Bad retcode from NATBPMG4, function REINIT: rtc
GBP0159 | Bad retcode from NATBPMG4, function INIT: rtc
GBP0197 | No Zaps applied
GBP0198 | Applied Zaps:
GBP0199 | Natural Global Buffer Pool Manager Version: xxxx

## Natural Global Buffer Pool Manager Driver Messages

In the following table, error-info format is:

failing function (macro), sub-function, request return (RC) or cancel code (CC), request failure reason code

Please see the relevant IBM documentation for an explanation of the return or abend codes of the relevant IBM request macro.

The following messages are listed below:

- Messages Issued by the Global Buffer Pool Manager Operating-system-dependent Driver Modules

- Messages Issued by the Global Buffer Pool Manager z/OS Driver Module

### Messages Issued by the Global Buffer Pool Manager Operating-system-dependent Driver Modules

Message Number | Message Text
--- | ---
GBP0200 | Specified file does not exist: file-name
GBP0201 | Reading parm input from file file-name
GBP0202 | EOF encountered reading file file-name
GBP0203 | Error reading file file-name
GBP0204 | Subsystem storage protection feature is required
GBP0205 | Insufficient authorization: error-info
GBP0206 | Job cancelled by operator
GBP0207 | Job cancelled due to unrecoverable abend abend-code

### Messages Issued by the Global Buffer Pool Manager z/OS Driver Module

Message Number | Message Text
--- | ---
GBP0300 | Sorry, z/OS is required
GBP0301 | Only `MODIFY` or `STOP` commands allowed
GBP0302 | `STOP` command received from operator
GBP0303 | GBP allocated in system key due to `ALLOWUSERKEYCSA(NO)`

### On this page

- Natural Global Buffer Pool Manager Syntax Error Messages
- Natural Global Buffer Pool Manager Run-Time Messages
- Natural Global Buffer Pool Manager Driver Messages