RM - Retransmit Modified Fields

#### Search Results

Search

# RM - Retransmit Modified Fields

This Natural profile parameter controls the retransmission of modified fields.

Possible settings | `ON` | Natural always sends back all modified fields.
`OFF` | Natural sends back modified fields only if they have been changed.
Default setting | `OFF` |
Dynamic specification | yes |
Specification within session | no |

Notes:

1. Some TP monitors translate input data automatically to upper-case characters.
2. As Natural's screen optimization only retransmits modified data back to the screen, the TP-monitor translation may cause input for a field which has been modified not to be retransmitted.