Natural for VSAM Interface Abend Codes

#### Search Results

Search

# Natural for VSAM Interface Abend Codes

This section lists the abend codes that may be issued by the Natural for VSAM.

Natural for VSAM abend codes are 2-digit numbers preceded by `NV`.

Abend Code | Explanation
--- | ---
Miscellaneous:
NV01 | Unexpected internal error.
NV02 | Too many nested groups in view.
NV03 | Error in view scan.
NV07 | Internal buffer handling error.
NV09 | NVS upgrade processing failed for an ESDS file.
NV10 | Relocation error.
NV11 | Roll-out error.
NV12 | System file processing: corrupted variable record, field length is zero.
NV13 | Roll-in error.
NV15 | Unexpected error for DDM buffer pool handling.
NV16 | Unexpected error from Routine `NATSEFA`.
NV18 | Unexpected error for `PATH=CHECK` or `RLS=CHECK` processing.
Natural for VSAM Initialization:
NV20 | Unexpected FREEMAIN error.
I/O Module NVSMISC:
NV30 | Invalid I/O request (DCR).
NV31 | ENDREQ error.
NV32 | RPL active by I/O request.
NV33 | FREEMAIN error (physical).
NV34 | GENCB/MODCB ACB error.
NV35 | GENCB/MODCB RPL error.
NV36 | SHOWCB error.
NV38 | AIX upgrade error for path processing.
NV39 | FWA queue full.
NV40 | FWA entry not found.
NV41 | Internal error (`NTOPRB`/`OPRB`).
NV42 | Unexpected error for BACKWARD processing.
I/O Module NVSCICS:
NV60 | Internal error (DCRREQCD invalid).
NV61 | Internal error (FREEMAIN failed).
NV62 | Corrupted exec interface block (EIB).
NV64 | Internal error (`*NUMBER`).
NV65 | FWA queue full.
NV66 | FWA entry not found.
NV67 | Unexpected error for BACKWARD processing.