Roll Server Messages

#### Search Results

Search

# Roll Server Messages

This section lists the messages that may be issued by the Natural Roll Server. Unlike Natural system messages, the explanatory long texts to these messages and codes are only available in this document, not online.

For information on the Roll Server, see:

- Natural Roll Server Functionality

- Natural Roll Server Operation

In addition, refer to the relevant IBM documents mentioned below.

## RSM0001 - Subsystem ID invalid

Explanation | A subsystem ID was specified that is longer than 4 characters.
Action | Specify a subsystem ID of 1 to 4 characters.

## RSM0002 - Roll file number not numeric

Explanation | The second parameter is not a number.
Action | Specify a valid number,

## RSM0003 - Invalid number of roll files

Explanation | A number greater than 5 was specified.
Action | Specify a number between 0 and 5.

## RSM0004 - Number of LRB slots not specified

Explanation | The third parameter was omitted.
Action | This is a mandatory parameter. Specify a valid number.

## RSM0005 - Number of LRB slots not numeric

Explanation | The third parameter is not a number.
Action | Specify a valid number.

## RSM0006 - Number of LRB slots > 32767

Explanation | The number of LRB slots specified is too large.
Action | Specify a maximum of 32767 LRB slots.

## RSM0007 - Invalid CF structure name

Explanation | A structure name of more than 16 characters was specified.
Action | Specify a structure name of 16 characters or less.

## RSM0008 - Bad return code from IEANTRT: rc

Explanation | The Name/Token Service returned return code rc.
Action | See the current IBM MVS Programming: Authorized Assembler Services Reference manual for information about the return code from the `IEANTRT` request.

## RSM0009 - DCB buffer could not be obtained. Reason: reasoncode

Explanation | A `STORAGE OBTAIN` request failed with reasoncode.
Action | Increase virtual storage available to the Roll Server. (`REGION` option of the JCL `EXEC` statement.)

## RSM0010 - OPEN failed for DDNAME: ddname

Explanation | The roll file specified under `DDNAME` ddname could not be opened.
Action | Specify a valid roll file DSN.

## RSM0011 - Duplicate roll file DSN

Explanation | The same DSN was specified for two roll file `DDNAME`s.
Action | Specify unique DSNs for each roll file.

## RSM0012 - Temp roll file buffer could not be obtained. Reason: reasoncode

Explanation | A `STORAGE OBTAIN` request failed with reasoncode.
Action | Increase virtual storage available to the Roll Server. (`REGION` option of the JCL `EXEC` statement.)

## RSM0013 - RF directory buffer could not be obtained. Reason: reasoncode

Explanation | A `STORAGE OBTAIN` request failed with reasoncode.
Action | Increase virtual storage available to the Roll Server. (`REGION` option of the JCL `EXEC` statement.)

## RSM0014 - LRB directory could not be obtained. Reason: reasoncode

Explanation | A `STORAGE OBTAIN` request failed with reasoncode.
Action | Increase virtual storage available to the Roll Server. (`REGION` option of the JCL `EXEC` statement.)

## RSM0015 - Unrecognized parameter or invalid value in parameter file

Explanation | An unknown keyword or invalid parameter value was found in the parameter file.
Action | Correct the parameter file.

## RSM0017 - Size for LRB > 524287 blocks

Explanation | The number of LRB slots times LRB slot size exceeds 2 Gigabytes.
Action | Specify fewer LRB slots or a smaller slot size.

## RSM0018 - LX table could not be obtained. Reason: reasoncode

Explanation | A `STORAGE OBTAIN` request failed with `reasoncode`.
Action | Increase virtual storage available to the Roll Server. (`REGION` option of the JCL `EXEC` statement.)

## RSM0019 - Roll Server Version vrs is active

Where vrs represents the relevant product version (see also Version in the Glossary).

Explanation | The Roll Server initialized successfully and is ready for work.
Action | None.

## RSM0020 - Subtask terminated: taskname rc

Explanation | The subtask indicated by `taskname` has terminated. If the return code is not zero, it is indicated as `rc`.
Action | If a nonzero `rc` is reported, contact Software AG Support.

## RSM0021 - Subtask termination initiated

Explanation | In response to a `TERM` or `DEAL` operator command, the Roll Server has started to terminate its subtasks.
Action | None.

## RSM0022 - All subtasks terminated

Explanation | In response to a `TERM` or `DEAL` operator command, the process of terminating the subtasks is finished.
Action | None.

## RSM0023 - Other than MODIFY or STOP command received

Explanation | The Roll Server received a `CIBVERB` other than `MODIFY` or `STOP`.
Action | Contact Software AG Support.

## RSM0026 - Command allowed in active state only: command

Explanation | In deallocated (`DEAL`) state, the Roll Server cannot accept operator command command.
Action | Issue the `START` operator command, then repeat the rejected command.

## RSM0027 - Unknown command command

Explanation | An invalid operator command was issued to the Roll Server.
Action | Check for typing error and correct.

## RSM0029 - Recursive abend in maintask. Now waiting for CANCEL command

Explanation | An abend occurred during abend recovery.
Action | Cancel the Roll Server started task and contact Software AG Support.

## RSM0030 - Low Water Mark not numeric or invalid

Explanation | The sixth parameter is not a number or exceeds 10.
Action | Specify a low water mark between 0 and 10.

## RSM0031 - High Water Mark not numeric or invalid

Explanation | The seventh parameter is not a number or exceeds 10.
Action | Specify a high water mark between 0 and 10.

## RSM0032 - Too few/many parameters for command

Explanation | The number of parameters is not the one that has been expected.
Action | Correct the number of parameters.

## RSM0033 - All resources deallocated

Explanation | In response to a `DEAL` (deallocate) operator command, the Roll Server is now in deallocated state.
Action | None.

## RSM0036 - DUMP successful for roll file n

Explanation | Slots from the Local Roll Buffer and the Roll File Directory were successfully written to Roll File n on disk.
Action | None.

## RSM0037 - DUMP failed for roll file n

Explanation | The Roll Server was unable to write slots and directory to Roll File n.
Action | Look for accompanying messages indicating the error situation that prevented a successful dump.

## RSM0038 - SNAP failed. Task RB could not be obtained

Explanation | A `STORAGE OBTAIN` request failed.
Action | Increase virtual storage available to the Roll Server. (`REGION` option of the JCL `EXEC` statement.)

## RSM0039 - XES functions not available

Explanation | Environmental error. XES functions are not available. This can occur because the coupling facility hardware necessary to provide XES functions is not present.
Action | Re-IPL the system or contact IBM.

## RSM0040 - IXLCONN unsuccessful. Reason code: reasoncode

Explanation | A connection to the Coupling Facility structure specified as fifth parameter could not be established.
Action | Determine the meaning of the reason code in the IBM document z/OS Programming: Sysplex Services Reference and follow the indicated action.

## RSM0041 - CF initialization successful for list: n

Explanation | The Roll File Directory for Roll File n was established in the list structure specified as fifth parameter.
Action | None.

## RSM0042 - CF initialization failed for list/RSN code: reasoncode

Explanation | The Roll File Directory for Roll File n could not be established in the list structure specified as fifth parameter. The reason codes are as follows:
`12` | `STORAGE OBTAIN` failed.
`16` | An abend occurred during initialization.
`20` | The Structure is allocated too small to hold the Roll File Directory.
`24` | Structure failure or connectivity lost.
Action | For Reason Code 12: | Increase virtual storage available to the Roll Server. (`REGION` option of the JCL `EXEC` statement.)
For Reason Code 16: | Contact Software AG Support.
For Reason Code 20: | Define a larger size for the CF structure in the CFRM policy.
For Reason Code 24: | Reset the structure using operator command `SETXCF FORCE,STR,STRNAME=name`. If the error persists, contact IBM.

## RSM0043 - IXCJOIN failed. Return/Reason code: reasoncode

Explanation | The Roll Server could not join its IXC message group.
Action | Determine the meaning of the reason code in the IBM document z/OS Programming: Sysplex Services Reference and follow the indicated action.

## RSM0044 - Act conn buffer could not be obtained

Explanation | A `STORAGE OBTAIN` request failed.
Action | Increase virtual storage available to the Roll Server. (`REGION` option of the JCL `EXEC` statement.)

## RSM0045 - Applied zaps:

Explanation | When Zaps are applied to the Roll Server, it issues this message, followed by a list of applied zaps.
Action | None.

## RSM0046 - Roll file in use by job jobname ASID asid

Explanation | The Roll Server cannot start because another Roll Server is using a roll file. The other Roll Server is running in job or started task named `jobname` with address space identifier `asid`. The message is followed by the roll file's DSN.
Action | Ensure that all Roll Servers have dedicated roll files.

## RSM0047 - Operator command: command

Explanation | The Roll Server echoes operator commands to `JESMSGLG`.
Action | None.

## RSM0048 - IARV64 GETSTOR failed. Return code: rc

Explanation | The Roll Server uses Memory Objects for the Local Roll Buffers. The Memory Objects are acquired using the IARV64 services. A `GETSTOR` function failed.
Action | Determine the action in the IARV64 description in the current IBM document MVS Programming: Authorized Assembler Services Reference manual.

## RSM0049 - Disconnected from CF with RSN=FAILURE

Explanation | The Roll Server disconnected from the Coupling Facility structure with parameter `REASON=FAILURE` in order to notify other participating Roll Servers of its own termination with failure.
Action | None.

## RSM0050 - Disconnected from CF with RSN=NORMAL

Explanation | The Roll Server disconnected from the Coupling Facility structure with parameter `REASON=NORMAL` in order to notify other participating Roll Servers of its own normal termination.
Action | None.

## RSM0051 - Roll file n is newer than the CF structure

Explanation | A roll file was newly formatted, but the Coupling Facility structure still contains its Roll File Directory.
Action | After formatting a roll file, re-initialize the CF structure using operator command `SETXCF FORCE,STR,STRNAME=name`

## RSM0052 - Not enough storage for IARV64 GETSTOR - Increase MEMLIMIT

Explanation | Not enough memory in Memory Objects could be allocated to hold the Local Roll Buffer(s). The allocatable amount is controlled by the `MEMLIMIT` parameter of the JCL `EXEC` statement and SMF exit `IEFUSI`.
Action | Increase the amount of usable storage in the `MEMLIMIT` parameter, or change the `IEFUSI` exit.

## RSM0053 - Not enough memory for SNAP

Explanation | A SNAP dump could not be taken because a `STORAGE OBTAIN` request failed.
Action | Increase virtual storage available to the Roll Server. (`REGION` option of the JCL `EXEC` statement.)

## RSM0054 - OPEN for SYSUDUMP failed

Explanation | A SNAP dump could not be taken because `SYSUDUMP` could not be opened.
Action | Ensure that the Roll Server job or started task includes a DD statement for `SYSUDUMP`.

## RSM0055 - CF structure does not contain enough lists

Explanation | For each roll file, the Roll Server maintains its directory in a separate list in the CF structure. The existing structure has fewer lists than the number of roll files to be used.
Action | Re-initialize the CF structure using operator command `SETXCF FORCE,STR,STRNAME=name`, or use fewer roll files.

## RSM0056 - LRB slotsize invalid or not numeric

Explanation | The fourth parameter is either not numeric or greater than `10000000`.
Action | Correct typing error or specify a smaller LRB slot size.

## RSM0057 - Bad return code from IEANTCR: rc

Explanation | The Name/Token Service denied a create request with return code rc.
Action | Determine the action from the description of `IEANTCR` in the current IBM document MVS Programming: Authorized Assembler Services Reference manual.

## RSM0058 - Rollserver already active in subsid: Job jobname ASID asid

Explanation | The Roll Server determined that in the Natural subsystem specified in the first parameter, `subsid`, another Roll Server is already active. The other Roll Server is running in job or started task named `jobname`, with address space identifier `asid`.
Action | Start only one Roll Server per Natural subsystem per MVS image.

## RSM0059 - Roll file ddname is below version 412

Explanation | The roll file specified in `ddname` has an incompatible format.
Action | Reformat the roll file using `NATRSRFI`. See Natural Roll Server Operation in the Natural Operations documentation.

## RSM0060 - User exit loaded: NATRSU14

Explanation | User exit `NATRSU14` is loaded and will be called to allocate users to roll files.
Action | None.

## RSM0061 - Slot size must be specified when no roll files are used

Explanation | When running without roll files, a default value for the LRB slot size cannot be determined.
Action | Specify LRB slot size as fourth parameter.

## RSM0062 - Running with in-core roll file

Explanation | The second parameter specified `0` for the number of roll files. Natural threads are held in Local Roll Buffer slots only and are lost when the Roll Server terminates.
Action | None.

## RSM0063 - Coupling Facility will not be used

Explanation | The second parameter specified `0` for the number of roll files, yet the fifth parameter specified a CF structure. To enable Natural to run on several MVS images in a Parallel Sysplex, the Roll Server needs to use roll files. Operation continues without roll files, but the Roll Server will not communicate with other Roll Servers in other MVS images.
Action | Specify roll files in a Parallel Sysplex, or do not specify a CF structure name with zero roll files.

## RSM0064 - High/low water marks ignored

Explanation | The second parameter specified `0` for the number of roll files, yet low or high watermarks were also specified. With no roll files, low and high watermark are meaningless. Operation continues.
Action | Do not specify watermarks with zero roll files.

## RSM0065 - XES Event exit received unexpected event type: nn

Explanation | The exit for the connection to the CF structure received an event type that it cannot handle. `nn` is the number corresponding to the event type.
Action | Contact Software AG Support.

## RSM0066 - REBUILD Start: CF structure temporarily unavailable

Explanation | Operator command `SETXCF START,REBUILD…` was issued for the Coupling Facility Structure that holds the Roll File Directory. Roll Server operation is quiesced until the Rebuild operation is complete.
Action | None.

## RSM0067 - REBUILD End: CF structure available again

Explanation | Operator command `SETXCF START,REBUILD…` was issued for the Coupling Facility Structure that holds the Roll File Directory. Rebuild is now complete and the Roll Server resumes normal operation.
Action | None.

## RSM0068 - LRB slot size parameter ignored

Explanation | When running with roll files, the roll file slot size determines the LRB slot size.
Action | Specify this parameter only when running without roll file.

## RSM0069 - Invalid non-activity time

Explanation | The eighth start-up parameter (or `TIMEOUT NAT` command) is not numeric or greater than `10000000`.
Action | Specify a valid number.

## RSM0070 - Invalid timeout check time

Explanation | The nineth start-up parameter (or `TIMEOUT TOC` command) is not numeric or not a valid time of day.
Action | Specify a valid time of the form h, hh, hhm, or hhmm

## RSM0072 - Timeout processing starting

Explanation | The routine to detect and delete non-active sessions is running.
Action | None.

## RSM0073 - Scheduled/Operator timeout processing deleted n sessions

Explanation | Timeout check has detected and deleted n sessions that had been inactive longer than the non-activity time specified as start-up parameter or with the `TIMEOUT NAT` command. Operator timeout processing was requested by the operator command `TIMEOUT NOW` while scheduled timeout processing was run according to the parameter settings.
Action | None.

## RSM0074 - Timeout processing ended with return code rc

Explanation | The routine to detect and delete non-active sessions has ended with return code `rc`. In case of return code 12, `rc` takes the form `rc/rsn`, where `rsn` is the reason code.
Action | Check in Return Codes and Reason Codes of the Roll Server Requests for an explanation of the return and reason code, and action to be taken.

## RSM0075 - TIMEOUT ON/NOW rejected: No valid timeout parameters

Explanation | No valid non-activity time and/or no valid timeout-check-time has been specified before this command was issued.
Action | For `TIMEOUT ON`, either specify non-activity time and timeout-check-time as start-up parameters, or precede the command with `TIMEOUT NAT` and `TIMEOUT TOC` commands. For `TIMEOUT NOW`, either specify non-activity time as start-up parameter or precede the command with `TIMEOUT NAT`.

## RSM0076 - Timeout processing disabled

Explanation | Timeout processing was disabled by a `TIMEOUT OFF` command.
Action | None.

## RSM0077 - REPEAT, TERSE, TOC, VERBOSE, or ?

Explanation | The `TIMEOUT` operator command was issued with an invalid sub-parameter.
Action | For a valid `TIMEOUT` command syntax, refer to Natural Roll Server Operation in the Natural Operations documentation.

## RSM0078 - Invalid parameter: parameter

Explanation | An invalid parameter was specified, or the last parameter was not `UCTRAN`.
Action | Correct the `PARM` string of the JCL `EXEC` statement.

## RSM0081 - Compression task n started successfully

Explanation | The Roll Server has started an additional task to handle the compression and decompression work load.
Action | None.

## RSM0082 - Compression task could not be started: Error n

Explanation | Error `n` occurred while the Roll Server was starting a new compression task.
Action | Contact Software AG Support.

## RSM0083 - Roll Server not in active state. TIMEOUT aborted.

Explanation | The Roll Server has deallocated its resources due to the operator command `DEAL` or a subtask abnormal end. The `TIMEOUT` command cannot execute in this situation.
Action | Reactivate the Roll Server with the operator command `START`, or terminate the Roll Server and restart it.

## RSM0084 - Low water mark cannot be above high water mark

Explanation | The low water mark must be below the high water mark.
Action | Correct the `PARM` string of the JCL `EXEC` statement, or the low water/high water values in the parameter file.

## RSM0085 - Module NATRSCMP not linked: Roll compression disabled.

Explanation | Module NATRSCMP must be linked to the Roll Server.
Action | Check the installation process of the Roll Server, and contact Software AG support.

## RSM0086 - Roll compression will run on zIIP

Explanation | The Roll Server has determined that the system includes one or more IBM System z Integrated Information Processors (zIIPs). Compression tasks will run as SRBs and be scheduled to run on the zIIP.
Action | None.

## RSM0087 - Enclave could not be created for SRB: n

Explanation | Error `n` occurred when the Roll Server tried to create a Work Load Manager (WLM) enclave for the compression SRB.
Action | Contact Software AG Support.

## RSM0088 - Enclave could not be redirected for SRB: n

Explanation | Error `n` was returned by the IBM service that was called to specify CPU offload to an IBM System z Integrated Information Processor (zIIP).
Action | Contact Software AG Support.

## RSM0089 - No zIIP available. Roll compression will run on GP.

Explanation | An IBM System z Integrated Information Processor (zIIP) is not installed. Thread compression and decompression will run on a general purpose processor.
Action | None.

## RSM0090 - DDNAME ddname does not designate a VSAM LINEAR file.

Explanation | The data set defined in the DD statement for `ddname` is a VSAM file but is not of type LINEAR.
Action | Specify a VSAM LINEAR file.

## RSM0091 - Unexpected reason code code opening DDNAME ddname

Explanation | A warning return code was received with reason code `code` when opening a VSAM roll file.
Action | Check message IEC161I in your JESMSGLG and follow the instructions IBM provides for this message in their MVS System Messages documentation.

## RSM0092 - Wrong ECSAD version: version

Explanation | NATRSMvr is started while there is still an ECSA-Directory present for another version of NATRSMvr for this subsystem-ID.
Action | Rename the subsystem-ID, IPL the system, or start NATASMvr with option `ECSADUPD`.

## RSM0093 - High water mark exceeded for roll file n

Explanation | The high water mark has been exceeded for the specified roll file n. The roll server triggers a cleanup, as if `TIMEOUT NOW` has been issued.
Action | If you want to manually free one or more slots, check the roll server slots occupation with `SYSTP` `R` > subsystem > `L`.

## RSM0094 - Low water mark exceeded for roll file n

Explanation | The low water mark has been exceeded, but the high water mark has not been reached yet.
Action | If this message occurs regularly, increase the size of the roll files to avoid the eventual exceeding of the the high water mark.

## RSM0095 - Filling rate under low water mark for roll file n

Explanation | Enough free spots were freed and the occupation level of the roll file n went under the low water mark.
Action | None.

## RSM0119 - Roll Server settings in effect:

Explanation | This message is issued at Roll Server start-up. It is followed by several `RSM0119` messages of varying contents, summarizing parameters in effect for this run. Selected `RSM0119` messages are also issued in response to the `TIMEOUT` operator command.
Action | None.

## RSM0120 - Start of Statistics

Explanation | This message is issued during shut-down and in response to the `STATS` operator command. Several `RMS0120` statistics messages with varying text follow this message.
Action | None.

## RSM0120 - End of Statistics

Explanation | This message is issued during shut-down and in response to the `STATS` operator command. It indicates the end of statistics output.
Action | None.

## RSM0131 - Environment error detected. SubRC: subrc

Explanation | Diagnostic message that goes along with RC = 16.
Action | Contact Software AG support.

## RSM0133 - DEAL and START commands are no longer supported.

Explanation | The `DEAL` and `START` operator commands are no longer available. It indicates the end of statistics output.
Action | If you want to refresh the roll server, use the z/OS STOP and START console commands.

## RSM0190 - +++++ Start of Diagnostics +++++

Explanation | This message is issued in response to the `DIAGNOSE` operator command. Several `RMS0190` messages with varying text may follow this message, depending on the nature of diagnostic Zaps supplied by Software AG.
Action | Follow advice given with diagnostic Zap.

## RSM0190 - +++++ End of Diagnostics +++++

Explanation | This message is issued in response to the `DIAGNOSE` operator command. It indicates the end of output generated by the `DIAGNOSE` command.
Action | Follow advice given with diagnostic Zap.

## RSM0313 - NATRSCMP return code 99. Diagnostic data follows:

Explanation | An unexpected error was encountered during thread compression/decompression.
Action | Contact Software AG support.

## RSM0313 - NATRSCMP return code 8. UserID and error message follow:

Explanation | An unexpected error was encountered during thread compression/decompression.
Action | Contact Software AG support.

## RSM0313 - DUMP requested by NATRSCMP. Check SYSUDUMP data set.

Explanation | An unexpected error was encountered during thread compression/decompression.
Action | Contact Software AG support.

### On this page

- RSM0001 - Subsystem ID invalid
- RSM0002 - Roll file number not numeric
- RSM0003 - Invalid number of roll files
- RSM0004 - Number of LRB slots not specified
- RSM0005 - Number of LRB slots not numeric
- RSM0006 - Number of LRB slots > 32767
- RSM0007 - Invalid CF structure name
- RSM0008 - Bad return code from IEANTRT: rc
- RSM0009 - DCB buffer could not be obtained. Reason: reasoncode
- RSM0010 - OPEN failed for DDNAME: ddname
- RSM0011 - Duplicate roll file DSN
- RSM0012 - Temp roll file buffer could not be obtained. Reason: reasoncode
- RSM0013 - RF directory buffer could not be obtained. Reason: reasoncode
- RSM0014 - LRB directory could not be obtained. Reason: reasoncode
- RSM0015 - Unrecognized parameter or invalid value in parameter file
- RSM0017 - Size for LRB > 524287 blocks
- RSM0018 - LX table could not be obtained. Reason: reasoncode
- RSM0019 - Roll Server Version vrs is active
- RSM0020 - Subtask terminated: taskname rc
- RSM0021 - Subtask termination initiated
- RSM0022 - All subtasks terminated
- RSM0023 - Other than MODIFY or STOP command received
- RSM0026 - Command allowed in active state only: command
- RSM0027 - Unknown command command
- RSM0029 - Recursive abend in maintask. Now waiting for CANCEL command
- RSM0030 - Low Water Mark not numeric or invalid
- RSM0031 - High Water Mark not numeric or invalid
- RSM0032 - Too few/many parameters for command
- RSM0033 - All resources deallocated
- RSM0036 - DUMP successful for roll file n
- RSM0037 - DUMP failed for roll file n
- RSM0038 - SNAP failed. Task RB could not be obtained
- RSM0039 - XES functions not available
- RSM0040 - IXLCONN unsuccessful. Reason code: reasoncode
- RSM0041 - CF initialization successful for list: n
- RSM0042 - CF initialization failed for list/RSN code: reasoncode
- RSM0043 - IXCJOIN failed. Return/Reason code: reasoncode
- RSM0044 - Act conn buffer could not be obtained
- RSM0045 - Applied zaps:
- RSM0046 - Roll file in use by job jobname ASID asid
- RSM0047 - Operator command: command
- RSM0048 - IARV64 GETSTOR failed. Return code: rc
- RSM0049 - Disconnected from CF with RSN=FAILURE
- RSM0050 - Disconnected from CF with RSN=NORMAL
- RSM0051 - Roll file n is newer than the CF structure
- RSM0052 - Not enough storage for IARV64 GETSTOR - Increase MEMLIMIT
- RSM0053 - Not enough memory for SNAP
- RSM0054 - OPEN for SYSUDUMP failed
- RSM0055 - CF structure does not contain enough lists
- RSM0056 - LRB slotsize invalid or not numeric
- RSM0057 - Bad return code from IEANTCR: rc
- RSM0058 - Rollserver already active in subsid: Job jobname ASID asid
- RSM0059 - Roll file ddname is below version 412
- RSM0060 - User exit loaded: NATRSU14
- RSM0061 - Slot size must be specified when no roll files are used
- RSM0062 - Running with in-core roll file
- RSM0063 - Coupling Facility will not be used
- RSM0064 - High/low water marks ignored
- RSM0065 - XES Event exit received unexpected event type: nn
- RSM0066 - REBUILD Start: CF structure temporarily unavailable
- RSM0067 - REBUILD End: CF structure available again
- RSM0068 - LRB slot size parameter ignored
- RSM0069 - Invalid non-activity time
- RSM0070 - Invalid timeout check time
- RSM0072 - Timeout processing starting
- RSM0073 - Scheduled/Operator timeout processing deleted n sessions
- RSM0074 - Timeout processing ended with return code rc
- RSM0075 - TIMEOUT ON/NOW rejected: No valid timeout parameters
- RSM0076 - Timeout processing disabled
- RSM0077 - REPEAT, TERSE, TOC, VERBOSE, or ?
- RSM0078 - Invalid parameter: parameter
- RSM0081 - Compression task n started successfully
- RSM0082 - Compression task could not be started: Error n
- RSM0083 - Roll Server not in active state. TIMEOUT aborted.
- RSM0084 - Low water mark cannot be above high water mark
- RSM0085 - Module NATRSCMP not linked: Roll compression disabled.
- RSM0086 - Roll compression will run on zIIP
- RSM0087 - Enclave could not be created for SRB: n
- RSM0088 - Enclave could not be redirected for SRB: n
- RSM0089 - No zIIP available. Roll compression will run on GP.
- RSM0090 - DDNAME ddname does not designate a VSAM LINEAR file.
- RSM0091 - Unexpected reason code code opening DDNAME ddname
- RSM0092 - Wrong ECSAD version: version
- RSM0093 - High water mark exceeded for roll file n
- RSM0094 - Low water mark exceeded for roll file n
- RSM0095 - Filling rate under low water mark for roll file n
- RSM0119 - Roll Server settings in effect:
- RSM0120 - Start of Statistics
- RSM0120 - End of Statistics
- RSM0131 - Environment error detected. SubRC: subrc
- RSM0133 - DEAL and START commands are no longer supported.
- RSM0190 - +++++ Start of Diagnostics +++++
- RSM0190 - +++++ End of Diagnostics +++++
- RSM0313 - NATRSCMP return code 99. Diagnostic data follows:
- RSM0313 - NATRSCMP return code 8. UserID and error message follow:
- RSM0313 - DUMP requested by NATRSCMP. Check SYSUDUMP data set.