Natural System Error Messages 3500-3549

#### Search Results

Search

# Natural System Error Messages 3500-3549

#### NAT3500: FCT definition for :1: incomplete; :2: missing.

    Text
    FCT definition for ... incomplete; ... missing.
    Explanation
    Natural for VSAM requires information from the CICS file control table
    to generate a CICS command; however, this information is missing.
    Action
    Contact your CICS administrator.

#### NAT3501: Internal Natural VSAM error, module :1: .

    Text
    Internal Natural VSAM error, module ... .
    Explanation
    An internal error condition has occurred.
    Action
    Contact Software AG support.

#### NAT3503: Internal Natural :1: error.

    Text
    Internal Natural ... error.
    Explanation
    Record buffer too small.
    Action
    Contact Software AG support.

#### NAT3504: File :1:, ENABLESTATUS/RESP :2:, RESP2 :3:.

    Text
    File ..., ENABLESTATUS/RESP ..., RESP2 ....
    Explanation
    Request could not be satisfied due to ENABLESTATUS problem.
    If the parameters ENADIS/ENAUNE in the macro NTVSAM of the Natural
    parameter module are set to "OFF", the ENABLESTATUS is indicated in the
    error message.
    If the parameters ENADIS/ENAUNE are set to "ON", Natural VSAM has issued
    an EXEC CICS SET ENABLED command; this command failed, and CICS
    has returned response codes as indicated in the error message.
    Action
    Contact your CICS administrator.

#### NAT3505: Loop reposition error occurred during ROLL-IN processing.

    Text
    Loop reposition error occurred during ROLL-IN processing.
    Explanation
    For the native AIX processing, a current base key cannot be
    found for a loop repositioning. Either the alternate indexes were
    destroyed or the record for this base key was deleted or
    changed by another user.
    Action
    Contact your Natural administrator.

#### NAT3506: Statement invalid for Natural VSAM.

    Text
    Statement invalid for Natural VSAM.
    Explanation
    This statement is not allowed for this type of VSAM
    dataset (for example, READ PHYSICAL for a KSDS type).
    Action
    Correct error in program.

#### NAT3507: USR0100N error: :1:.

    Text
    USR0100N error: ....
    Explanation
    The program that invokes the user exit USR0100N contains an error.
    Action
    Correct error in invoking program.

#### NAT3508: Logical key length is too big.

    Text
    Logical key length is too big.
    Explanation
    The sum of the logical key and prefix lengths, defined
    in the corresponding DDM, is greater than the maximum  VSAM
    key length.
    Action
    Correct error in DDM/program.

#### NAT3509: Complex search criteria not allowed for Natural VSAM.

    Text
    Complex search criteria not allowed for Natural VSAM.
    Explanation
    Connecting search criteria and coupling of files is
    not possible for VSAM files.
    See the Natural documentation, FIND statement, for valid
    search criteria.
    Action
    Correct error in program.

#### NAT3510: Invalid operator in FIND statement for Natural VSAM.

    Text
    Invalid operator in FIND statement for Natural VSAM.
    Explanation
    The FIND statement contains an invalid search criterion
    for VSAM files.
    Action
    Correct error in program.

#### NAT3511: Invalid search buffer.

    Text
    Invalid search buffer.
    Explanation
    Either the DDM was changed between cataloging and execution of the
    program, or the FIND statement contains a clause not applicable to
    VSAM.
    Action
    Contact your Natural administrator;
    or correct error in program.

#### NAT3512: File :1: is not defined as path.

    Text
    File ... is not defined as path.
    Explanation
    The NTVSAM parameter PATH=ON is specified for this session,
    but the file is not a path for an alternate index.
    Action
    Contact your system administrator.

#### NAT3513: Not enough storage for Natural VSAM in table :1:.

    Text
    Not enough storage for Natural VSAM in table ....
    Explanation
    One of the Natural for VSAM internal tables, defined as fixed
    buffer type, is too small. The eye-catcher of the internal
    table which is too small is indicated in the variable.
    Action
    Use the Buffer Usage Statistics function of the SYSTP utility to
    ascertain which parameter has to be adjusted in the NTVSAM macro.

#### NAT3514: Record to be updated is not in "hold" status.

    Text
    Record to be updated is not in "hold" status.
    Explanation
    An UPDATE statement was issued for a record which was not in
    "hold" status.
    This may be caused, for example, by the UPDATE statement
    referring to a FIND FIRST statement which found nothing.
    Action
    Correct program or provide other search criteria.

#### NAT3515: UPD table is full.

    Text
    UPD table is full.
    Explanation
    A record has been read for update. Natural for VSAM tried to save
    the appropriate fields in its UPD table, but received a response
    indicating that the UPD table was not large enough to contain the
    fields.
    Action
    Contact your Natural administrator to increase UPDL size in NTVSAM
    macro; or change program to reduce the amount of data held per
    transaction.

#### NAT3516: File: :1: Cmd: :2: Cond: :3: Rc: :4:.

    Text
    File: ... Cmd: ... Cond: ... Rc: ....
    Explanation
    Natural for VSAM received an unexpected response from CICS.
    File:  Name of involved dataset taken from DDM.
    Cmd:   Mnemonic of CICS command issued by Natural for VSAM.
    Cond:  Mnemonic of CICS condition.
    Rc:    VSAM return code and error code taken from EIB (if provided by
           CICS).
    Action
    See IBM"s CICS and VSAM documentation for further information.

#### NAT3517: UPDATE loop for path :1: to ESDS file :2: not supported.

    Text
    UPDATE loop for path ... to ESDS file ... not supported.
    Explanation
    CICS only supports path access to an ESDS file with restricted
    options. The related RBA for the ESDS base record is not
    returned from the READNEXT/READPREV path call by CICS,
    and an UPDATE is therefore not possible.
    Action
    In this case, use native AIX file processing.

#### NAT3518: Error in format buffer for Natural VSAM.

    Text
    Error in format buffer for Natural VSAM.
    Explanation
    The DDM was changed between cataloging and executing the Natural
    program.
    Action
    Contact your Natural administrator.

#### NAT3519: Error in format buffer for INSERT, base key omitted.

    Text
    Error in format buffer for INSERT, base key omitted.
    Explanation
    The base key was not specified for a KSDS file in the STORE statement.
    Action
    Correct error in program.

#### NAT3520: Held VSAM record modified by another transaction.

    Text
    Held VSAM record modified by another transaction.
    Explanation
    The record held by a previous READ/FIND for UPDATE was modified by
    another transaction.
    Action
    Check your application"s handling of concurrency control problems;
    or issue the RETRY statement in an ON ERROR clause to ignore the
    error situation.

#### NAT3521: Direction changed for an active READ in variable sequence.

    Text
    Direction changed for an active READ in variable sequence.
    Explanation
    For an active READ loop, the ascending/descending direction
    was changed to descending/ascending sequence.
    Action
    Correct error in program.

#### NAT3522: DD/DLBL name for file :1: is not defined in the JCL stream.

    Text
    DD/DLBL name for file ... is not defined in the JCL stream.
    Explanation
    The NTVSAM parameter PATH=CHECK is specified and the file
    is not defined in the system (no FCT entry for CICS, no UFILE
    entry for Com-plete, or no JCL card for any other environment).
    Action
    Contact your system administrator.

#### NAT3523: Insertion of :1: "LA" record without "LB" field.

    Text
    Insertion of ... "LA" record without "LB" field.
    Explanation
    Insertion of LA record into system file with LB field having been
    omitted (internal error).
    Action
    Contact your Natural administrator.
    If necessary, contact Software AG technical support.

#### NAT3524: Maximum VSAM record length exceeded at insertion/update.

    Text
    Maximum VSAM record length exceeded at insertion/update.
    Explanation
    Insertion/updating was requested for a record which is longer than the
    permitted maximum; or an attempt was made to increase the length of a
    "fixed length" record.
    Action
    Check record-length definition in VSAM cluster and in the DDM.

#### NAT3525: OPEN utility is active, specify OPSUPP=ON in NVSPARM.

    Text
    OPEN utility is active, specify OPSUPP=ON in NTVSAM macro.
    Explanation
    The user exit USR2008P is active, but the NTVSAM parameter
    OPSUPP=OFF is specified.
    Action
    Contact your Natural administrator.

#### NAT3526: Read on :1: "LB" subfile with other "DE" specified.

    Text
    Read on ... "LB" subfile with other "DE" specified.
    Explanation
    This is an internal Natural for VSAM, Natural for ISAM or
    Natural for LEASY error.
    Action
    Contact your Natural administrator.
    If necessary, contact Software AG technical support.

#### NAT3527: DDM VSAM file organization and VSAM type are not compatible.

    Text
    DDM VSAM file organization and VSAM type are not compatible.
    Explanation
    Either the DDM VSAM file organization is "extended" and the actual
    VSAM file is not of extended format, or vice versa.
    Action
    Correct the combination of the DDM VSAM file organization and the
    VSAM file format.

#### NAT3528: Specified :1: "DE" is not a secondary one.

    Text
    Specified ... "DE" is not a secondary one.
    Action
    Check program and correct error.

#### NAT3529: Field in HISTOGRAM must be a descriptor.

    Text
    Field in HISTOGRAM must be a descriptor.
    Explanation
    See the Natural documentation for valid HISTOGRAM syntax.
    Action
    Correct error in program.

#### NAT3530: UPD=OFF not allowed for Natural :1: :2:.

    Text
    UPD=OFF not allowed for Natural ... ....
    Explanation
    Inconsistency between DDM and NTVSAM macro.
    If the parameter UPD=OFF is set in the NTVSAM macro,
    logical files are not supported.
    Action
    Change DDM or NTVSAM macro.

#### NAT3531: No entry found with given command ID for Natural :1:.

    Text
    No entry found with given command ID for Natural ....
    Explanation
    This is an internal error.
    Action
    Contact your Natural administrator.

#### NAT3532: File :1: not known to CICS.

    Text
    File ... not known to CICS.
    Explanation
    CICS returned a DSIDERR condition upon Natural for VSAM"s
    INQUIRE command.
    Action
    Contact your CICS administrator.

#### NAT3533: File :1:, VSAM record deleted from another terminal.

    Text
    File ..., VSAM record deleted from another terminal.
    Explanation
    While UPDATE waited for a response, another terminal or
    batch user deleted the record in question; or the alternate index
    is destroyed.
    Action
    Check your application logic or the file structure.

#### NAT3534: Duplicate VSAM record in file :1:.

    Text
    Duplicate VSAM record in file ....
    Explanation
    An attempt was made to write a duplicate record to a unique-key
    VSAM dataset.
    Action
    Correct error in program.

#### NAT3535: A Natural :1: end-of-file condition has occurred.

    Text
    A Natural ... end-of-file condition has occurred.
    Action
    Contact your Natural administrator.

#### NAT3536: :1: error, feedback code :2:, file :3:.

    Text
    ... error, feedback code ..., file ....
    Action
    See IBM documentation for explanation of feedback code (RPLERRCD).

#### NAT3537: :1: failed, return/reason code :2:/:3:.

    Text
    ... failed, return/reason code .../....
    Explanation
    Natural for VSAM needed a temporary storage area outside
    VSIZE (for example, as I/O area); the appropriate GETMAIN
    or FREEMAIN request failed.
    The return code comes from NATGETM ,the reason code from the
    system.
    Action
    Increase available storage.

#### NAT3538: Response from CICS: INVREQ.

    Text
    Response from CICS: INVREQ.
    Explanation
    The statement is not allowed according to the dataset entry
    specification in the CICS File Control Table (FCT).
    If the Natural session runs with DU=ON, a NV63 ABEND with a
    transaction dump is forced in instead of NAT3538.
    Action
    Use CEDF to examine the cause of this problem, or start your session
    with DU=ON and analyze the trace table in the dump.

#### NAT3539: File :1: not :2:, :3:.

    Text
    File ... not ..., ....
    Explanation
    Open/close error. If available to Natural for VSAM, the original
    return code is indicated in the error message. For an explanation
    of the return code, see the corresponding IBM documentation.
    Action
    Contact your Natural administrator.

#### NAT3540: No more space in VSAM file :1:.

    Text
    No more space in VSAM file ....
    Explanation
    The VSAM file must be reorganized.
    Action
    Contact your Natural administrator.

#### NAT3541: File :1:, control interval/record held by another user.

    Text
    File ..., control interval/record held by another user.
    Action
    Check your application"s transaction logic or issue a
    RETRY in an ON ERROR clause to ignore the error condition.

#### NAT3542: File :1:, primary key must not be modified.

    Text
    File ..., primary key must not be modified.
    Explanation
    You are not allowed to modify the primary key area.
    Action
    Correct error in program.

#### NAT3543: File :1: invalid record length or length defined as fixed.

    Text
    File ... invalid record length or length defined as fixed.
    Explanation
    The length of a record exceeds the maximum record size or is shorter
    than the minimum record size.
    For an AIX file, the record length was not sufficient to contain the new
    alternate index key pointer.
    Action
    Check DDM and VSAM file definitions.
    If the file is a member of an UPGRADE set, increase the max. CI size
    or enlarge the file.

#### NAT3544: END of TRANSACTION not successful, RC: :1:.

    Text
    END of TRANSACTION not successful, RC: ....
    Explanation
    Under CICS, this error may be caused, for example, by a failure in the
    synchronization of remote systems.
    In DFSMStvs, a program or environmental error has occurred, or the
    Resource Recovery Service (RRS) is not available.
    Action
    Under CICS, use CEDF to determine the cause of this error.
    In DFSMStvs, refer to the IBM documentation on Callable RRS.

#### NAT3545: BACKOUT TRANSACTION not successful, RC: :1:.

    Text
    BACKOUT TRANSACTION not successful, RC: ....
    Explanation
    Under CICS, this error may be caused, for example, by a failure in the
    synchronization of remote systems.
    In DFSMStvs, a program or environmental error has occurred, or the
    Resource Recovery Service (RRS) is not available.
    Action
    Under CICS, use CEDF to determine the cause of this error.
    In DFSMStvs, refer to the IBM documentation on Callable RRS.

#### NAT3546: File :1: opened for input, :2: not allowed.

    Text
    File ... opened for input, ... not allowed.
    Action
    Either set the OPRB parameter to "O" (for output) for this database,
    or omit the OPRB parameter.
    Check the NTDB setting in the Natural parameter module.

#### NAT3547: Overflow of FCT table.

    Text
    Overflow of FCT table.
    Explanation
    Natural for VSAM"s internal file control table is full.
    Action
    Increase parameter TAFE in the NTVSAM macro of the Natural parameter
    module.

#### NAT3548: Now it is too late for BACKOUT TRANSACTION.

    Text
    Now it is too late for BACKOUT TRANSACTION.
    Explanation
    The program contains a design error: it attempts to backout updates
    which have already been committed.
    The most likely reason is that a terminal I/O has forced the end of
    the logical transaction; that is, internally a SYNCPOINT command has
    already been executed by the TP monitor at the time when the BACKOUT
    TRANSACTION statement is executed.
    Nevertheless, Natural VSAM has executed a BACKOUT TRANSACTION. This
    means that the actual scope of the BACKOUT TRANSACTION is different
    from the expected one.
    Action
    Correct error in program.

#### NAT3549: Working storage for user exit :1: cannot be allocated.

    Text
    Working storage for user exit ... cannot be allocated.
    Explanation
    Overflow on Natural internal buffer CFWSIZE.
    Action
    Contact Software AG support.