Natural under Com-plete/SMARTS User Abend Codes

#### Search Results

Search

# Natural under Com-plete/SMARTS User Abend Codes

This document contains the user abend codes and error messages issued by the Natural Com-plete/SMARTS Interface.

See also Natural under Com-plete/SMARTS in the TP Monitor Interfaces of the Natural for Mainframes documentation.

Abend Code | Explanation
--- | ---
`U0301` | An abend has been forced via `CMABEND` and `DU``=ON/FORCE` has been specified. The session will be terminated immediately with clean-up for `DU=ON` and without any cleanup for `DU=FORCE`. IOCB field `TPABCDE` (Register 10 + x18C) contains the abend code. IOCB offset `x'290'` contains the PSW and the Registers 0 to 15.
`U0302` | An abend has occurred and `DU``=ABEND` has been specified. The session will be cleaned up before it is abended. IOCB offset `x'290'` contains the PSW and the Registers 0 to 15.
`U0304` | An abend has occurred, and Natural is not ready to handle it. The session will be terminated immediately without any clean-up. IOCB offset `x'290'` contains the PSW and the Registers 0 to 15.
`U0305` | An abend has occurred and Natural's BB could not be addressed.
`U0307` | The Natural under Com-plete save area stack is exhausted.
`U0308` | An abend has occurred and the Natural Com-plete `ABEXIT` handler abends recursive.
`U0309` | Attention key has been pressed, and Natural is not ready to handle it. The session will be terminated immediately without any clean-up. IOCB offset `x'290'` contains the PSW and the Registers 0 to 15.
`U0310` | An unexpected error at Terminal I/O has occurred. The session will be terminated immediately without any clean-up. IOCB offset `x'290'` contains the PSW and the Registers 0 to 15.
`U0312` | The Natural shared nucleus has been displaced during a terminal I/O, and the Natural relocation module returns a non-zero return code.
`U0313` | An unexpected error for `ABEXIT` entry has occurred.The session will be terminated immediately without any clean-up. IOCB offset `x'290'` contains the PSW and the Registers 0 to 15.
`U0316` | Roll-Out Failure. Тhe request to pass the data from a session to the Roll Server has failed аt session suspension. IOCB offset x'298' contains the Registers 0 to 15, where R15 is a Roll Server return code, and R0 is a Roll Server reason code. For more information on reason and return codes, see Return Codes and Reason Codes of the Roll Server Requests.
`U0317` | Roll-In Failure. Тhe request to pass the data from a session to the Roll Server has failed аt session resumption. IOCB offset x'298' contains the Registers 0 to 15, where R15 is a Roll Server return code, and R0 is a Roll Server reason code. For more information on reason and return codes, see Return Codes and Reason Codes of the Roll Server Requests.