SAF* - SAF Daemon Messages

#### Search Results

Search

# SAF* - SAF Daemon Messages

The following messages may be issued by the SAF daemon.

### Meldungen im Überblick

`SAF001I | SAF002I | SAFD01S | SAFD02S | SAFD03E | SAFD04I | SAFD05E | SAFD06E | SAFD07E | SAFD08E | SAFD09I | SAFD10E | SAFD11I | SAFD12I | SAFD13E | SAFD14I | SAFD15I | SAFD22E | SAFD25E | SAFD26E | SAFD30E | SAFD31E | SAFD34E | SAFD40S | SAFD42S | SAFD43S`

SAF001I | Unable to load required module: xxxxxx
Erläuterung | The SAF kernel or one of the modules it needs could not be loaded. Ensure that all SAF modules (including those created by installation assembly jobs – SAFCFG, SAFPSEC and SAFPMAC) are available.

SAF002I | Unable to obtain anchor storage
Erläuterung | A memory allocation failed during initialization. Increase the region size.

SAFD01S | SAF CANNOT INITIALISE, GETMAIN ERROR
Erläuterung | There is insufficient memory for the SAF daemon to initialize. Increase the region size.

SAFD02S | SAF CANNOT INITIALISE, KERNEL LOAD ERROR
Erläuterung | Installation error (SAFCKN load module not available). Ensure that all required load modules are available.

SAFD03E | DDCARD open error: ## - terminating
Erläuterung | The SAF daemon was enable to open DDCARD. Ensure that the DDCARD DD statement is specified correctly.

SAFD04I | Input parameter: xxx
Erläuterung | The daemon echoes the values of the supplied DDCARD parameters.

SAFD05E | Invalid parameter: ###########
Erläuterung | DDCARD contained an invalid parameter. The SAF daemon terminates. Correct the parameter in error.

SAFD06E | Product parameter not specified
Erläuterung | DDCARD did not contain `PRODUCT=SAF`. Ensure that `PRODUCT=SAF` and `DEFAULT=SAF` are both specified.

SAFD07E | MPM failure - function: ## error ##
Erläuterung | The SAF daemon received an error from ADAMPM. This message will usually be preceded by an explanatory message. If in doubt, contact your technical support representative for assistance.

SAFD08E | IOR failure - function: ## error ##
Erläuterung | An error occurred during an ADAIOR service call. Contact your technical support representative for assistance.

SAFD09I | Shutdown requested
Erläuterung | The SAF daemon has been instructed to shut down.

SAFD10E | Getmain for command queue failed
Erläuterung | The SAF daemon failed to allocate its command queue. Increase the region size.

SAFD11I | SAF Kernel is active on node nnnnn sss CIB=aaaaaaaa
Erläuterung | The daemon is now active and ready to receive security requests; nnnnn is the node ID, sss is the SVC number, and aaaaaaaa is the address of the daemon's main storage area.

SAFD12I | Oper type in: SAF xxxxx
Erläuterung | Message 12I is issued before processing of an operator command.

SAFD13E | Invalid operator command
Erläuterung | An invalid operator command was entered.

SAFD14I | Target nnnnn termination in progress
Erläuterung | Message 14I is issued during daemon termination (nnnnn is the daemon's node ID).

SAFD15I | Target nnnnn ended normally
Erläuterung | Message 15I is issued during daemon termination (nnnnn is the daemon's node ID).

SAFD22E | Load for module: ######## failed
Erläuterung | The indicated module could not be loaded. Ensure that it is available.

SAFD25E | ### is an invalid product name
Erläuterung | An invalid `PRODUCT= parameter` was specified in DDCARD.

SAFD26E | Proxy module SAFPXY was not found, product SAF will not be called
Erläuterung | Ensure that SAFPXY and all other required load modules are available.

SAFD30E | Getmain for product parm block failed
Erläuterung | A memory allocation failed during initialization. Increase the region size.

SAFD31E | Cab allocation error in module syscoru
Erläuterung | A memory allocation failed during initialization. Increase the region size.

SAFD34E | UAB allocation error in module syscoru
Erläuterung | A memory allocation failed during initialization. Increase the region size.

SAFD40S | Abend code Psw pppppppp pppppppp
Erläuterung | Message 40S is issued during abnormal termination. It shows the abend code, Program Status Word, module that abended and register contents. In the event of an abend, please ensure you collect the messages, the dump and any trace messages or snaps that have been generated.

SAFD42S | Module module entry entry-point offset offset
Erläuterung | Message 42S is issued during abnormal termination. It shows the abend code, Program Status Word, module that abended and register contents. In the event of an abend, please ensure you collect the message, the dump and any trace messages or snaps that have been generated.

SAFD43S | Regs 00-03 register contents
Regs 04-07 register contents
Regs 08-11 register contents
Regs 12-15 register contents
Erläuterung | Message 43S is issued during abnormal termination. It shows the abend code, Program Status Word, module that abended and register contents. In the event of an abend, please ensure you collect the message, the dump and any trace messages or snaps that have been generated.