Natural System Error Messages 1050-1099

#### Search Results

Search

# Natural System Error Messages 1050-1099

#### NAT1070: Buffer pool initialization not linked.

    Text
    Buffer pool initialization is not linked.
    Explanation
    Driver entry CMBPGETS is missing.
    Natural environment is incomplete.
    Action
    Check your Natural environment.

#### NAT1071: Incompatible version for :1: buffer pool :2:.

    Text
    Incompatible version for ... buffer pool ....
    Explanation
    The version of the buffer pool already initialized is not supported by
    the current Natural version.
    Action
    Ensure that the buffer pool is allocated and initialized by a compatible
    Natural version.

#### NAT1072: Incompatible type for :1: buffer pool :2:.

    Text
    Incompatible type for ... buffer pool ....
    Explanation
    Natural has various buffer pools to share common virtual memory.
    For example: - type Natural for Natural programs,
                 - type SORT for common external sort space,
                 - type EDIT for common external editor buffers,
                 - type MONITOR for common monitor data.
    Because the buffer pool types have different storage layouts,
    it is not possible to use the buffer pool types interchangeably.
    Action
    Check NTBPI macro settings in your Natural parameter module for local
    pools or the parameter settings in your startup JCL for global buffer
    pools.

#### NAT1073: Initialization of :1: buffer pool failed. (:2:).

    Text
    Initialization of ... buffer pool failed. (...).
    Explanation
    The indicated buffer pool could not be initialized for one
    of the following reasons:
    - GETMAIN for the local buffer pool storage failed
    - specified buffer pool size (BPSIZE parameter) is too small
    - missing LINK for the EDTSTUB (installation error)
    Action
    Please check installation and correct the problem.

#### NAT1074: Global :1: buffer pool :2: not found.

    Text
    Global :1: buffer pool :2: not found.
    Explanation
    The global buffer pool :2: of type :1: could not be found.
    Either the global buffer pool is not yet allocated or the used
    name of the global buffer pool is wrong.
    If the buffer pool could not be found because the Natural subsystem does
    not exist, the name of the Natural subsystem is appended to the name of
    the global buffer pool, separated by a slash (/).
    Action
    Check the name of the global buffer pool (Natural profile parameter
    BPNAME or NTBPI/BPI subparameter NAME) and/or the name of the Natural
    subsystem (Natural profile parameter SUBSID).

#### NAT1075: Global :1: buffer pool :2: allocated in system key.

    Text
    Global ... buffer pool ... allocated in system key.
    Explanation
    The indicated global buffer pool has been allocated in system key, but
    the authorized services manager (ASM) has not been started or is not
    of the required minimum version.
    To process a buffer pool that has been allocated in system key, the ASM
    is required.
    Action
    Start an authorized services manager of the required minimum version
    for the Natural subsystem in use.

#### NAT1076: Error :1: while loading preload list :2: :3:.

    Text
    Error :1: while loading preload list :2: :3:.
    Explanation
    Natural error :1: has occurred when Natural tried to load the buffer
    pool preload list :2: at the start of the Natural session.
    If the Natural error occurs when the preload list is being read, the
    information :3: is blank.
    If the Natural error occurs when an object named in the preload list
    is being loaded, :3: contains library and program name of the object.
    The typical Natural error will be NAT0082, which means that either
    the preload list or one the named objects could not be found.
    Action
    Check the object names in your preload list.

#### NAT1077: Buffer pool propagation failed.

    Text
    Buffer pool propagation failed.
    Explanation
    The propagation of changes to the currently used Natural buffer
    pool is requested by the current setting of the Natural profile
    parameter BPPROP, but the propagation failed.
    Possible reasons:
    - The Natural Authorized Services Manager is not started for the
      Natural subsystem ID used by the current Natural session.
    - The Natural Authorized Services Manager is started without an
      XCF group name and BPPROP=PLEX or BPPROP=GPLEX is requested by
      the current Natural session.
    Action
    Contact the Natural administrator
    and/or check the setting of the Natural profile parameter BPPROP.

#### NAT1078: Allocation of local buffer pool cache failed.

    Text
    Allocation of local buffer pool cache failed.
    Explanation
    A buffer pool cache has been requested for a local Natural buffer pool,
    but the cache could not be allocated. The local Natural buffer pool is
    operational, but runs without a cache.
    This error message is preceded by other error messages which indicate
    the reason.
    Action
    Check the preceding error messages.

#### NAT1079: Work area could not be obtained by Authorized Services Manager.

    Text
    Work area could not be obtained by Authorized Services Manager.
    Explanation
    The Authorized Services Manager (ASM) could not obtain the work area for
    the PC routine which is used to access a buffer pool in system key.
    Action
    Increase the amount of available space for the ASM address space.
    If the problem persists, contact technical support.

#### NAT1080: Cache creation failure :1: :2: :3: Reason= :4:.

    Text
    Cache creation failure :1: :2: :3: Reason= :4:.
    Explanation
    The cache create function has failed.
    The message shows the failing operating-system macro and the macro
    function (:1:).
    It also indicates the type of macro-request failure (:2:), that is,
    whether the macro failed due to macro failure (RC=) or ABEND (CC=).
    Parameter :3: is the ABEND code or macro-request return code
    respectively.
    Parameter :4: is the associated reason code.
    Action
    See the relevant operating-system manuals for the reason of the failure.

#### NAT1081: Cache deletion failure :1: :2: :3: Reason= :4:.

    Text
    Cache deletion failure :1: :2: :3: Reason= :4:.
    Explanation
    The cache delete function has failed.
    The message shows the failing operating-system macro and the macro
    function (:1:).
    It also indicates the type of macro request failure (:2:), that is,
    whether the macro failed due to macro failure (RC=) or ABEND (CC=).
    Parameter :3: is the ABEND code or macro-request return code
    respectively.
    Parameter :4: is the associated reason code.
    Action
    See the relevant operating-system macros for the reason of the failure.