Natural System Error Messages 5750-5799

#### Search Results

Search

# Natural System Error Messages 5750-5799

#### NAT5750: Invalid operand within operand list.

    Text
    ESY5750 Invalid operand within operand list.
    Explanation
    Incorrect usage of an Entire System Server view.
    Action
    No action is required.

#### NAT5751: Not enough memory to execute the function.

    Text
    ESY5751 Not enough memory to execute the function.
    Explanation
    There is not enough memory to execute the function.
    Action
    Check with systems programmer.

#### NAT5752: Message/Message length missing.

    Text
    ESY5752 Message/Message length missing.
    Explanation
    Possible reasons:  - no message length specified
                       - message length lower than 4
                       - message length greater than 1250 during use
                         of field MESSAGE-ARRAY
                       - message length greater than 250 during use
                         of field MESSAGE-TEXT
                       - no message specified
    Action
    Correct input values and try again.

#### NAT5753: I-T-C name missing.

    Text
    ESY5753 I-T-C name missing.
    Explanation
    ITC name must be specified for functions OPEN, RECEIVE and SEND.
    Action
    Specify ITC name.

#### NAT5754: not done.

    Text
    ESY5754          not done.

#### NAT5755: Invalid or no SWITCH type specified.

    Text
    ESY5755 Invalid or no SWITCH type specified.
    Explanation
    Neither USER nor PROCESS as switch type specified.
    Action
    Correct switch type.

#### NAT5756: Job Variable name missing or invalid.

    Text
    ESY5756 Job Variable name missing or invalid.
    Explanation
    Invalid syntax used or no value specified.
    Action
    Please correct name specification.

#### NAT5757: Error during user management.

    Text
    ESY5757 Error during user management.

#### NAT5758: User ID is missing.

    Text
    ESY5758 User ID is missing.
    Explanation
    No user name specified.
    Action
    Please specify name.

#### NAT5759: Name is missing.

    Text
    ESY5759 Name is missing.

#### NAT5760: Processor name is missing.

    Text
    ESY5760 Processor name is missing.

#### NAT5761: Start operand is missing.

    Text
    ESY5761 Start operand is missing.

#### NAT5762: Line/Station is missing.

    Text
    ESY5762 Line/Station is missing.

#### NAT5763: Info type operand is missing.

    Text
    ESY5763 Info type operand is missing.

#### NAT5764: Virtual call is missing.

    Text
    ESY5764 Virtual call is missing.

#### NAT5765: Required Catalog ID not accessible.

    Text
    ESY5765 Required Catalog ID not accessible.

#### NAT5766: User ID or Terminal ID missing.

    Text
    ESY5766 User ID or Terminal ID missing.
    Explanation
    Neither User ID nor processor-/terminal-name specified.
    Action
    Please specify requested values.

#### NAT5767: No TSN found.

    Text
    ESY5767 No TSN found.

#### NAT5768: Invalid command in macro list.

    Text
    ESY5768 Invalid command in macro list.

#### NAT5769: Short name is missing.

    Text
    ESY5769 Short name is missing.

#### NAT5770: Serialisation name missing.

    Text
    ESY5770 Serialisation name missing.

#### NAT5771: No information found.

    Text
    ESY5771 No information found.
    Explanation
    No information found for specified request.
    Action
    No action required.

#### NAT5772: BS2000 Command has returned error.

    Text
    ESY5772 BS2000 Command has returned error.

#### NAT5773: New version operand missing.

    Text
    ESY5773 New version operand missing.

#### NAT5774: No core available.

    Text
    ESY5774 No core available.
    Explanation
    Not enough space available to allocate an NPR User Block.
    Action
    Please contact technical support.
    For BS2000 only: The number of NPR User Blocks can be configured with
    startup parameter NUMUSER.

#### NAT5775: Invalid Priority Value specified.

    Text
    ESY5775 Invalid Priority Value specified.

#### NAT5776: Request was cancelled.

    Text
    ESY5776 Request was cancelled.
    Explanation
    Request was cancelled internally because user has been
    timed out.

#### NAT5777: Request has abended.

    Text
    ESY5777 Request has abended.
    Explanation
    An internal error occurred. Condensed abend information is contained
    in the job-log.
    Action
    Check with the systems programmer. Contact technical support.

#### NAT5778: Cannot perform command - not APF authorized.

    Text
    ESY5778 Cannot perform command - not APF authorized.
    Explanation
    The Entire System Server nucleus is not running APF authorized.
    Action
    Check with the systems programmer.

#### NAT5779: IDCAMS utility has abended.

    Text
    ESY5779 IDCAMS utility has abended.
    Explanation
    The IDCAMS utility has abended.
    Action
    Check job-log for additional information.

#### NAT5780: Completion code not ok.

    Text
    ESY5780 Completion code not ok.
    Explanation
    The execution of the request was not successful.
    Action
    Check input data of request.

#### NAT5781: Unable to obtain storage for work area extension.

    Text
    ESY5781 Unable to obtain storage for work area extension.
    Explanation
    A request failed to obtain storage for the work area extension.
    Action
    Increase the region size above 16 MB for Entire System Server.

#### NAT5782: Error from :1: for :2:, RC :3:, REASON :4:.

    Text
    ESY5782 Error from ... for ..., RC ..., REASON ....
    Explanation
    A request failed while attempting to read the VTOC.
    Action
    Contact your systems programmer.

#### NAT5783: Unable to allocate :1:, RC :2:, REASON :3:.

    Text
    ESY5783 Unable to allocate ..., RC ..., REASON ....
    Explanation
    The specified volume could not be allocated.
    Action
    Contact your systems programmer.

#### NAT5784: Unable to open VTOC on :1:, RC :2:.

    Text
    ESY5784 Unable to open VTOC on ..., RC ....
    Explanation
    An OPEN request failed for the VTOC on the specified volume.
    Action
    Try again. If the problem persists, contact your systems programmer.

#### NAT5785: CVAF :1: failed with RC :2: and CVSTAT :3:.

    Text
    ESY5785 CVAF ... failed with RC ... and CVSTAT ....
    Explanation
    A request failed to the Common VTOC Access Facility.
    Action
    Contact your systems programmer.

#### NAT5786: Unable to obtain storage for CSI work area.

    Text
    ESY5786 Unable to obtain storage for CSI work area.
    Explanation
    A request failed to obtain storage for the CSI work area.
    Action
    Increase the region size above 16 MB for Entire System Server.

#### NAT5787: CSI request failed, Module :1:, Reason :2:, RC :3:.

    Text
    ESY5787 CSI request failed, Module ..., Reason ..., RC ....
    Explanation
    A request to the catalog search interface failed.
    Action
    Contact your systems programmer.

#### NAT5788: Unable to substitute symbol :1:, RC :2:.

    Text
    ESY5788 Unable to substitute symbol ..., RC ....
    Explanation
    A request failed to substitute text for a system symbol.
    Action
    Contact your systems programmer.

#### NAT5789: Unable to get UCB copy for :1:, RC :2:.

    Text
    ESY5789 Unable to get UCB copy for ..., RC ....
    Explanation
    A request failed to get a UCB copy for the volume specified.
    Action
    Contact your systems programmer.

#### NAT5790: Abend :1: during IEBCOPY.

    Text
    ESY5790 Abend :1: during IEBCOPY.
    Explanation
    An abend has occurred while processing the IEBCOPY utility.
    Action
    Contact your systems programmer.

#### NAT5798: Task was not started under TSOS.

    Text
    Task was not started under TSOS.
    Explanation
    The ENTIRE SYSTEM SERVER does not run under TSOS and does not have the
    required privileges to process the user requests.
    Action
    Check the job control and make sure that all tasks of the ENTIRE SYSTEM
    SERVER run under TSOS. Do a restart after changing the job control.

#### NAT5799: ENTIRE SYSTEM SERVER internal error.

    Text
    ESY5799 Entire System Server internal error.
    Explanation
    An internal error has occured.
    Action
    Contact your technical support.