SYSERR Functions

#### Search Results

Search

# SYSERR Functions

You invoke a SYSERR utility function by entering the code that corresponds to the required function and one or more parameters in the input fields of the SYSERR main menu. This section describes the functions provided in the menu and the parameters that can be specified for each function. For general instructions on the use of parameters, see the section Parameters.

- Adding Messages

- Deleting Messages

- Displaying Messages

- Modifying Messages

- Printing Messages

- Scanning Messages

- Selecting Messages from a List

- Translating Messages into other Languages

## Adding Messages

To add new messages

1. The SYSERR utility is case-sensitive by default. If you want lower to upper case translation for the messages to be created, enter the following terminal command:

       %U

   Any lower case characters you type when adding message text are then converted to upper case characters for the duration of the current Natural session. Message text is also converted to upper case if the profile parameter `TS` is set to `ON` (see the Parameter Reference documentation).

   For detailed information on `%U`, see the Terminal Commands documentation.

2. Invoke the SYSERR main menu and enter the following values:

   Field | Input Value
   --- | ---
   Code | `AD`
   Message type |
   `NS` | Natural system short messages
   `NL` | Natural system long messages
   `US` | User-defined short messages
   `UL` | User-defined long messages
   A long message can only be added if the corresponding short message already exists, as the long message is intended to be an explanation of the short message.
   Library | Any existing Natural library.
   Message number | Two numbers of up to four digits corresponding to the first and last numbers of the range of messages to be added. If you only want to add one message, either enter the number of the new message in the left Message number field and clear the right field, or enter the number in both fields.
   Language codes | The code of the language for which the message is to be added. If the message type is `NS` or `NL`, the language code must be `1` for English. For other message types, the first language code entered in the field is used; all others are ignored.

3. Press ENTER.

   An Add Short Message screen similar to the example below is displayed:

       15:56:01              ***** NATURAL SYSERR UTILITY *****             2008-11-28
       Lower Case ON               - Add Short Message -

       Number        Short Message (English)
       ------------  -----------------------------------------------------------------
       SYSERR1004
                     ....+....1....+....2....+....3....+....4....+....5....+..

       Sample ...... Message sample number 0000

       Enter-PF1---PF2---PF3---PF4---PF5---PF6---PF7---PF8---PF9---PF10--PF11--PF12---
       Add               Exit                    -     +                       Canc

   The Number field indicates the message number (in the example above, `1004`), which is prefixed with the library ID (in the example above, `SYSERR`).

4. In the input line next to the message number, type in a short message text and press ENTER.

   Oder:
   If the line labeled Sample contains a sample message text as shown in the example above, copy this text into the input line by entering `.C` and then pressing ENTER. If the sample message text contains the string `0000`, this string is replaced by the new message number as illustrated in the following example:

       15:30:46              ***** NATURAL SYSERR UTILITY *****             2008-11-28
       Lower Case ON               - Add Short Message -

       Number        Short Message (English)
       ------------  -----------------------------------------------------------------
       SYSERR1004    Message sample number 1004
                     ....+....1....+....2....+....3....+....4....+....5....+..

       Sample ...... Message sample number 0000

       Message has been added.

       Enter-PF1---PF2---PF3---PF4---PF5---PF6---PF7---PF8---PF9---PF10--PF11--PF12---
       Mod               Exit                    -     +     Long              Canc

   For instructions on creating a sample message, see the `SAMPLE` command described in Direct Commands.

5. Press PF9 to add a corresponding long message text.

   An Add Long message-number screen similar to the example below appears:

       16:20:24       - Add Long SYSERR1004 (English) - Lower Case ON       2008-11-28
        1 Tx. Message sample number 1004
        2     .
        3     .
        4 Ex. .
        5     .
        6     .
        7     .
        8     .
        9     .
       10     .
       11     .
       12     .
       13     .
       14     .
       15     .
       16     .
       17     .
       18 Ac. .
       19     .
       20     .

       Enter-PF1---PF2---PF3---PF4---PF5---PF6---PF7---PF8---PF9---PF10--PF11--PF12---
       Add               Exit                                Short Copy        Canc

6. Enter text in the three input areas: Tx. (text), Ex. (explanation) and Ac. (action).

7. Press ENTER to save the long message.

8. Press PF9 to return to the short message or to add the next short message in ascending order if you selected a range of message numbers.

9. Press PF3 or PF12 to return to the SYSERR main menu.

   Oder:
   Press PF8 or PF7 to add the next short message in ascending or descending order if you selected a range of message numbers.

## Deleting Messages

To delete messages

- In the fields of the SYSERR main menu, enter the following values:

  Field | Input Value
  --- | ---
  Code | `DE`
  Message type |
  `NS` | Natural system short messages
  `NL` | Natural system long messages
  `US` | User-defined short messages
  `UL` | User-defined long messages
  It is possible to delete a long message without deleting the corresponding short message, but not vice versa. If you try to delete a short message for which a long message exists, you are asked to confirm the deletion of both.
  Library | Any existing Natural library.
  Message number | Two numbers of up to four digits corresponding to the first and last numbers of the range of messages to be deleted.
  Language codes | The code(s) of the language(s) in which the messages are to be deleted. To indicate that the messages specified are to be deleted in all languages available, enter an asterisk (*).

## Displaying Messages

To display messages

1. In the fields of the SYSERR main menu, enter the following values:

   Field | Input Value
   --- | ---
   Code | `DI`
   Message type |
   `NS` | Natural system short messages
   `NL` | Natural system long messages
   `US` | User-defined short messages
   `UL` | User-defined long messages
   Library | Any existing Natural library.
   Message number | Two numbers of up to four digits corresponding to the first and last numbers of the range of messages to be displayed.
   Language codes | The code of the language in which the messages are to be displayed. Only one language code is accepted. If more than one code is specified, only the first one is used; all others are ignored.

2. Press ENTER.

   For short messages, a Display Short Messages screen similar to the example below appears:

       15:41:11              ***** NATURAL SYSERR UTILITY *****             2008-11-28
                                 - Display Short Messages -

       Number        Short Message (English)
       ------------  -----------------------------------------------------------------
       NAT0001       Missing/invalid syntax; undefined variable name/keyword.
       NAT0002       No file is available with specified name or number.
       NAT0003       Invalid character string for file name or file number.
       NAT0004       DEFINE DATA must be the first statement if present.
       NAT0005       Closing parenthesis missing in arithm/logical expression.
       NAT0006       ESCAPE statement used when no processing loop active.
       NAT0007       Invalid THRU or TO clause in READ LOGICAL or HISTOGRAM.

       Enter-PF1---PF2---PF3---PF4---PF5---PF6---PF7---PF8---PF9---PF10--PF11--PF12---
       +                 Exit                          +                       Canc

   Press PF8 to page forwards.

   For long messages, the Display Long Message screen is displayed where the messages are displayed one after another by pressing PF8 to page forwards or PF7 to page backwards. The Display Long Message screen is similar to the Modify Long Message screen shown in Modifying Messages.

## Modifying Messages

To modify messages

1. The SYSERR utility is case-sensitive by default. If you want lower to upper case translation for the messages to be modified, enter the following terminal command:

       %U

   Any lower case characters you type when editing message text are then converted to upper case characters for the duration of the current Natural session. Message text is also converted to upper case if the profile parameter `TS` is set to `ON` (see the Parameter Reference documentation).

   For detailed information on `%U`, see the Terminal Commands documentation.

2. In the fields of the SYSERR main menu, enter the following values:

   Field | Input Value
   --- | ---
   Code | `MO`
   Message type |
   `NS` | Natural system short messages
   `NL` | Natural system long messages
   `US` | User-defined short messages
   `UL` | User-defined long messages
   Library | Any existing Natural library.
   Message number | Two numbers of up to four digits corresponding to the first and last numbers of the range of messages to be modified.
   Language codes | The code of the language in which the messages are to be modified. Only one language code is accepted. If more than one code is specified, only the first one is used; all others are ignored.

3. Press ENTER.

   A Modify Short Message screen similar to the example below is displayed:

       16:46:31              ***** NATURAL SYSERR UTILITY *****             2008-11-28
       Lower Case ON             - Modify Short Message -

       Number        Short Message (English)
       ------------  -----------------------------------------------------------------
       SYSERR1004    Message sample number 1004
                     ....+....1....+....2....+....3....+....4....+....5....+..

        1 Tx. Input missing.
        2     .
        3     .
        4 Ex. Input value missing in field XYZ.
        5     Enter an alphanumeric value.
        6     .
        7     .
        8     .
       18 Ac. Enter value in field XYZ.
       19     .
       20     .

       Enter-PF1---PF2---PF3---PF4---PF5---PF6---PF7---PF8---PF9---PF10--PF11--PF12---
       Mod               Exit                    -     +           Copy        Canc

   For reference purposes, the long message is displayed in the bottom half of the screen.

   When you modify long messages, the Modify Long message-number screen is displayed:

       16:56:08     - Modify Long SYSERR1004 (English) - Lower Case ON      2008-11-28
        1 Tx. Input missing.
        2     .
        3     .
        4 Ex. Input value missing in field XYZ.
        5     Enter an alphanumeric value.
        6     .
        7     .
        8     .
        9     .
       10     .
       11     .
       12     .
       13     .
       14     .
       15     .
       16     .
       17     .
       18 Ac. Enter value in field XYZ.
       19     .
       20     .

       Enter-PF1---PF2---PF3---PF4---PF5---PF6---PF7---PF8---PF9---PF10--PF11--PF12---
       Mod               Exit                    -     +           Copy        Canc

4. Press ENTER to save any modifications.

5. Press PF8 or PF7 to modify the next message in ascending or descending order if you selected a range of numbers.

## Printing Messages

To print messages

1. In the fields of the SYSERR main menu, enter the following values:

   Field | Input Value
   --- | ---
   Code | `PR`
   Message type |
   `NS` | Natural system short messages
   `NL` | Natural system long messages
   `US` | User-defined short messages
   `UL` | User-defined long messages
   Library | Any existing Natural library.
   Message number | Two numbers of up to four digits corresponding to the first and last numbers of the range of messages to be printed.
   Language codes | The code of the language in which the messages are to be printed. Only one language code is accepted. If more than one code is specified, only the first one is used; all others are ignored.

2. Press ENTER.

   A print window similar to the example below opens:

       +------Print Natural System Messages-------+
       !                                          !
       !   Language code .... 1                   !
       !                                          !
       !   Long texts, too .. N                   !
       !   Message number ... 1___ -  25          !
       !   Lines per page ... 60_                 !
       !   Left margin ...... 10                  !
       !   Top margin ....... 0_                  !
       !   Bottom margin .... 0_                  !
       !   Printer ID ....... PRT1____            !
       !                                          !
       !                                          !
       +------------------------------------------+

3. Specify the options provided in the print window and the logical printer name.

   See the `DEFINE PRINTER` statement in the Natural Statements documentation for details on logical printer names.

4. Press ENTER to output the selected messages on a printer.

To print all Natural system messages

- In the fields of the SYSERR main menu, enter the following values:

  - Code `PR`,

  - Message type `NS` or `NL`,

  - Message number range `1` - `9999,`

  - Language code `1` (English) or `2` (German).

  A library ID is not required and possible entries are ignored.

## Scanning Messages

This function is used to scan messages for a specific string of characters. Only short messages can be scanned.

To scan messages

1. In the fields of the SYSERR main menu, enter the following values:

   Field | Input Value
   --- | ---
   Code | `SC`
   Message type |
   `NS` | Natural system short messages
   `US` | User-defined short messages
   Library | Any existing Natural library.
   Message number | Two numbers of up to four digits corresponding to the first and last numbers of the range of messages to be scanned.
   Language codes | Specify a maximum of nine language codes from the ranges 1 - 9, A - Z and a - y, or enter an asterisk (*) for all languages.

2. Press ENTER.

   A scan window similar to the example below opens:

       +--------------------------------------+
       |   Scan value(s)       Or/And/Not     |
       |   ----------------    ----------     |
       |   ________________       OR_         |
       |   ________________                   |
       |   ________________                   |
       |   ________________                   |
       |                                      |
       |   Absolute ..... X                   |
       |   Immediate .... _                   |
       |                                      |
       +--------------------------------------+

   In the fields provided, you can specify the search criteria to be used for scanning:

   Scan value(s) | In the four empty fields, enter up to four character strings to be searched for. The scan finds the specified terms in both upper and lower case.
   Or/And/Not |
   You can perform a Boolean search query by entering one of the following operators:
   `OR` | Searches for one or more of the character strings entered in Scan value(s). This is the default setting.
   `AND` | Searches for all of the character strings entered in Scan value(s).
   `NOT` | Searches for none of the character strings entered in Scan value(s).
   The operator is ignored if you only fill one of the Scan value(s) fields.
   Absolute | If you mark this field, the string of characters is found even if it is part of a word. For example, if you scan for the value `meter`, the search would also find words such as parameter and millimeter. If you remove the mark, the search is restricted to match entire words only.
   Immediate | If you mark this field, messages are displayed individually, one after another. Otherwise, a list of messages is displayed after the search is completed. If you specify more than one language or an asterisk (*) in the Language codes field, Immediate must be marked.

3. Specify search criteria as shown in the following example:

       +--------------------------------------+
       !   Scan value(s)       Or/And/Not     !
       !   ----------------    ----------     !
       !   BUFFER__________       AND         !
       !   POOL____________                   !
       !   ________________                   !
       !   ________________                   !
       !                                      !
       !   Absolute ..... X                   !
       !   Immediate .... _                   !
       !                                      !
       +--------------------------------------+

   In the example above, the scan finds all short messages that contain both the words `buffer` and `pool.`

4. Press ENTER.

   All messages to which the specified search criteria apply are listed on the screen as shown in the following example:

       11:32:27              ***** NATURAL SYSERR UTILITY *****             2008-11-28
                                 - Scan in Short Messages -

       Number        Short Message (English)
       ------------- -----------------------------------------------------------------
       NAT0777       Buffer pool full.

       End of scan reached.

       Enter-PF1---PF2---PF3---PF4---PF5---PF6---PF7---PF8---PF9---PF10--PF11--PF12---
       +                 Exit                          +           Crit        Canc

   The word in which the search string is found is highlighted.

   From this screen, you can display the search criteria used for the current scan by pressing PF10.

## Selecting Messages from a List

This function is used to display a range of messages and select single ones for further processing. Only short messages can be displayed.

To select messages

1. In the fields of the SYSERR main menu, enter the following values:

   Field | Input Value
   --- | ---
   Code | `SE`
   Message type |
   `NS` | Natural system short messages
   `US` | User-defined short messages
   Library | Any existing Natural library. If an asterisk (*) is appended to the library ID, a list of all libraries available is displayed for selection.
   Message number | Two numbers of up to four digits corresponding to the first and last numbers of the range of messages to be displayed for selection.
   Language codes | The code of the language in which the messages are to be displayed. If more than one code is specified, only the short message text of the first one is displayed. Enter an asterisk (*) to display the languages available for each message.

2. Press ENTER.

   A Select Messages screen similar to the example below is displayed:

       17:08:13             ***** NATURAL SYSERR UTILITY *****              2008-11-28
                                    - Select Messages -
                                                                        Languages
       Se Number       Short Message (English)                          short     long
       -- ------------ ------------------------------------------------ --------- ----
       __ NAT0001      Missing/invalid syntax; undefined variable name/ 1         1
       __ NAT0002      No file is available with specified name or numb 1         1
       __ NAT0003      Invalid character string for file name or file n 1         1
       __ NAT0004      DEFINE DATA must be the first statement if prese 1         1
       __ NAT0005      Closing parenthesis missing in arithm/logical ex 1         1
       __ NAT0006      ESCAPE statement used when no processing loop ac 1         1
       __ NAT0007      Invalid THRU or TO clause in READ LOGICAL or HIS 1         1
       __ NAT0008      Invalid search syntax.                           1         1
       __ NAT0009      Invalid relational operator in a relational expr 1         1
       __ NAT0010      Error in value specification in a relational exp 1         1
       __
       __
       __
       __
       __
       __

       Enter-PF1---PF2---PF3---PF4---PF5---PF6---PF7---PF8---PF9---PF10--PF11--PF12---
             Help        Exit                          +                       Canc

3. In the Se column, enter one of the following line commands:

   Command | Explanation
   --- | ---
   `DE` | Deletes the message.
   `DI` | Converts the Select Messages screen to the Display Short Messages screen shown in Displaying Messages. Additionally, places the message selected with this command at the top of the list and reduces the number of messages displayed as described for `.X`.
   `LA` | Shows the codes of the languages for which translations exist.
   `MO` | Modifies the message.
   `PR` | Outputs the message on a printer.
   `SH` | Displays the short message. This command is only available if an asterisk (*) has been entered in the Language codes field of the SYSERR main menu.
   `TR` | Translates the message into another language.
   `.X` | Defines a shorter message range by placing a selected message at the top of the list and thus reducing the number of messages displayed: The message selected with this command is placed at the top of the list and any messages that were listed above this message are removed from the display. The message range in the SYSERR main menu is reset accordingly and starts with the message selected here on the Select Messages screen.
   `.Y` | Defines a shorter message range by listing messages only up to a selected message: All messages that were listed below the message selected with this command are removed from the display. The message range in the SYSERR main menu is reset accordingly and ends with the message selected here on the Select Messages screen.

4. Press ENTER to continue.

## Translating Messages into other Languages

This function is used to translate short messages from one language to one or more other languages. To translate long messages into other languages, proceed as described in Adding Messages.

To translate short messages

1. In the fields of the SYSERR main menu, enter the following values:

   Field | Input Value
   --- | ---
   Code | `TR`
   Message type |
   `NS` | Natural system short messages
   `US` | User-defined short messages
   Library | Any existing Natural library.
   Message number | Two numbers of up to four digits corresponding to the first and last numbers of the range of messages to be displayed for selection.
   Language codes | Specify a maximum of nine language codes. The language codes are single alphanumeric characters in the ranges 1 - 9, A - Z and a - y.

2. Press ENTER.

   A Translate Short Message screen similar to the example below appears:

       13:37:14             ***** NATURAL SYSERR UTILITY *****              2009-01-16
       Lower Case ON            - Translate Short Message -

       Number ...... SYSERR0001
       Languages ... 1..45.......................................................

       ------------- ....+....1....+....2....+....3....+....4....+....5....+..
       English       Short message English (1)________________________________________
       German        _________________________________________________________________
       French        _________________________________________________________________
       Spanish       Short message Spanish (4)________________________________________
       Italian       Short message Italian (5)________________________________________
                     _________________________________________________________________
                     _________________________________________________________________
                     _________________________________________________________________
                     _________________________________________________________________
       ------------- ....+....1....+....2....+....3....+....4....+....5....+..

        1 Short message English (1)
        4 Explanation: English long message
       18 Action: English long message

       Enter-PF1---PF2---PF3---PF4---PF5---PF6---PF7---PF8---PF9---PF10--PF11--PF12---
       Mod   Help        Exit                    -     +           Opts        Canc

   The Languages field displays the language codes in which the message already exists (in the example above: 1, 4 and 5).

   The section below Number and Languages lists all languages for which a language code was entered earlier in the Language codes field of the SYSERR main menu (in the example above: 1, 2, 3, 4, 5). English (1), Spanish (4) and Italian (5) translations already exist whereas new translations can be entered for German (2) and French (3).

   For reference purposes, the bottom section of the screen displays three lines of the long message that corresponds to the language that is listed first in the languages/short messages section (in the example above, English). Lines 1, 4 and 18 are displayed by default. You can display any other line of the long message by overwriting any of the three line numbers (1, 4 or 18) with another line number and pressing ENTER.

3. Enter the translation in the input line next to the new language specified.

4. Press ENTER.

To modify translations of short messages

1. On the Translate Short Message screen, press PF10.

   An Options window similar to the example below opens:

       +------------------------ Options ------------------------+
       !                                                         !
       !  Modification of all fields allowed ....... N           !
       !                                                         !
       !  Currently recognized language codes ...... 123456789   !
       !                                                         !
       +---------------------------------------------------------+

2. In the upper field, replace `N` (default) by `Y` and enter the required language code(s) in the lower field. You can specify up to nine new language codes for translation.

To copy a translation into an empty input line

1. On the Translate Short Message screen, enter `.C` in the first two positions of an empty line.

2. Place the cursor anywhere in the line of a short message that already exists for another language. (You can only copy text that appears in display mode.)

3. Press ENTER.

### On this page

- Adding Messages
- Deleting Messages
- Displaying Messages
- Modifying Messages
- Printing Messages
- Scanning Messages
- Selecting Messages from a List
- Translating Messages into other Languages