Compression/Decompression Error Messages

#### Search Results

Search

# Compression/Decompression Error Messages

This section lists the error messages (NUS02nn) that may be issued by the Natural thread compression routine as a result of internal errors.

## NUS0201 - INVALID OP.CODE OR FIRST ENTRY IS NOT THE COMPRESSION BUFFER

Explanation | Internal error.
Action | Send the corresponding dump to support.

## NUS0202 - NUMBER OF TABLE ELEMENTS IS ZERO

Explanation | Internal error.
Action | Send the corresponding dump to support.

## NUS0203 - NUMBER OF TABLE ELEMENTS IS GREATER MAX.

Explanation | Internal error.
Action | Send the corresponding dump to support.

## NUS0204 - TOTAL THREAD LENGTH LOWER COMPRESSED

Explanation | Internal error.
Action | Send the corresponding dump to support.

## NUS0205 - BUFFER TYPE MISSING

Explanation | Internal error.
Action | Send the corresponding dump to support.

## NUS0206 - COMPRESSED BUFFER GREATER TOTAL LENGTH

Explanation | Internal error.
Action | Send the corresponding dump to support.

## NUS0207 - TOTAL LENGTH GREATER UPPER LIMIT

Explanation | The Natural user thread is too small.
Action | Enlarge the Natural user thread.

## NUS0208 - INCORRECT TOTAL BUFFER LENGTH

Explanation | Internal error.
Action | Send the corresponding dump to support.

## NUS0209 - INCORRECT USED BUFFER LENGTH

Explanation | Internal error.
Action | Send the corresponding dump to support.

## NUS0210 - THREAD TOO SMALL FOR DECOMPRESSION

Explanation | The Natural user thread is too small.
Action | Enlarge the Natural user thread.

## NUS0211 - BUFFER OFFSET/ADDRESS NOT POSITIVE

Explanation | Internal error.
Action | Send the corresponding dump to support.

## NUS0212 - ERROR IN BUFFER SORT SEQUENCE

Explanation | Internal error.
Action | Send the corresponding dump to support.

## NUS0213 - INCORRECT BUFFER OVERLAPPING

Explanation | Internal error.
Action | Send the corresponding dump to support.

## NUS0214 - TOTAL OR USED BUFFER LENGTH IS INVALID

Explanation | Internal error.
Action | Send the corresponding dump to support.

## NUS0215 - INVALID THREAD STATUS FOR OPERATION

Explanation | Internal error.
Action | Send the corresponding dump to support.

## NUS0216 - INVALID BUFFER LENGTH IN PREFIX

Explanation | Internal error.
Action | Send the corresponding dump to support.

## NUS0217 - INVALID LENGTH LOW END IN PREFIX

Explanation | Internal error.
Action | Send the corresponding dump to support.

## NUS0218 - INVALID LENGTH HIGH END IN PREFIX

Explanation | Internal error.
Action | Send the corresponding dump to support.

## NUS0219 - INVALID LENGTH BEFORE COMPR. BUFFER

Explanation | Internal error.
Action | Send the corresponding dump to support.

## NUS0220 - CMCCBR CALLED WITH COMPRESSED THREAD

Explanation | Internal error.
Action | Send the corresponding dump to support.

## NUS0221 - CMCCBR THREAD STATUS IS UNDEFINED

Explanation | Internal error.
Action | Send the corresponding dump to support.

## NUS0222 - INVALID BUFFER ID OR EYE CATCHER DESTROYED

Explanation | Internal error.
Action | Send the corresponding dump to support.

## NUS0223 - ERROR FROM CMFREMP FOR OUTSIDE BUFFER

Explanation | Internal error.
Action | Send the corresponding dump to support.

## NUS0224 - PHYS.GETMAIN ERROR FOR A FIXED BUFFER BELOW

Explanation | Internal error.
Action | Send the corresponding dump to support.

## NUS0225 - PHYS.GETMAIN ERROR FOR A VAR.BUFFER BELOW

Explanation | Internal error.
Action | Send the corresponding dump to support.

## NUS0226 - FREE MAIN FOR WORKPOOLS NOT DONE

Explanation | Internal error.
Action | Send the corresponding dump to support.

## NUS0227 - STORAGE OVERFLOW - yyy BYTES GREATER zzz

yyy | represents the number of bytes which exceed the value defined by the keyword parameters `OVSIZE` or `WPSIZE`.
zzz | represents the value defined for the operand of the keyword parameters `OVSIZE` or `WPSIZE` of the macro `NTPRM`.

Explanation | During a physical `GETMAIN`, one of the maximum sizes defined in the keyword parameters `OVSIZE` or `WPSIZE` in the macro `NTPRM` is exceeded.
Action | Increase the maximum size of `OVSIZE` or `WPSIZE` of the macro `NTPRM`.

## NUS0228 - GETMAIN FOR BIT TABLE BUFFER FAILED

Explanation | Internal error.
Action | Send the corresponding dump to support.

### On this page

- NUS0201 - INVALID OP.CODE OR FIRST ENTRY IS NOT THE COMPRESSION BUFFER
- NUS0202 - NUMBER OF TABLE ELEMENTS IS ZERO
- NUS0203 - NUMBER OF TABLE ELEMENTS IS GREATER MAX.
- NUS0204 - TOTAL THREAD LENGTH LOWER COMPRESSED
- NUS0205 - BUFFER TYPE MISSING
- NUS0206 - COMPRESSED BUFFER GREATER TOTAL LENGTH
- NUS0207 - TOTAL LENGTH GREATER UPPER LIMIT
- NUS0208 - INCORRECT TOTAL BUFFER LENGTH
- NUS0209 - INCORRECT USED BUFFER LENGTH
- NUS0210 - THREAD TOO SMALL FOR DECOMPRESSION
- NUS0211 - BUFFER OFFSET/ADDRESS NOT POSITIVE
- NUS0212 - ERROR IN BUFFER SORT SEQUENCE
- NUS0213 - INCORRECT BUFFER OVERLAPPING
- NUS0214 - TOTAL OR USED BUFFER LENGTH IS INVALID
- NUS0215 - INVALID THREAD STATUS FOR OPERATION
- NUS0216 - INVALID BUFFER LENGTH IN PREFIX
- NUS0217 - INVALID LENGTH LOW END IN PREFIX
- NUS0218 - INVALID LENGTH HIGH END IN PREFIX
- NUS0219 - INVALID LENGTH BEFORE COMPR. BUFFER
- NUS0220 - CMCCBR CALLED WITH COMPRESSED THREAD
- NUS0221 - CMCCBR THREAD STATUS IS UNDEFINED
- NUS0222 - INVALID BUFFER ID OR EYE CATCHER DESTROYED
- NUS0223 - ERROR FROM CMFREMP FOR OUTSIDE BUFFER
- NUS0224 - PHYS.GETMAIN ERROR FOR A FIXED BUFFER BELOW
- NUS0225 - PHYS.GETMAIN ERROR FOR A VAR.BUFFER BELOW
- NUS0226 - FREE MAIN FOR WORKPOOLS NOT DONE
- NUS0227 - STORAGE OVERFLOW - yyy BYTES GREATER zzz
- NUS0228 - GETMAIN FOR BIT TABLE BUFFER FAILED