Natural System Error Messages 5850-5899

#### Search Results

Search

# Natural System Error Messages 5850-5899

#### NAT5850: Error :1: when processing VTOC.

#### NAT5851: File not on volume.

    Text
    ESY5851 File not on volume.
    Explanation
    The requested file does not exist on the specified volume.
    Action
    No action is required.

#### NAT5852: No password supplied / VSAM data space.

    Text
    ESY5852 No password supplied / VSAM data space.
    Explanation
    No password was specified before attempting to access a password
    protected VSAM file.
    Action
    Specify a password.

#### NAT5853: Retention cycle unexpired / NEWNAME exists.

    Text
    ESY5853 Retention cycle unexpired / NEWNAME exists.
    Explanation
    A VTOC-UPDATE RENAME function was attempted; however, the retention
    cycle is unexpired, and the NEWNAME still exists.
    Action
    Specify a different NEWNAME, or wait until the retention cycle has
    expired.

#### NAT5854: Permanent I/O error.

    Text
    ESY5854 Permanent I/O error.
    Explanation
    A permanent I/O error was detected.
    Action
    This is probably a hardware error. Contact data center personell.

#### NAT5855: Volume not mounted.

    Text
    ESY5855 Volume not mounted.
    Explanation
    The requested volume was not mounted.
    Action
    Make sure that the volume is mounted before re-issuing the request.

#### NAT5856: Operator unable to mount volume.

    Text
    ESY5856 Operator unable to mount volume.
    Explanation
    The operator is not able to mount the volume.
    Action
    No action is required.

#### NAT5857: File in use.

    Text
    ESY5857 File in use.
    Explanation
    The file is in use.
    Action
    Retry later.

#### NAT5858: Not authorized.

    Text
    ESY5858 Not authorized.
    Explanation
    A security violation was detected.
    Action
    No action is required.

#### NAT5859: File definition not deleted by RACF.

    Text
    ESY5859 File definition not deleted by RACF.
    Explanation
    The file definition has not been deleted by RACF.
    Action
    Execute RACF file deletion.

#### NAT5860: Member under MSHP control or changed with MSHP bypass.

    Text
    ESY5860 Member under MSHP control or changed with MSHP bypass.
    Explanation
    The member to be overwritten is under MSHP control or was changed with
    MSHP bypass.
    Action
    Use MSHP=YES to indicate MSHP bypass required.

#### NAT5861: Member contains SYSIPT data.

    Text
    ESY5861 Member contains SYSIPT data.
    Explanation
    Member to be overwritten contains SYSIPT data.
    Action
    Use INLINE-DATA=YES to confirm SYSIPT data required,
    or INLINE-DATA=OFF to switch off the SYSIPT indicator.

#### NAT5870: RECORD field not in search buffer.

    Text
    ESY5870 RECORD field not in search buffer.
    Explanation
    RECORD must be specified for WRITE-FILE.
    Action
    Specify RECORD value.

#### NAT5871: MEMBER/MEMBER-TYPE not specified.

    Text
    ESY5871 MEMBER/MEMBER-TYPE not specified.
    Explanation
    The member name and/or type was not specified.
    Action
    Specify a member name and/or type.

#### NAT5872: Record format not supported.

    Text
    ESY5872 Record format not supported.
    Explanation
    The record format of the desired data set is not supported.
    Action
    No action is required.

#### NAT5873: RECORD-LENGTH missing.

    Text
    ESY5873 RECORD-LENGTH missing.
    Explanation
    The RECORD-LENGTH value is missing.
    Action
    Specify RECORD-LENGTH value.

#### NAT5874: RECORD-LENGTH > LRECL.

    Text
    ESY5874 RECORD-LENGTH > LRECL.
    Explanation
    The specified RECORD-LENGTH value is greater than the LRECL of
    the data set.
    Action
    Specify valid RECORD-LENGTH value.

#### NAT5875: Position of data field > RECORD-LENGTH.

    Text
    ESY5875 Position of data field > RECORD-LENGTH.
    Explanation
    Invalid parameter specified.
    Action
    Check program and correct error.

#### NAT5876: No NEW-field for CHANGE request.

    Text
    ESY5876 No "NEW-" field for CHANGE request
    Explanation
    No NEW-CLASS, NEW-DESTINATION or NEW-USERID field was supplied
    for the CHANGE request.
    Action
    Supply "NEW-" value.

#### NAT5877: VSAM (SHOWCAT) processing error.

    Text
    ESY5877 VSAM (SHOWCAT) processing error.
    Explanation
    A SHOWCAT error was detected when processing the requested VSAM
    file. This generally indicates that the requested file is not a
    a VSAM cluster or non-VSAM file, but rather a VSAM catalog or
    other VSAM non-file object.  Information cannot be displayed
    about this file.

#### NAT5878: Volume defined as DYNAM/D pool name.

    Text
    ESY5878 Volume defined as DYNAM/D pool name.
    Explanation
    The requested volume is defined to Entire System Server as a DYNAM/D
    "virtual" pool name. The requested function cannot be performed.

#### NAT5881: Error occurred while opening file.

    Text
    ESY5881 Error occurred while opening file.
    Explanation
    An error occurred during OPEN.
    Action
    Check the status of the data set.

#### NAT5882: Error occurred while closing file.

    Text
    ESY5882 Error occurred while closing file.
    Explanation
    An error occurred during CLOSE.
    Action
    Check the status of the data set.

#### NAT5883: Data set is full.

    Text
    ESY5883 Data set is full.
    Explanation
    The data set is full.
    Action
    Compress the PDS, or increase the data set size.

#### NAT5886: Event is in use.

    Text
    ESY5886 Event is in use.
    Explanation
    An attempt was made to delete an event someone was waiting for.
    Action
    Issue "POST" request prior to delete an event.

#### NAT5887: Event is already defined.

    Text
    ESY5887 Event is already defined.
    Explanation
    An attempt was made to define an event which already exists.
    Action
    No action is required.

#### NAT5888: Event name must be specified.

    Text
    ESY5888 Event name must be specified.
    Explanation
    An EVENTING request was issued without specifying the EVENT-NAME.
    Action
    Specify an EVENT-NAME.

#### NAT5889: Permanent I/O error while writing data set.

    Text
    ESY5889 Permanent I/O error while writing data set.
    Explanation
    An I/O error was detected during WRITE access.
    Action
    This is probably a hardware error. Contact data center personell.

#### NAT5890: Event does not exist.

    Text
    ESY5890 Event does not exist.
    Explanation
    The specified event does not exist.
    Action
    No action is required.

#### NAT5891: Timeout waiting for event.

    Text
    ESY5891 Timeout while waiting for event.
    Explanation
    A timeout happened before the event was posted.
    Action
    No action is required.

#### NAT5893: Getmain failed.

    Text
    ESY5893 Getmain failed.
    Explanation
    There was not sufficient storage available to proceed with the request.
    Action
    Notify systems programmer.

#### NAT5894: Enable Eventing failed.

    Text
    ESY5894 Enable Eventing failed.
    Explanation
    Internal eventing error occurred.
    Action
    Contact your Software AG technical support representative.

#### NAT5895: :1: must be specified.

    Text
    ESY5895 :1: must be specified.
    Explanation
    Required value :1: was not specified.
    Action
    Provide required value.

#### NAT5896: Error occurred when sending E-Mail.

    Text
    ESY5896 Error occurred when sending E-Mail.
    Explanation
    Severe error occurred during E-MAIL processing. Further information
    are returned in field SYSTEM-MESSAGE to identify subfunction and
    response code.
    Action
    Please contact Software AG support.

#### NAT5897: Mailer response: :1:.

    Text
    ESY5897 Mailer response :1:.
    Explanation
    Error :1: occurred during E-MAIL processing in Mailer function.
    E-MAIL was not delivered to recipient(s) if serious error occurred.
    Action
    Please contact Entire System Server Administrator. Mailer report may
    contain further error diagnostics.

#### NAT5899: Permanent I/O error while reading data set.

    Text
    ESY5899 Permanent I/O error while reading data set.
    Explanation
    An I/O error was detected during READ access.
    Action
    This is probably a hardware error. Contact data center personell.