Natural System Error Messages 9900-9949

#### Search Results

Search

# Natural System Error Messages 9900-9949

#### NAT9901: Natural/TSO runtime environment is not TSO.

    Text
    Natural/TSO runtime environment is not TSO.
    Explanation
    Natural/TSO has been started in a non-TSO environment.
    Action
    Natural/TSO can run in a TSO environment only. Link the appropriate
    frontend interface for this environment to your nucleus.

#### NAT9902: Dataset cannot be opened - :1:.

    Text
    Dataset cannot be opened - ....
    Explanation
    The required dataset cannot be opened. Either it is not or
    incorrectly defined in the JCL, or it cannot be opened due to other
    reasons.
    Action
    Supply the correct dataset definition in the JCL. Check for
    operating-system error messages in the job log to ascertain the cause
    of the error.

#### NAT9903: NATSTUB not linked to Natural nucleus :1:.

    Text
    NATSTUB not linked to Natural nucleus :1:.
    Explanation
    Either the module NATSTUB is not linked to the Natural nucleus; or
    the shared nucleus :1: has been loaded; but NATSTUB is not defined
    as its entry point.
    Action
    Link the module NATSTUB to the Natural nucleus. If a shared nucleus
    is used, specify CMSTUB as its entry point in the link job.

#### NAT9904: Invalid Natural nucleus - :1:.

    Text
    Invalid Natural nucleus - ....
    Explanation
    The version of the Natural nucleus module, as indicated in the error
    message, does not correspond to the front-end interface module.
    For example, the front-end has loaded a shared nucleus of a different
    version.
    Action
    Link the correct Natural nucleus; or specify a correct shared nucleus
    name, using the profile parameter NUCNAME.

#### NAT9905: Terminal I/O error - :1:: RC=:2:.

    Text
    Terminal I/O error - :1:: RC=:2:.
    Explanation
    A terminal I/O error has occurred. The I/O response code RC=:2:
    indicates the reason for the failure of request :1:.
    Under TSO, the response code comes from the failing TSO I/O request
    macro TPUT or TGET.
    Action
    Check the meaning of the response code in the TSO documentation.
    Contact Software AG Support for further problem analysis.

#### NAT9906: Natural server cannot run as LE main routine.

    Text
    Natural server cannot run as LE main routine.
    Explanation
    The Natural front-end (NATOS) received control from a front-end server
    stub which did not initialize the IBM language environment. NATOS is
    linked with LE support and cannot run as an LE main routine.
    Action
    Either link NATOS without LE support or generate the front-end server
    stub with LE support if possible.

#### NAT9907: Unsupported operating-system version.

    Text
    Unsupported operating-system version.
    Explanation
    The current operating-system version is not supported by this
    Natural version.
    Action
    See Natural documentation for supported operating systems and versions.

#### NAT9908: Nucleus module does not reside below 16 MB line - :1:

    Text
    Nucleus module does not reside below 16 MB line - ...
    Explanation
    The nucleus module specified in the message must be executed
    below the 16 MB line due to operating-system requirements.
    Action
    Re-link the specified nucleus module with parameter MODE RMODE(24).

#### NAT9909: Unsupported teleprocessing system version.

    Text
    Unsupported teleprocessing system version.
    Explanation
    This version of the teleprocessing system (e.g. Com-plete) is not
    supported by Natural. It is either an old version which does not
    contain the facilities required by Natural, or a new version which is
    not yet supported by your version of Natural.
    Action
    Either install a newer version of the teleprocessing system,
    or install a newer version of Natural.

#### NAT9910: Session communication area missing or invalid.

    Text
    Session communication area missing or invalid.
    Explanation
    The Natural server session communication area is missing or invalid.
    The session communication area is internally used by the Natural
    server and must be supplied by the front-end server stub.
    Action
    Contact Software AG Support for further problem analysis.

#### NAT9911: Invalid storage thread size specified.

    Text
    Invalid storage thread size specified.
    Explanation
    Running Natural as a server requires the acquisition of main-storage
    threads of a fixed size. The thread size defined by the front-end
    server stub is invalid. It must be in the range from 256 kilobytes
    to 16 megabytes.
    Action
    Specify a correct thread size in the front-end server stub definitions.

#### NAT9912: The number of threads is invalid or too high.

    Text
    The number of threads is invalid or too high.
    Explanation
    Running Natural as a server requires the acquisition of main-storage
    threads. The number of threads defined by the front-end server stub
    is invalid or too great. It must be in the range from 0 to 8191, and
    the total thread storage must be less than 2 gigabytes.
    Action
    Reduce the number of threads or the thread size in the front-end
    server stub definitions.

#### NAT9913: Server environment already initialized.

    Text
    Server environment already initialized.
    Explanation
    The front-end server stub requested Natural to initialize the server
    environment, but the server environment has already been initialized.
    Action
    Terminate the server environment before restarting it.
    Contact Software AG Support for further problem analysis.

#### NAT9914: GETMAIN for common server table failed.

    Text
    GETMAIN for common server table failed.
    Explanation
    The Natural server environment cannot be initialized because the
    GETMAIN for its central control block has failed. Sufficient region
    storage must be available.
    Action
    Increase the region size for the Natural server. If the problem cannot
    be solved, contact SAG technical support for further problem analysis.

#### NAT9915: GETMAIN for thread storage failed.

    Text
    GETMAIN for thread storage failed.
    Explanation
    The Natural server environment cannot be initialized because a
    GETMAIN for its storage threads has failed. Sufficient region
    storage must be available.
    Action
    Increase the region size for the Natural server or reduce the number
    or the size of its storage threads in the frontend stub definitions.

#### NAT9916: Error retrieving server name token. RC=:1:.

    Text
    Error retrieving server name token. RC=....
    Explanation
    The central anchor for the Natural server is an MVS name token.
    The retrieve request for the name token has failed with the decimal
    return code shown in the message. The explanation of the return code
    can be found in the IBM MVS Authorized Assembler Services Reference
    under the IEANTRT macro call description.
    Action
    If you cannot find the reason for the problem and correct it, contact
    Software AG technical support for further problem analysis.

#### NAT9917: Error creating server name token. RC=:1:.

    Text
    Error creating server name token. RC=....
    Explanation
    The central anchor for the Natural server is an MVS name token.
    The create request for the name token has failed with the decimal
    return code shown in the message. The explanation of the return code
    can be found in the IBM MVS Authorized Assembler Services Reference
    under the IEANTCR macro call description.
    Action
    If you cannot find the reason for the problem and correct it, contact
    Software AG technical support for further problem analysis.

#### NAT9918: Error deleting server name token. RC=:1:.

    Text
    Error deleting server name token. RC=....
    Explanation
    The central anchor for the Natural server is an MVS name token.
    The delete request for the name token has failed with the decimal
    return code shown in the message. The explanation of the return code
    can be found in the IBM MVS Authorized Assembler Services Reference
    under the IEANTDL macro call description.
    Action
    If you cannot find the reason for the problem and correct it, contact
    Software AG technical support for further problem analysis.

#### NAT9919: Invalid server function code.

    Text
    Invalid server function code.
    Explanation
    The frontend server stub called the Natural server with an
    invalid server function code.
    Action
    Contact SAG technical support for further problem analysis.

#### NAT9920: Roll server not active. SUBSID=:1:.

    Text
    Roll server not active. SUBSID=:1:.
    Explanation
    The Natural server environment requires the Natural roll server for
    running multiple server sessions within a limited number of storage
    threads. Either there is no roll server started for the specified
    Natural subsystem ID or the SUBSID profile parameter is incorrectly
    or dynamically specified in the Natural parameter module.
    Action
    Start the Natural roll server for the subsystem ID or set the SUBSID
    profile parameter correctly or use SUBSID=" " to run without a roll
    server or specify this in the frontend server stub definitions.

#### NAT9921: Server environment not initialized.

    Text
    Server environment not initialized.
    Explanation
    The frontend server stub called Natural with a server function
    code other than "initialize server" and the Natural server
    environment is in uninitialized state.
    Action
    Restart the frontend server stub to reset its state completely.
    Contact SAG technical support for further problem analysis.

#### NAT9922: The initialization session cannot be rolled.

    Text
    The initialization session cannot be rolled.
    Explanation
    The frontend server stub requested a session create, roll-out
    or roll-in server function while the Natural server was initializing.
    During the server initialization phase these server functions are
    not allowed.
    Action
    Contact SAG technical support for further problem analysis.

#### NAT9923: No server clone session available.

    Text
    No server clone session available.
    Explanation
    The frontend server stub requested a session create but the
    clone session had not been saved yet.
    Action
    Contact SAG technical support for further problem analysis.

#### NAT9924: Session ID missing or invalid.

    Text
    Session ID missing or invalid.
    Explanation
    The Natural server session ID is a unique internal ID to identify
    a Natural session. The frontend server stub passed either no
    session ID or a hexadecimal null session ID which is not allowed
    or the session ID hads been modified.
    Action
    Contact SAG technical support for further problem analysis.

#### NAT9925: Session ID already exists.

    Text
    Session ID already exists.
    Explanation
    The front-end server stub requested a "session create" but a
    session with the same session ID exists already and
    is ready to run.
    Action
    Contact Software AG Support for further problem analysis.

#### NAT9926: Session not in rolled-in status.

    Text
    Session not in rolled-in status.
    Explanation
    The frontend server stub requested a session roll-out, execute
    or save clone function, but the session is not in rolled-in state.
    Action
    Contact SAG technical support for further problem analysis.

#### NAT9927: Session not in rolled-out status.

    Text
    Session not in rolled-out status.
    Explanation
    The frontend server stub requested a session roll-in function,
    but the session is not in rolled-out state.
    Action
    Contact SAG technical support for further problem analysis.

#### NAT9928: Compression failed during roll-out. RC=:1:.

    Text
    Compression failed during roll-out. RC=....
    Explanation
    The Natural thread storage compression failed. The exact reason
    is indicated by the decimal return code RC=00nn. It is explained in
    the Natural documentation.
    Action
    Contact Software AG support for further problem analysis.

#### NAT9929: Decompression failed during roll-in. RC=:1:.

    Text
    Decompression failed during roll-in. RC=....
    Explanation
    The Natural thread storage decompression failed. The exact reason
    is indicated by the decimal return code RC=00nn. It is explained in
    the Natural documentation.
    Action
    Contact SAG technical support for further problem analysis.

#### NAT9930: GETMAIN failed for roll buffer.

    Text
    GETMAIN failed for roll buffer.
    Explanation
    During Natural session thread storage roll-out the GETMAIN request
    for the roll buffer failed. Sufficient region storage must be
    available to save the compressed session storage.
    Action
    Increase the region size for the Natural server or use the Natural
    roll server as roll facility.

#### NAT9931: The AUTOTERM facility cannot be initialized.

    Text
    The AUTOTERM facility cannot be initialized.
    Explanation
    In a Natural server environment, the automatic server termination
    facility helps to avoid problems caused by an unintended DETACH of
    the server initialization TCB (e.g. MVS abends A03, no server resource
    cleanup etc.). The AUTOTERM facility cannot be initialized due to
    storage protection problems.
    Action
    Disable the AUTOTERM facility in the frontend server stub definitions
    or contact SAG technical support for further problem analysis.

#### NAT9932: Natural runtime error occurred - :1:.

    Text
    Natural runtime error occurred - :1:.
    Explanation
    During the execution of a Natural server session, the indicated
    Natural runtime error :1: occurred.
    Action
    Check the complete runtime error message issued by Natural.
    It can be found either in the return data on the client side
    or in the Natural standard output dataset of the server.

#### NAT9933: Roll server ALLOCATE request failed. RC=:1:/:2:.

    Text
    Roll server ALLOCATE request failed. RC=.../....
    Explanation
    During session creation, the ALLOCATE request for a new roll-file slot
    failed. Sufficient roll-file storage must be available. The reason
    for the failure is indicated by the decimal return/reason codes. These
    are explained in the Natural documentation.
    Action
    If you cannot find the reason for the problem and correct it, contact
    Software AG support for further problem analysis.

#### NAT9934: Roll server WRITE request failed. RC=:1:/:2:.

    Text
    Roll server WRITE request failed. RC=.../....
    Explanation
    During session roll-out, the WRITE request to the Natural roll server
    failed. The reason for the failure is indicated by the decimal
    return/reason codes. These are explained in the Natural documentation.
    Action
    If you cannot find the reason for the problem and correct it, contact
    Software AG support for further problem analysis.

#### NAT9935: Roll server READ request failed. RC=:1:/:2:.

    Text
    Roll server READ request failed. RC=:1:/:2:.
    Explanation
    During session roll-in the READ request from the Natural roll server
    failed. The reason for the failure is indicated by the decimal
    return/reason codes. These are explained in the Natural Documentation.
    Action
    If you cannot find the reason for the problem and correct it, contact
    SAG technical support for further problem analysis.

#### NAT9936: Roll server FREE request failed. RC=:1:/:2:.

    Text
    Roll server FREE request failed. RC=.../....
    Explanation
    During session termination, the FREE request to the Natural roll
    server failed. The reason for the failure is indicated by the
    decimal return/reason codes. These are explained in the Natural
    documentation.
    Action
    If you cannot find the reason for the problem and correct it, contact
    Software AG support for further problem analysis.

#### NAT9937: Server I/O subtask cannot be started. RC=:1:/:2:.

    Text
    Server I/O subtask cannot be started. RC=:1:/:2:.
    Explanation
    In the Natural server environment, the whole I/O handling is done
    by a separate MVS subtask, started during server initialization.
    The ATTACH request for the I/O subtask failed. The reason for the
    failure is indicated by RC=:1:/:2:, where :1: is the decimal return
    code of the internal function code :2:.
    Action
    Contact Software AG Support for further problem analysis.

#### NAT9938: Termination of SMARTS environment failed.

    Text
    Termination of SMARTS environment failed.
    Explanation
    No further explanation available.
    Action
    Contact Software AG support.

#### NAT9939: :1: RC=:2:

    Text
    Remote front-end communication error. RC=...
    Explanation
    A Natural server environment uses the Natural remote front-end to
    dispatch a Natural session in a remote TP environment. This is used,
    for example, by the CICS or IMS Adapter for NDV or NWO.
    This error indicates an error in the communication between the
    Natural server environment and the remote TP environment.
    The meaning of the RC value depends on the error text. For example:
    - "Cannot load NCI front-end RC= ":
      RC contains the CICS EIB response code.
    - "Error at Remote Gateway Obtain/Restore":
      RC contains the response code from the NDV remote gateway.
    Action
    In case of a CICS EIB response code, examine the CICS messages or the
    remote front-end trace for further error information.
    In case of a remote gateway RC, contact Software AG technical support.

#### NAT9940: Server parameter list(s) missing or invalid.

    Text
    Server parameter list(s) missing or invalid.
    Explanation
    A mandatory Natural server parameter list is missing or invalid.
    A Natural front-end server stub communicates with a Natural server
    session using internal parameter lists, which are mandatory
    depending on the internal server function.
    Action
    Contact Software AG Support for further problem analysis.

#### NAT9941: Wrong Smarts version for use of LE/370.

    Text
    Wrong Smarts version for use of LE/370.
    Explanation
    Smarts version V272 is required to support the CEEPIPI interface for
    LE/370 programs.
    Action
    Install the required Smarts version.

#### NAT9942: Server Front-End incompatible with Natural version.

    Text
    Server Front-End incompatible with Natural version.
    Explanation
    The Front-End Server Stub requires a Natural version different from
    the version of the current Natural environment-dependent nucleus.
    Action
    Install and use a compatible Natural version according to the
    Front-End Server Stub documentation.

#### NAT9943: Logic error in Natural program for asynchronous session.

    Text
    Logic error in Natural program for asynchronous session.
    Explanation
    Input data requested, but an asynchronous session runs without any
    input device.
    To avoid this error situation, check the Natural system variable
    *SCREEN-IO.
    Action
    Correct the program logic.

#### NAT9944: Roll server COMPRESS request failed. RC=:1:/:2:.

    Text
    Roll server COMPRESS request failed. RC=.../....
    Explanation
    During session roll-out, the COMPRESS request to the Natural roll server
    failed. The reason for the failure is indicated by the decimal
    return/reason codes. These are explained in the Natural documentation.
    Action
    If you cannot find the reason for the problem and correct it, contact
    Software AG support for further problem analysis.

#### NAT9945: Roll server DECOMPRESS request failed. RC=:1:/:2:.

    Text
    Roll server DECOMPRESS request failed. RC=.../....
    Explanation
    During session roll-in, the DECOMPRESS request from the Natural roll
    server failed. The reason for the failure is indicated by the decimal
    return/reason codes. These are explained in the Natural documentation.
    Action
    If you cannot find the reason for the problem and correct it, contact
    Software AG support for further problem analysis.