NGU-CLIENT-EXECUTE Subprogram

#### Search Results

Search

# NGU-CLIENT-EXECUTE Subprogram

This document covers the following topics:

- Natural Object Name

- Description

- Parameters

## Natural Object Name

NGUCLEXE

## Description

Requests the server identified by DDE-VIEW.CONV-ID to execute a command. The field DDE-VIEW.DATA describes the command to be executed.

## Parameters

Name/Data Type | Explanation
--- | ---
1 DDE-VIEW | Input/Output PDA for DDE subprograms.
2 SERVICE (A20) | Service name.
2 TOPIC (A20) | Topic name.
2 CONV-ID (I4) | Conversation ID.
2 MESSAGE (A20) | Message information.
2 ITEM (A20) | Item of current conversation.
2 FORMAT (A20) | Format of data to be sent.
2 TIMEOUT (I4) | Time interval before the conversation is interrupted because there is no server message.
2 DATALEN (I2) | Length of data.
2 DATA-ARRAY (A1/1:V) |
1 Max-Index (I2) | Input Highest index of DATA-ARRAY; can be set to any I2 value.
1 Response (I4) | Output Natural error (if applicable).

### On this page

- Natural Object Name
- Description
- Parameters