Natural System Error Messages 5800-5849

#### Search Results

Search

# Natural System Error Messages 5800-5849

#### NAT5800: Specified level is a data set name.

    Text
    ESY5800 Specified level is a data set name.
    Explanation
    The specified level name is a data set name.
    Action
    No action is required.

#### NAT5801: Job not found.

    Text
    ESY5801 Job not found.
    Explanation
    The requested job was not found.
    Action
    No action is required.

#### NAT5802: GETMAIN for CSA area failed.

    Text
    ESY5802 GETMAIN for CSA area failed.
    Explanation
    An attempt was made to access main storage, and GETMAIN for the CSA
    area failed.
    Action
    Notify the systems programmer.

#### NAT5803: Cannot access data.

    Text
    ESY5803 Cannot access data.
    Explanation
    An attempt was made to access main storage, and the data specified
    cannot be accessed.
    Action
    No action is required.

#### NAT5804: Request to access data has timed out.

    Text
    ESY5804 Request to access data has timed out.
    Explanation
    Main storage was accessed, and SRB was scheduled to run in an address
    space. SRB must be completed within 10 seconds.
    Action
    No action is required.

#### NAT5805: Invalid TCB address.

    Text
    ESY5805 Invalid TCB address.
    Explanation
    An invalid TCB-ADDRESS was specified.
    Action
    Specify valid TCB-ADDRESS.

#### NAT5806: Permanent I/O error on catalog.

    Text
    ESY5806 Permanent I/O error on catalog.
    Explanation
    A permanent I/O error occurred while accessing the catalog.
    Action
    This may be a hardware error. Contact data center personell.

#### NAT5807: Invalid track address.

    Text
    ESY5807 Invalid track address.
    Explanation
    An invalid track address was specified.
    Action
    Specify valid track address.

#### NAT5808: SRB failed RC :1: CMP :2: RET :3: RSN :4:

    Text
    SRB failed RC :1: CMP :2: RET :3: RSN :4:
    Explanation
    A request failed to schedule an SRB. The return, completion and reason
    codes provide more information about the type of the failure.
    Action
    Contact technical support.

#### NAT5809: Subsystem not active.

    Text
    ESY5809 Subsystem not active.
    Explanation
    The related subsystem has not been started properly. Therefore, the
    requested function is not available in this run of ESY.
    The following views return this error code on BS2000:
     - views SPOOL-QUEUE, SPOOL-FILES, WRITE-SPOOL if SPOOL=NONE is defined;
     - views SEND-MESSAGE, CONSOLE if CONSOLE task is not running;
     - views CONSOLE, EVENTING if EVENTING task is not running.
    Action
    Contact your administrator to get the subsystem started for the next
    NPR run.

#### NAT5810: Error detected in catalog, processing terminated.

    Text
    ESY5810 Error detected in catalog, processing terminated.
    Explanation
    An error in the catalog structure was detected.
    Action
    Notify the systems programmer.

#### NAT5811: Specified level is an empty index.

    Text
    ESY5811 Specified level is an empty index.
    Explanation
    The level specified is an empty index.
    Action
    No action is required.

#### NAT5820: Unknown command.

    Text
    ESY5820 Unknown command.
    Explanation
    A command which is not known to Entire System Server was entered.
    Action
    Check the spelling and the syntax of the command. Check to see whether
    the command is a Natural command.

#### NAT5821: Job no longer active.

    Text
    ESY5821 Job no longer active.
    Explanation
    An attempt was made to access a job which is no longer active.
    Action
    No action required.

#### NAT5822: Logical error on JES3 spool.

    Text
    ESY5822 Logical error on JES3 spool.
    Explanation
    A logical error occurred while reading the JES3 spool data set.
    Action
    Try again. If error persists, it may indicate a bad control block on the
    JES3 spool (which may be caused by a hardware error).

#### NAT5823: Requested job in input queue.

    Text
    ESY5823 Requested job in input queue.
    Explanation
    An attempt was made to access output data of a job which is in the
    input queue.
    Action
    Wait until job is processed.

#### NAT5824: I/O error on JES3 spool.

    Text
    ESY5824 I/O error on JES3 spool.
    Explanation
    A READ operation to JES3 spool failed to complete normally.
    Action
    Probably a hardware failure. A JES3 warmstart (with analysis) should
    be considered.

#### NAT5825: JES3 command data set is full.

    Text
    ESY5825 JES3 command data set is full.
    Explanation
    A WRITE operation to the JES3 command data set failed because the
    data set is full.
    Action
    Wait until space becomes available.

#### NAT5826: I/O error on JES3 command data set failed.

    Text
    ESY5826 I/O error on JES3 command data set.
    Explanation
    A WRITE attempt to the JES3 command data set failed.
    Action
    This is probably a hardware error. If error persists, it may be
    advisable to relocate the JES3 command data set.

#### NAT5830: JES interface is not active.

    Text
    ESY5830 JES interface is not active.
    Explanation
    The JES interface is not active.
    Action
    Check the JES parameter in the Entire System Server parameter file.

#### NAT5831: Error during queue initialization.

    Text
    ESY5831 Error during queue initialization.
    Explanation
    An error occurred while reading JES control blocks.
    Action
    This is probably a hardware error. Contact data center personell.

#### NAT5832: Error during queue open.

    Text
    ESY5832 Error during queue open.
    Explanation
    An error occurred during open of JES spool data set.
    Action
    Check with the systems programmer.

#### NAT5833: You are not allowed to alter this job.

    Text
    ESY5833 You are not allowed to alter this job.
    Explanation
    An attempt was made to alter a job. The user is not authorized to alter
    the specified job. This error message is issued by the security system
    with which Entire System Server interfaces.
    Action
    No action is required.

#### NAT5834: Command failed, MGCRE RC = :1:.

    Text
    ESY5834 Command failed, MGCRE RC = ....
    Explanation
    A request failed to issue an internal JES or system command.
    Action
    Check with the systems programmer. Contact technical support.

#### NAT5840: VTAM operator ACB is not open.

    Text
    ESY5840 VTAM operator ACB is not open.
    Explanation
    The VTAM operator ACB was not opened successfully during initialization.
    Action
    Either active VTAM support has not been requested by the system
    parameters, or an open error occurred during initialization.
    The job-log contains further information.

#### NAT5841: Error in SENDCMD - RTNCD=:1: FDBK2=:2:.

    Text
    ESY5841 Error in SENDCMD - RTNCD=... FDBK2=....
    Explanation
    A VTAM error occurred while sending a command.
    Note: A more detailed message is returned when field
          ERROR-TEXT is specified.
    Action
    Check the command requested. The RTNCD and FDBK2 values are defined
    in the appropriate VTAM documentation.

#### NAT5842: Invalid VTAM command.

    Text
    ESY5842 Invalid VTAM command.
    Explanation
    An invalid VTAM command was requested.
    Action
    No action is required.

#### NAT5843: Printer is not available.

#### NAT5844: Buffer is waiting to be printed.

#### NAT5845: Printer is active for user :1:.

    Text
    ESY5845 Printer is active for user ....
    Explanation
    Another user is working with the printer.
    Action
    Wait until printer is not busy anymore.

#### NAT5846: Use function STATUS to get results.

#### NAT5847: Print mode ASIS error.

#### NAT5849: Print failed. Fct=:1: FD=:2: S=:3:.

    Text
    ESY5849 Print failed. Fct=... FD=... S=....
    Explanation
    The print request failed. For further details check the variable data
    of FUNCTION, FEEDBACK and STATUS. You may find the explanation of these
    fields in the VTAM documentation.
    Action
    Please contact your systems programmer.