Natural System Error Messages 1150-1199

#### Search Results

Search

# Natural System Error Messages 1150-1199

#### NAT1150: Attribute buffer overflow.

    Text
    Attribute buffer overflow.
    Explanation
    An overflow of the attribute buffer is caused by too many
    attributes for one logical page.
    Action
    Reduce the number of fields on one page.

#### NAT1151: Invalid access to Natural system function.

    Text
    Invalid access to Natural system function.
    Explanation
    An invalid access to a Natural system function was attempted.
    For example, an attempt was made to assign a value to a
    read-only function.
    Action
    Check program and correct error.

#### NAT1152: Invalid function in screen paging.

    Text
    Invalid function in screen paging.
    Explanation
    An invalid function code was entered during screen-page processing.
    Action
    Enter a valid function code.

#### NAT1153: Requested screen pages are not available.

    Text
    Requested screen pages are not available.
    Explanation
    Screen pages were requested during screen paging,
    but these pages are not available.
    Action
    Correct error.

#### NAT1155: Reporting mode not permitted.

    Text
    Reporting mode not permitted.
    Explanation
    Switching to reporting mode is not permitted if Natural was started
    with structured mode (parameter SM=ON).
    Switching to reporting mode can be done via the GLOBALS command.
    Action
    Make sure you are using the correct programming mode.

#### NAT1156: Statement not possible within TOP OF PAGE or END OF PAGE.

    Text
    Statement not possible within TOP OF PAGE or END OF PAGE.
    Explanation
    The specified statement must not be specified within an
    AT TOP OF PAGE or AT END OF PAGE statement block.
    Action
    Correct error in program.

#### NAT1157: Invalid format of operand.

    Text
    Invalid format of operand.
    Explanation
    During runtime, the format of an operand is not contained in the list
    of valid formats.
    Action
    Contact SAG support.

#### NAT1160: Error in "Recording" activation.

    Text
    Error in "Recording" activation.
    Explanation
    This error is caused by one of the following:
    - The requested recording has not been found.
    - You have specified no recording name.
    - For a new recording, you have specified the name of an already
      existing recording.
    Action
    Make sure you use the right recording name in the right library.

#### NAT1161: DBCS: Invalid SO/SI pair in line :1: column :2:.

    Text
    DBCS: Invalid SO/SI pair in line ... column ....
    Explanation
    Natural checks the correct pairing of SO/SI for
    DBCS (double-byte character set) terminals.
    Action
    Check program logic and generate correct SO/SI pairs.

#### NAT1162: Invalid character or shift character in DBCS-only field.

    Text
    Invalid character or shift character in DBCS-only field.
    Explanation
    A DBCS-only field is an alphanumeric field for which the session
    parameter PM=D is set. It must contain only valid DBCS characters;
    shift-out/shift-in characters (SO/SI) are not allowed within such
    a field.
    If either
    - a shift-out/shift-in character (SO/SI) or
    - a character code that is not a valid DBCS character
    is detected, this error is issued.
    Shift-out/shift-in characters (SO/SI) are always detected. Because
    the detection of non-DBCS characters requires ICU, it will not be
    performed if ICU is not available (that is, if the profile parameter
    CFICU=OFF has been set).
    Action
    Correct the content of the DBCS-only field.

#### NAT1165: The WINDOW statements are no longer consistent.

    Text
    The WINDOW statements are no longer consistent.
    Explanation
    Natural tried to execute the internal reference to the DEFINE WINDOW
    statement during the execution of an INPUT WINDOW=window-name or
    SET WINDOW window-name. The reference is not the correct statement
    anymore. Probably the generated program has been destroyed.
    Action
    Clear the buffer pool and restart Natural.
    Recatalog the program.

#### NAT1166: Invalid window width specified in SIZE clause.

    Text
    Invalid window width specified in SIZE clause.
    Explanation
    The value for the number of columns in the SIZE clause of the DEFINE
    WINDOW statement is outside the valid range.
    The minimum number of columns if the FRAME clause is used is 13.
    The minimum number of columns if the FRAME clause is not used is 10.
    The maximum number of columns is the physical screen size.
    Action
    Correct program.

#### NAT1167: Invalid window length specified in SIZE clause.

    Text
    Invalid window length specified in SIZE clause.
    Explanation
    The value for the number of lines in the SIZE clause of the DEFINE
    WINDOW statement is outside the valid range.
    The minimum number of lines if the FRAME clause is used is 4.
    The minimum number of lines if the FRAME clause is not used is 2.
    The maximum number of lines is the physical screen size.
    Action
    Correct program.

#### NAT1168: Invalid window start line (:1:).

    Text
    Invalid window start line (...).
    Explanation
    The current size of the window inhibits the position of the
    window at the specified line in the screen.
    Action
    Reduce the size of the window, or use a smaller line value.

#### NAT1169: Invalid window start column (:1:).

    Text
    Invalid window start column (...).
    Explanation
    The current window size is too large to start the window at the
    specified column on the screen.
    Action
    Reduce the window size, or use a smaller column value.

#### NAT1170: PC access method not available.

    Text
    PC access method not available.
    Explanation
    Natural checks to see if the terminal command "%+" is valid
    in the current environment. The PC access method is not linked
    to the Natural nucleus.
    Action
    Do not use "%+", or contact your Natural administrator.

#### NAT1171: The required terminal converter module is missing.

    Text
    The required terminal converter module is missing.
    Explanation
    This error occurs if the terminal command "%T=nnnn" has been entered,
    but the specified terminal type is not defined by the macro NTDVCE in
    source module NATCONFG, or the required converter module has not been
    linked to the Natural nucleus.
    Action
    Specify a correct terminal type; or link the required converter
    module to the Natural nucleus.

#### NAT1172: PC connection already active.

    Text
    PC connection already active.
    Explanation
    The terminal command "%+" has been entered, but PC connection
    was already active.
    Action
    No action required.

#### NAT1173: PC connection not active.

    Text
    PC connection not active.
    Explanation
    The terminal command "%-" has been entered, but the
    PC connection was not active or had already been
    de-activated.
    Action
    No action required.

#### NAT1174: Not in lower case for upload.

    Text
    Not in lower case for upload.
    Explanation
    For uploads, Natural has to be in lower case to be able to compute
    the right check sum and to upload binary data.
    Action
    Set lower case on and try again.

#### NAT1175: Upload aborted due to check sum errors.

    Text
    Upload aborted due to check sum errors.
    Explanation
    The sent check sum is different from the one computed by Natural.
    Action
    Try upload again later.

#### NAT1176: Terminal type :1: cannot be used in this environment.

    Text
    Terminal type ... cannot be used in this environment.
    Explanation
    The terminal type specified by the TTYPE profile parameter or by
    the terminal command %T= cannot be used in this environment.
    For example, an online terminal type cannot be used in a batch
    environment.
    The terminal type specified by the terminal command %T= or in a
    SET CONTROL "T=" statement does not support MBCS code pages.
    Action
    Specify a correct terminal type for this environment.

#### NAT1177: Unsupported format type found.

    Text
    Unsupported format type found.
    Explanation
    Supported format types for the old PC access method are alphanumeric
    and numeric.
    Supported format types for the new PC access method are:
        - alphanumeric
        - numeric
        - packed
        - logical
        - floating point
        - integer
        - binary.
    Action
    Correct your program and retry.

#### NAT1178: Uploaded data are not a DDM or Natural 2 source/object.

    Text
    Uploaded data are not a DDM or Natural 2 source/object.
    Explanation
    The data used when uploading a DDM or a source binary or an
    object are not of the appropriate type.
    The used file on the PC does not hold a binary downloaded DDM or
    source or object.
    Action
    Use an appropriate file and retry.

#### NAT1179: Used work file number not assigned to PC or PCNEW.

    Text
    Used work file number not assigned to PC or PCNEW.
    Explanation
    The work file number used in the subprogram for the current up-/download
    is either not assigned to PCNEW if up/downloading binary
    or not assigned to PC or PCNEW if up-/downloading as source.
    Use SYSFILE to check which work files are assigned to PC and PCNEW.
    Action
    Use correct work file number and retry.

#### NAT1180: Invalid type entered for "Upload from PC".

    Text
    Invalid type entered for "Upload from PC".
    Explanation
    Valid types for "Upload from PC" are: P, N, S, H, C, K, T, M, 4.
    Action
    Use appropriate type.

#### NAT1181: Source or object for download does not exist.

    Text
    Source or object for download does not exist.
    Explanation
    An attempt was made to download a non-existing source or object.
    Action
    Check the name and the library of the source or object you want to
    download and retry.

#### NAT1182: Source to download is of invalid type.

    Text
    Source to download is of invalid type.
    Explanation
    An attempt was made to download a data area as source.
    Sources of data areas can only be downloaded binary.
    Action
    Download source of data area binary.

#### NAT1183: Specified work file cannot be used for COMMAND download.

    Text
    Specified work file cannot be used for COMMAND download.
    Explanation
    The specified work file cannot be used for a
    WRITE/DOWNLOAD PC/WORK 5 COMMAND statement,
    for one of the following reasons:
    - The work file is not defined for the new PC access method.
    - The work file is already being used.
    Action
    Define the work file correctly, or use a different work file.

#### NAT1184: Downloaded command rejected by PC.

    Text
    Downloaded command rejected by PC.
    Explanation
    The command that was downloaded has been rejected by the PC,
    because the command is not valid.
    See the Natural Connection documentation for
    information on which commands can be downloaded.
    Action
    Correct program and retry download.

#### NAT1185: Catalog the object before you download/upload it.

    Text
    Catalog the object before you download/upload it.
    Explanation
    The object contains an error or inconsistency which prevents
    its being downloaded/uploaded.
    Action
    Catalog the object to be downloaded/uploaded;
    then try again to download/upload it.

#### NAT1186: Buffer overflow due to too many or too long field names.

    Text
    Buffer overflow due to too many or too long field names.
    Explanation
    While downloading/uploading data with field names, a buffer
    overflow has occurred. The reason that the field names do not
    fit into the corresponding buffer, either because too many
    fields are sent or because the field names are too long.
    Action
    Upload/download the data without field names (see PC profile parameter),
    or reduce the number of fields to be uploaded/downloaded.

#### NAT1187: GETMAIN for PC Connection work area failed.

    Text
    GETMAIN for PC Connection work area failed.
    Explanation
    During upload or download processing the transferred data are stored
    intermediately in the PC Connection work area. An increase of this
    buffer failed.
    Action
    Contact your database administrator.

#### NAT1188: Maximum record length (32 KB) for PC file access exceeded.

    Text
    Maximum record length (32 KB) for PC file access exceeded.
    Explanation
    The maximum allowed record length for an access to a PC file is 32 KB.
    Action
    Reduce the number or size of the operands in the appropriate
    READ/WRITE WORK FILE statement.

#### NAT1190: Type "unformatted" is not supported for PC work files.

    Text
    Type "unformatted" is not supported for PC work files.
    Explanation
    Unformatted file transfer between PC and z/OS is currently not
    supported.
    Action
    Use a different type of file transfer.

#### NAT1191: Option ADJUST is not supported for PC work files.

    Text
    Option ADJUST is not supported for PC work files.
    Explanation
    The option ADJUST is currently not supported with the READ WORK FILE
    statement for PC work files.
    Action
    Use a different type of file transfer.