INPUT-SET-SELECTION Action

#### Search Results

Search

# INPUT-SET-SELECTION Action

This document covers the following topics:

- Description

- Parameters

## Description

Selects an area (position to position) in an Edit Area Control or in an Input Field Control .

## Parameters

Name/Data Type | Explanation
--- | ---
HANDLE OF EDITAREA or INPUTFIELD | Input Specifies an Edit Area Control or an Input Field Control.
Position from (I4) | Input Selection starts from this position onwards.
Position to (I4) | Input Last selected position. If you specify "0", the selection will extend to the last character.
Response (I4) | Output Natural error (if applicable).

#### Example:

       #POSITION-FROM := 10  /* Select from the 10th to the 22nd character
       #POSITION-TO := 22
       PROCESS GUI ACTION INPUT-SET-SELECTION WITH #EA-1 #POSITION-FROM #POSITION-TO
       GIVING #RESPONSE

### On this page

- Description
- Parameters