Barcode Control

#### Search Results

Search

# Barcode Control

The CISFO:BARCODE2 control represents a barcode. The text/number of a barcode is derived from a property of the data object that is associated with the page. There are diverse types of barcodes with diverse parameters that are supported.

The barcode internally uses the Krysalis open source framework (http://www.krysalis.org/).

## Properties

Basic
valueprop | Name of adapter property that provides the value that is translated into a corresponding barcode output. Dependent on the barcode type you might only be able to return a limited set of characters as value (e.g. "only number"). The valid character codes are listed in the documentation for the barcodes - please read details there. | Obligatory |
barcodetype | Barcode type that is used for creating the barcode output. There are certain different industry standards that might be used for rendering the barcode. | Optional | INTERLEAVED2OF5 CODE39 USD3 3OF9 CODABAR USD4 NW7 2OF7 CODE128 EAN_UCC128 UPCA UPCE EAN13 EAN8 POSTNET
height | The height of the barcode. The unit is 'mm', 'cm' or 'pt'. The minmal and maximal height depends from the barcode type you use. Look at the description of the barcodes for details. | Optional | 1pt 12pt 0.5in 1in 1mm 5mm 1cm 1.5cm
humandreadable | Definition if the barcode should contain human readbly characters. If set to "bottom" then readable characters are rendered below the barcode lines, if set to "top" then they are rendered above. Define "none" if no characters are to be output as part of the barcode. | Optional | BOTTOM NONE TOP
modulewidth | Width of a narrow element. The minmal and maximal width is dependent from the barcode. Look at the description of the barcodes for exact definition. | Optional |
quitezone | Size of the space left and right of the barcode. The minmal and maximal quite zone is dependent from the barcode. Look at the description of the barcodes for exact definition. | Optional |
Special
checksummode | The checksum mode determines the behaviour for checksums. The posible values are: "add" for adding a checksum, "auto" for the barcode type's default, "check" for creating a checksum and "ignore" for no processing. | Optional | ADD AUTO CHECK IGNORE
igw | Intercharacter gap width. The intercharacter gap width is dependent from the barcode. Look at the description of the barcodes for exact definition. | Optional |
widefactor | A multiply-factor for the wide element. The wide factor is dependent from the barcode. Look at the description of the barcodes for exact definition. | Optional |
POSTNET
baselinealignment | Determines the alignment of the line in POSTNET barcodes. Posible values are 'bottom' and 'top', as consequence short and long lines are aligned correspondingly. | Optional | BOTTOM TOP
shortbarheight | The height of the short bars. | Optional |
tallbarheight | The height of the tall bars. | Optional |