NATPROC-LOGON

#### Search Results

Search

# NATPROC-LOGON

File | 190
Op-Sys | z/OS, z/VSE, BS2000 Note Support for z/VSE is deprecated. Support for BS2000 is also deprecated, except in conjunction with the ESM adapter. Features that are z/VSE and BS2000 specific will be removed from future releases.
Statement | `PROCESS`
Task | Logon to any Entire System Server accessible via Entire Net-Work

## Common Fields for all Operating Systems

Dictionary Field Name | F/L | Mu | DE | Remarks
--- | --- | --- | --- | ---
`CPU` | N5.2 |  |  |
`ERROR-CODE` | N3 |  |  |
`ERROR-TEXT` | A58 |  |  |
`IO-COUNT` | N7 |  |  |
`NODE` | N5 |  | D |
`NODE-NAME` | A16 |  | D |
`SYSTEM-MESSAGE-CODE` | A10 |  |  |
`LOGON-ID` | A8 |  | D | Required.
`PASSWORD` | A32 |  | D | Required in z/OS and z/VSE.
`FUNCTION` | A8 |  | D | Required.

## Additional fields Supported for z/OS, z/VSE

Dictionary Field Name | F/L | Mu | DE | Remarks
--- | --- | --- | --- | ---
`NEW-PASSWORD` | A32 |  | D |
`RACF-GROUP` | A8 |  | D | z/OS only.
`SECURITY-MESSAGE` | A80 |  |  | z/OS only.
`PASSPHRASE` | A100 |  | D | z/OS only.
`NEW-PASSPHRASE` | A100 |  | D | z/OS only.

## Relevant Error Codes

Code | Text | z/OS | z/VSE | BS2000
--- | --- | --- | --- | ---
509 | Logon failed - check `LOGON-ID` / `PASSWORD` | X | X | X
511 | Function must be `LOGON`/`LOGOFF` | X | X | X

## Field Descriptions

Field Name | Type/Length | Operating System
--- | --- | ---
`CPU` | (N5.2) | z/OS, z/VSE, BS2000

Amount of CPU consumed (format SSSSS.HH), returned with `FUNCTION=LOGOFF`.

Field Name | Type/Length | Operating System
--- | --- | ---
`FUNCTION` | (A8) | z/OS, z/VSE, BS2000

Possible options:

Field Name | Type/Length | Operating System
--- | --- | ---
`IO-COUNT` | (N7) | z/OS, z/VSE, BS2000

Number of I/O operations so far, returned with `FUNCTION=LOGOFF`.

Option | Explanation
--- | ---
`LOGOFF` | Logoff from the system.
`LOGON` | Logon to the system.

Field Name | Type/Length | Operating System
--- | --- | ---
`LOGON-ID` | (A8) | z/OS, z/VSE, BS2000

System user ID.

Field Name | Type/Length | Operating System
--- | --- | ---
`NEW-PASSPHRASE` | (A100) | z/OS

New password phrase for user ID.

Field Name | Type/Length | Operating System
--- | --- | ---
`NEW-PASSWORD` | (A32) | z/OS, z/VSE

New password for system user ID.

Field Name | Type/Length | Operating System
--- | --- | ---
`PASSPHRASE` | (A100) | z/OS

Password phrase for user ID.

Field Name | Type/Length | Operating System
--- | --- | ---
`PASSWORD` | (A32) | z/OS, z/VSE, BS2000

Password for system user ID.

Field Name | Type/Length | Operating System
--- | --- | ---
`RACF-GROUP` | (A8) | z/OS

Group to which the user ID is defined in RACF or security interface.

Field Name | Type/Length | Operating System
--- | --- | ---
`SECURITY-MESSAGE` | (A80) | z/OS

Message returned by security interface.

### On this page

- Common Fields for all Operating Systems
- Additional fields Supported for z/OS, z/VSE
- Relevant Error Codes
- Field Descriptions