System Messages

#### Search Results

Search

# System Messages

This document lists the system messages, together with their explanation and the action required.

This document covers the following topics:

- System Messages ESY3000 - ESY55xx

- System Messages ESY5600 - ESY5699

- System Messages ESY5700 - ESY5799

- System Messages ESY5800 - ESY5899

- System Messages ESY5900 - ESY5999

## System Messages ESY3000 - ESY55xx

Message | Explanation | Action
--- | --- | ---
ESY3000 <variable text> | The request has been completed successfully | Check for view-dependant information in variable text.
ESY5500 - VSAM error during job submission. | An error occurred during job submission. | Resubmit job. If error persists, contact the systems programmer.
ESY5502 - SYSQL Error. | Internal ESY Error. | Please contact our support.
ESY5503 - RECALL Error. | Dataset could not be recalled using ARCHRCAL macro. Check if the dataset has actually been migrated. If it has, contact the systems programmer regarding the installed migration tool. | Check dataset status and/or migration tool with systems programmer.
ESY5506 - Dataset is migrated. | Dataset is archived on external storage media. | Please use startup parameter RECALL in ESY.
ESY5507 - Too many parallel ESY requests. | You may only use 5 nested loops in ESY. | Please check programs and correct error.
ESY5508 - Adabas response code :1: returned from ESY. | Adabas Rsp :1: return from ESY. | Please contact your database administrator. In Case of Rsp 111 see Troubleshooting.
ESY5509 - Logon failed - check LOGON-ID / PASSWORD. | The attempted logon failed. Note: A more detailed message is returned by the installed security system when the ERROR-TEXT field is specified. | Try to logon again, using a valid LOGON-ID and PASSWORD.
ESY5510 - Logon required. |  | Logon to Entire System Server (view NATPROC-LOGON).
ESY5511 - Function must be LOGON/LOGOFF. | An invalid function was given in view NATPROC-LOGON. | Check source program. Valid functions are LOGON and LOGOFF.
ESY5520 - No core available. | The amount of core required for each user is: MAXFBL + MAXSBL + MAXCBL + (NUMREQ * BUFLEN) | Increase the auxiliary buffer size (ASIZE parameter).
ESY5521 - NATPNI/NATPNIP unresolved. | This Natural nucleus is unable to perform Entire System Server functions. | Contact the Natural Administrator.
ESY5530 - Access denied by Security facility. | A security violation has occurred. This return code has been issued by the security system with which Entire System Server interfaces. | No action is required.
ESY5531 - Password missing or incorrect. | The dataset is password protected, i.e. a password must be supplied. | Enter a valid password.
ESY5533 - Requested number of records scanned. | Requested number of records in READ-FILE or READ-SPOOL scanned and no match for search criteria found. | No action required.
ESY5534 - File is not a load library. | File is not a load library. |
ESY5535 - File has invalid format. | File has not supported DSORG. | Check with the systems programmer.
ESY5536 - CVA error :1: accessing VTOC. | Macro CVAFDIR caused error. | Check inline error code with the systems programmer.
ESY5537 - Time limit reached. | Time limit reached and no record was found for this search criterion. |
ESY5538 - Invalid record-length specified. |  |
ESY5539 - DFHSMREQ failed with RC=:1:. | A request failed to delete a migrated dataset. | Contact your storage administrator.
ESY5541 - Member generation not found in directory. | An attempt was made to access a member generation which does not exist. | Specify a valid combination of member name and generation number.
ESY5542 - GENERATION not valid for this library. | A generation number has been specified but the library does not support member generations. | Specify a generation number only for a PDSE library that supports member generations.
ESY5543 - GENERATION not valid for FUNCTION =:1:. | A GENERATION cannot be specified for the requested FUNCTION. | Specify a GENERATION only for FUNCTION=SCRATCH.
ESY5544 - Invalid File-ID. | The requested file-id does not exist. | Specify valid file-id.
ESY5548 - CLOSE required for :1: | A sequence of WRITE-FILE requests ended without a terminating request with FUNCTION='CLOSE' specified. | Specify FUNCTION='CLOSE' for the last WRITE-FILE request.
ESY5549 - Not a PDSE dataset. | The data set is not in PDSE format. | No action is required.
ESY5550 - Not a PDS or LIBRARIAN file or VSAM dataset. | An attempt was made to access the directory of a non-PDS file. | No action is required.
ESY5551 - Member not specified. | An attempt was made to access a PDS member without specifying its name. | Specify member name.
ESY5552 - NEWNAME / ALIAS operand missing. | No value for NEWNAME or ALIAS was given. Formats are: NEWNAME (A8) - view PDS-UPDATE ALIAS (A8) - view CATALOG-UPDATE NEWNAME (A44) - view VTOC-UPDATE | Supply a value for NEWNAME or ALIAS.
ESY5553 - I/O error on directory. | An error occurred while reading a PDS directory. | The directory of the specified dataset is probably invalid. Check with the systems programmer.
ESY5554 - MEMBER not found in directory. | An attempt was made to access a member which does not exist. | Specify valid member name.
ESY5555 - NEWNAME / ALIAS already exists in directory. | Values for NEWNAME and ALIAS must be unique within a directory. The value specified already exists. | Enter a unique value for NEWNAME or ALIAS.
ESY5556 - File is in use. | The file is under exclusive control of another user. | Retry at a later time.
ESY5557 - File is held by linkage editor. | The file is under exclusive control of the linkage editor. | Retry at a later time.
ESY5558 - No space in Directory. | No space is available in the Directory. | Enlarge the Directory.
ESY5559 - STOW error. | An error occurred during a STOW attempt. | No action is required.
ESY5560 - Segment length greater than 253. | The maximum segment length is 253. | Specify a valid SEGMENT-LENGTH.
ESY5561 - Required catalog does not exist. | The specified catalog does not exist. | Specify a valid CVOL.
ESY5562 - Catalog entry not found. | The entry was not found in the catalog. | No action is required.
ESY5563 - dataset is an index. | The dataset to be cataloged is an index. | Specify a valid dataset name.
ESY5564 - dataset not at lowest index level. | The dataset name entered must be at the lowest index level. | Enter a valid dataset name.
ESY5565 - Syntax error in dataset name. | A syntax error was detected in the dataset name. | Specify a valid dataset name.
ESY5566 - Syntax error in catalog name. | A syntax error was detected in the catalog name. | Specify a valid catalog name.
ESY5567 - Invalid OPTION, specify LONG or USERCAT. | An invalid OPTION was specified, valid options are LONG or USERCAT. | Specify a valid OPTION (LONG or USERCAT).
ESY5571 - DSNAME operand missing. | A fully qualified dataset name must be specified. | Enter a valid DSNAME.
ESY5572 - NEWNAME missing. | A fully qualified DSNAME must be specified as NEWNAME for the RENAME function. | Specify a valid DSNAME in the NEWNAME field for the RENAME function.
ESY5573 - SCRATCH invalid. |  |
ESY5574 - RENAME invalid. | The NEW dataset name contains invalid characters. | Check NEW dataset name for invalid characters.
ESY5575 - Dataset not renamed, CATALOG-UPDATE function failed. | The new dataset name cannot be cataloged. Therefore, the old dataset name is still valid, and the dataset can only be accessed by specifying the correct volume. | Check with your systems programmer why the new dataset name cannot be cataloged.
ESY5576 - SCRATCH returned with RC :1: and status :2:. | SCRATCH could not be performed. See the z/OS DFSMSdfp Advanced Services Manual for a detailed explanation of the return code and status code. | Check status of dataset.
ESY5577 - RENAME returned with RC :1: and status :2:. | RENAME could not be performed. See the z/OS DFSMSdfp Advanced Services Manual for a detailed explanation of the return code and status code. | Check status of dataset.
ESY5578 - RENAME fatal error; VOL :1: DSN :2:. | RENAME could not be performed. Check the dataset (see DSN value) on volume (see VOL value). | Check with your systems programmer.
ESY5580 - Binder API :1: call, rc :2:, rsn :3:. | A call to the Binder API failed. | Note any IEW-prefix messages in the console log and Contact Customer support if necessary.
ESY5590 - End of data reached during inplace-update. | It is not possible to add records with the UPDATE-INPLACE function. | Do not use UPDATE-INPLACE for adding records.
ESY5591 - Member not found for inplace-update. |  | Specify a valid MEMBER.
ESY5592 - Record length error for variable inplace-update. |  | Check the source program. RECORD-LENGTH may not be changed.

## System Messages ESY5600 - ESY5699

Message | Explanation | Action
--- | --- | ---
ESY5600 - Unknown function. | An invalid value was specified in the FUNCTION field. | Specify valid FUNCTION value.
ESY5602 - Device is invalid. | An invalid DEVICE value was specified. | Specify valid DEVICE value.
ESY5603 - INDEX / ALIAS missing. |  | Specify INDEX / ALIAS.
ESY5604 - No volumes specified. | No VOLUMES were specified for CATLG / RECATLG. | Specify VOLUMES.
ESY5605 - IGWASMS returned with RC :1: and reason :2:. | A request failed to retrieve attributes for a dataset. | Contact your systems programmer.
ESY5606 - Managed datasets cannot be uncataloged. | A request was issued to uncatalog an SMS-managed dataset. | Do not ask to uncatalog an SMS-managed dataset.
ESY5608 - ISITMGD failed with RC :1: and reason :2:. | A request failed to retrieve attributes for a data set. | Check with systems programmer. Contact Customer support.
ESY5610 - QNAME is missing. | No value was specified in the QNAME field. | Specify valid QNAME value.
ESY5611 - QNAME cannot start with SYS. | Major names beginning with SYS are not allowed. | Specify valid QNAME value.
ESY5612 - RNAME is missing. | No value was specified in the RNAME field. | Specify RNAME value.
ESY5613 - RNAME length is missing or invalid. | No value was specified in the RNAME-LENGTH field. | Specify valid RNAME-LENGTH value.
ESY5614 - Resource is in use. | Resource is already allocated as shareable by another task, and exclusive access was requested. | Retry at a later time.
ESY5615 - Resource held by another task. | Resource is already allocated exclusively by another task. | Retry at a later time.
ESY5616 - Error in GQSCAN routine. | An internal error occurred as a result of the GQSCAN macro request. | Notify systems programmer. (technical support should be notified as well).
ESY5621 - Identifier missing/duplicate/not found. | The identifier associated with the area was missing/duplicate/not found. | Specify correct identifier.
ESY5622 - NUMBER-OF-ENTRIES missing or invalid. | The specification of the maximum number of entries was missing/invalid. | Specify a valid NUMBER-OF-ENTRIES value.
ESY5623 - ENTRY-LENGTH missing or invalid. | The specification of the entry length was missing/invalid. | Specify a valid ENTRY-LENGTH value.
ESY5624 - ENTRY-NUMBER missing or invalid. | The specification of the entry number was missing/invalid. | Specify correct entry number.
ESY5625 - Cannot allocate area. | Insufficient storage was available to allocate the area. | Decrease amount of requested storage or notify systems programmer.
ESY5626 - DATA missing. | No data was specified. | Specify the DATA field.
ESY5627 - Field position + length > 250. | The field extends the maximum area length (250). | Specify valid field position/length.
ESY5628 - Error in editor. | An internal editor error occurred. | Notify systems programmer.
ESY5629 - Area is protected. | Area is protected. | No action required.
ESY5630 - Console not defined or not active. | The specified console ID was not found. | Specify valid console ID.
ESY5631 - Console table not found. | Console table could not be found. | Contact your systems programmer.
ESY5632 - General or Control object not found. | General or Control object returned by Multi Console Support (MCS) could not be found. | Contact your systems programmer.
ESY5633 - Cannot lock Console table. | Console table could not be locked for exclusive use. | Retry operation. If problem persists, please contact your systems programmer.
ESY5634 - Invalid record number. | Requested record number is invalid. | Retry operation. If problem persists, please contact your systems programmer.
ESY5635 - Attempt to alter key in KSDS file. | Modifying keys in KSDS files is not allowed. | Check program and correct error.
ESY5636 - Too many active requests on this ACB. | There may be a nested loop while accessing VSAM files or there are too many parallel requests open. | Check your program and check also with your ESY-DBA.
ESY5637 - VSAM subtask is not active. | The ESY subtask for VSAM access may be abended. Check with your ESY-DBA to restart ESY. | Contact your ESY-DBA or Contact Customer support.
ESY5638 - Key not found. | Key to access the requested record in your file not found. | Check program and correct error.
ESY5639 - Cannot delete record in ESDS file. | Deleting records from ESDS files is not allowed. | Check program and correct error.
ESY5640 - Error generating VSAM control blocks. | An error occurred generating VSAM control blocks. | Notify systems programmer.
ESY5641 - Error :1: while opening SMF or VSAM file. | A VSAM error occurred while opening an SMF file. | Notify systems programmer.
ESY5642 - Error :1: while reading SMF or VSAM file. | A VSAM error occurred while reading an SMF file. | Notify systems programmer.
ESY5643 - SMF not active / not recording. | At the time of the request SMF is not active / not recording. | Notify systems programmer.
ESY5644 - XXXXXXXX ERROR IN POWER xxx=yyzz. | An error occurred during communications between ENTIRE SYSTEM SERVER and POWER and/or XPCC. | XXXXXXXX is the requested function; xxx indicates either failure of POWER or XPCC, whilst yyzz is the return and reason codes. Contact Customer support.
ESY5645 - Invalid RBA was specified. | The requested RBA was not found. | Specify valid RBA value.
ESY5646 - Write to VSAM only allowed on base cluster. | An attempt was made to write to a none-base cluster. | Check program and correct error.
ESY5647 - VSAM cluster is not defined as reusable. | Access to VSAM cluster only allowed if reusable. | Define your VSAM cluster reusable.
ESY5648 - Record not in ascending key sequence. | An attempt was made to write a record with a wrong key. | Check program and correct error.
ESY5649 - ESY User not found or cannot be cancelled. | The ESY user could not be found for various functions. | Correct input data.
ESY5650 - Invalid sequential file. | The requested sequential file does not exist. | Please check file name and rerun program.
ESY5651 - Requested catalog does not exist. | The requested CVOL does not exist. | Specify valid CVOL.
ESY5652 - Catalog structure inconsistent. | The catalog structure is inconsistent. | Notify the systems programmer.
ESY5653 - Cannot delete index. | The index cannot be deleted. | No action is required.
ESY5654 - Index structure does not exist. |  | No action is required.
ESY5655 - Insufficient space on catalog dataset. | The catalog dataset is full. | Notify the systems programmer.
ESY5656 - Error cataloging generation dataset. | An error occurred while cataloging a generation dataset. | Check specified values. If valid, contact the systems programmer.
ESY5657 - I/O error on catalog. | An I/O error occurred while accessing the catalog. | This is probably a hardware error. Contact the systems programmer.
ESY5658 - dataset is not cataloged. | The specified dataset is not cataloged. | No action is required.
ESY5659 - dataset is already cataloged. | The specified dataset is already cataloged. | No action is required.
ESY5660 - :1: - :2: module not available. | The specified Natural module was not found. | Specify name of an existing Natural module.
ESY5661 - :1: - Natural sub-task already active. | A Natural subtask is already active for this user. | Make sure that subtask is closed prior restarting it.
ESY5662 - :1: - Natural sub-task not allowed. | The Natural subtask system has not been initialized. | Notify systems programmer.
ESY5663 - :1: - Natural sub-task not active. | The Natural subtask does not exist. | No action is required.
ESY5664 - :1: - Natural sub-task table full. | The maximum number of Natural subtasks is reached. | Notify systems programmer.
ESY5665 - :1: - invalid action requested. | An invalid action was requested. | Specify valid action.
ESY5666 - :1: - Natural sub-task must have parameters. | An attempt was made to start a Natural subtask without parameters. | Specify parameter for Natural subtask.
ESY5670 - View not supported. | This view is not supported on the local operating system. |
ESY5671 - Class missing or is invalid. | The function CHANGE requires a valid NEW-CLASS, NEW-DESTINATION or NEW-USERID value. |
ESY5672 - Segment option requires JOBNAME/JOBNUMBER. | Specifying the SEGMENT option (SEGMENT-NUMBER > 0) requires that the job is identified with JOB-NAME and JOB-NUMBER. |
ESY5673 - Access error due to FILETABLE=STATIC. | The requested file could not be accessed because the Entire System Server startup parameter FILETABLE was specified as STATIC. Only those files available at ESY initialization time (STD,PARSTD & TEMP labels) can therefore be accessed. | To allow dynamic access of files NOT specified at ESY initialization time, change the FILETABLE parameter to DYNAMIC and restart Entire System Server.
ESY5674 - VTOC error reading format-3 labels. | VTOC error reading format-3 labels for the requested file. | Information message only. No action necessary or possible.
ESY5675 - :1: not supported. | Entire System Server has detected that the requested file has attributes which are not supported by this version of ESY e.g. Multi-volume files, Multi-extent output files etc. |
ESY5676 - Not first volume of a multi-volume file. | Entire System Server has detected that the file on the specified volume is NOT the first volume/extent of a multi-volume file. |
ESY5678 - Member already exists. | In WRITE-FILE or COPY-FILE, REPLACE = 'NO' was specified, however the member exists. | No action is required
ESY5679 - Input and output files are incompatible. | COPY-FILE has determined that the record formats of the input and output files are not compatible (RECFM does not match, block size incompatibilities, etc.). | Verify dataset attributes and reissue request with correct parameters.
ESY5680 - Job/output is protected. | The user is not authorized to access the specified job/output. | Notify systems programmer.
ESY5681 - Job/output is active. | The specified job/output is currently active. | There is no action required.
ESY5682 - Job/output is not dispatchable. | The job/output is not dispatchable. | There is no action required.
ESY5683 - FAMS error. | A FAMS error occurred while COPY-FILE was copying one or more program objects. | Note any IGW-prefix messages in the console log and Contact Customer support if necessary.
ESY5684 - Remote program object copy currently unsupported. | In this release of Entire System Server, use of COPY-FILE for copying program objects between different nodes is not supported. | A workaround is to first copy the program object to a PDS on the local mode, then copy to a PDS on the remote node, then copy to the target PDSE on the remote node.
ESY5685 - FAMS subtask abended. | One of the subtasks used by remote program object copy has abnormally terminated. The ERROR-NODE and ERROR-VIEW fields will show which node had the ABEND. Information regarding the ABEND will be in the JES log. | Note any IGW-prefix and IEA995I messages in the JES log and Contact Customer support.
ESY5687 - Bad variable record. | Bad variable record. | No action is required.
ESY5688 - Return code :1: HCF function :2:. | The HCF function failed. The return code is the HCF return code. | Notify systems programmer.
ESY5690 - 1: error :2: during :3:. | An error occurred accessing CA-Panvalet or CA-Librarian data. | Notify systems programmer.
ESY5691 - Error while accessing librarian member. | An error occurred accessing a CA-Librarian member. | There is no action required.
ESY5692 - You are not permitted to access member. | This user is not authorized to access the specified member. | Check with systems programmer.
ESY5693 - :1:. | A CA-Panvalet error occurred. | See message text.
ESY5694 - Strange error opening VTOC. | A strange internal error occurred reading the VTOC. | Notify systems programmer.
ESY5695 - VTOC is in use. | The VTOC is currently in use. | Retry.
ESY5696 - Cannot assign logical unit. | A logical unit could not be assigned. | Notify systems programmer.
ESY5697 - Library/sublibrary not found. | The specified library/sublibrary was not found. | Specify valid library/sublibrary name.
ESY5698 - Internal LIBRARIAN error has occurred. | An internal LIBRARIAN error occurred. | Notify systems programmer.
ESY5699 - Not enough main storage available. | Not enough main storage was available to process the request. | Notify systems programmer.

## System Messages ESY5700 - ESY5799

Message | Explanation | Action
--- | --- | ---
ESY5700 - Invalid value specified (DSORG / RECFM / TYPE). | An invalid value was specified for view FILE-ALLOCATE. Note: A more detailed message is returned when field ERROR-TEXT is specified. | Specify valid value for DSORG / RECFM / TYPE.
ESY5701 - DSNAME missing. | The DSNAME was missing. | Specify a valid DSNAME.
ESY5702 - OUTADD error-code :1: reason-code :2: key :3:. |  |
ESY5703 - Copying of empty files not permitted. |  |
ESY5710 - Allocation failed with code :1:. | The allocation failed. The code is the DYNALLOC return code. Note: A more detailed message is returned when field ERROR-TEXT is specified. | Check the DYNALLOC return code.
ESY5711 - Logical Error occurred in Common JES Interface. | A logical error has occurred in the Common JES Interface. Additional messages describing the type of error may have been issued to the console. | Check the system log for additional messages. Contact Software AG customer support.
ESY5712 - Request to Common JES Interface failed. | A request failed to access spool data. | Contact Customer support.
ESY5713 - Jobname and Job ID missing. One of them required. | Neither JOB-NAME nor JOB-ID / JOB-NUMBER have been specified. At least one of them is required to process the request. | Specify JOB-NAME, JOB-ID or JOB-NUMBER with the request.
ESY5714 - Unable to read :1: type SYSOUT datasets. | The specified spool file TYPE is invalid or cannot be processed. | Specify a valid spool file type (AL, CC, JL, SI, SM or SO).
ESY5715 - Duplicate jobnames found. Please specify job id. | Multiple jobs were found for the specified job name. | Additionally specify job id / job number.
ESY5717 - GENCB for ACB or RPL failed with RC :1: and RSN :2:. | An ACB or RPL could not be generated to access a SYSOUT dataset. | Check with systems programmer. Contact Customer support.
ESY5719 - Unable to :1: SYSOUT dataset. | An error occurred during open or close of a SYSOUT dataset. | Check with systems programmer. Contact Customer support.
ESY5720 - Invalid TYPE. | An invalid TYPE was given in the READ-SPOOL view. | Check source program. Valid values for TYPE are: in MVS: JL, SI, SO, SM and CC. in VSE: LS, PU, RD, XM, CC.
ESY5721 - Job found, but not for specified spool ID. | The job was found on a different spool than the one specified. | No action is required.
ESY5722 - Requested dataset not found. | The requested dataset could not be found. | No action is required.
ESY5723 - Job not in output service. | The requested job is not in output service. | No action is required.
ESY5724 - Requested Job not found. | The requested job could not be found on the JES spool. | No action is required.
ESY5725 - I/O error on JES3 spool. | A READ request to the JES spool failed. | Retry. If the error persists, this is probably a hardware error.
ESY5726 - Logical error on JES3 spool. | A logical error occurred while reading the JES3 spool dataset. | Notify systems programmer. technical support should be notified as well.
ESY5727 - Spanned record is too large. | A spanned record is too large. | No action is required.
ESY5728 - You are not allowed to see this job. | The user attempted to access a job for which he or she has not been authorized. This error is issued by the security system with which Entire System Server interfaces. | No action is required.
ESY5729 - Invalid job TYPE, specify JOB, STC or TSU. | The specified job TYPE is invalid. | Specify a valid job type (JOB, STC, or TSU).
ESY5730 - Unknown error during spool open. | An unknown error occurred during spool open. | Notify systems programmer and technical support.
ESY5731 - Error occurred during spool GET. | An error occurred during spool GET. | Notify systems programmer and technical support.
ESY5732 - Account number missing. | Account number was not supplied. | Check program and correct error.
ESY5733 - No JOIN entry found for user. | The user is not defined in the system. | No action is required.
ESY5734 - ARCHIVE run with errors. | An error occurred during ARCHIVE execution. | Check with systems programmer.
ESY5735 - Logical error using I-T-C. | The inter-task-communication was not used correctly. | No action is required.
ESY5736 - MESSAGE-ID missing. | No MESSAGE-ID value supplied. | Specify a MESSAGE-ID.
ESY5737 - No more index space for inserting record. | The number of records exceeds the available index range. | No action required.
ESY5738 - Error when using memory-pools. | Incorrect use of the MAIN-STORAGE view. | No action is required.
ESY5739 - Error when using Job Variables. | Incorrect use of JOB-VARIABLES view. More details are available in SYSTEM-MESSAGE-CODE. | Please analyze the SYSTEM-MESSAGE-CODE.
ESY5740 - Error when using BTAM file. | An error occurred while allocating a file. | No action is required.
ESY5741 - Error when using SAM file. | An error occurred while allocating a file. | No action is required.
ESY5742 - Error when using PAM file. | An error occurred while allocating a file. | No action is required.
ESY5743 - Error when using ISAM file. | An error occurred while allocating a file. | No action is required.
ESY5744 - Invalid eventing name given. | An invalid eventing name was specified. | No action is required.
ESY5745 - Error occurred when executing Eventing. | Logical error using P1-Eventing. | Contact your systems programmer.
ESY5746 - Serialization running in error. | A serialization request has failed. Detailed information available in SYSTEM-MESSAGE-CODE. | Repeat the request later.
ESY5747 - LENGTH or SUBSTRING-LENGTH invalid. | Invalid value specification for view JOB-VARIABLES. Possible reasons: position greater than length of JV; substring length greater than JV length minus position; position greater than JV length | Correct values and try again.
ESY5748 - Internal LMS error has occurred. | An internal LMS error has been returned from LMS subprogram interface. Check SYSTEM-MESSAGE-CODE for details. | Please check SYSTEM-MESSAGE-CODE
ESY5749 - PVS (CATID) not available. | The requested CATID is not available for the User ID of caller. | No action possible.
ESY5750 - Invalid operand within operand list. | Incorrect usage of an Entire System Server view. | No action is required.
ESY5751 - Not enough memory to execute the function. | There is not enough memory to execute the function. | Check with systems programmer.
ESY5752 - Message/Message length missing. | Possible reasons: no message length specified; message length lower than 4; message length greater than 1250 during use of field MESSAGE-ARRAY; message length greater than 250 during use of field MESSAGE-TEXT; no message specified | Correct input values and try again.
ESY5753 - I-T-C name missing. | ITC name must be specified for functions OPEN, RECEIVE and SEND. | Specify ITC name.
ESY5754 - not done. |  |
ESY5755 - Invalid or no SWITCH type specified. | Neither USER nor PROCESS specified as switch type. | Correct switch type.
ESY5756 - Job Variable name missing or invalid. | Invalid syntax used or no value specified. | Please correct.
ESY5757 - Error during user management. |  |
ESY5758 - User ID is missing. | No user name specified. | Please specify name.
ESY5759 - Name is missing. |  |
ESY5760 - Processor name is missing. |  |
ESY5761 - Start operand is missing. |  |
ESY5762 - Line/Station is missing. |  |
ESY5763 - Info type operand is missing. |  |
ESY5764 - Virtual call is missing. |  |
ESY5765 - Required Catalog ID not accessible. |  |
ESY5766 - User ID or Terminal ID missing. | Neither User ID nor processor-/terminal-name specified. | Please specify requested values.
ESY5767 - No TSN found. |  |
ESY5768 - Invalid command in macro list. |  |
ESY5769 - Short name is missing. |  |
ESY5770 - Serialization name missing. |  |
ESY5771 - No information found. | No information found for specified request. | No action required.
ESY5773 - New version operand missing. |  |
ESY5774 - No core available. | Not enough space available to allocate an ESY User Block. | Please contact Software GmbH.
ESY5775 - Invalid Priority Value specified. |  |
ESY5776 - Request was cancelled. | Request was cancelled internally because user has been timed out. |
ESY5777 - Request has abended. | An internal error occurred. Condensed abend information is contained in the job-log. | Check with systems programmer. Contact Customer support.
ESY5778 - Cannot perform command - not APF authorized. | The Entire System Server nucleus is not running APF authorized. | Check with systems programmer.
ESY5779 - IDCAMS utility has abended. | The IDCAMS utility has abended. | Check job-log for additional information.
ESY5780 - Completion code not ok. | The execution of the request was not successful. | Check input data of request.
ESY5781 - Unable to obtain storage for work area extension. | A request failed to obtain storage for the work area extension. | Increase the region size to more than 16 MB for Entire System Server.
ESY5782 - Error from :1: for :2:, RC :3:, REASON :4:. | A request failed while attempting to read the VTOC. | Contact your systems programmer.
ESY5783 - Unable to allocate :1:, RC :2:, REASON :3:. | The specified volume could not be allocated. | Contact your systems programmer.
ESY5784 - Unable to open VTOC on :1:, RC :2:. | An OPEN request failed for the VTOC on the specified volume. | Try again. If the problem persists, contact your systems programmer.
ESY5785 - CVAF :1: failed with RC :2: and CVSTAT :3:. | A request failed to the common VTOC Access Facility. | Contact your systems programmer.
ESY5786 - Unable to obtain storage for CSI work area. | A request failed to obtain storage for the CSI work area. | Increase the region size to more than 16 MB for Entire System Server.
ESY5787 - CSI request failed, Module :1:, Reason :2:. RC :3:. | A request to the Catalog Search Interface failed. | Contact your systems programmer.
ESY5788 - Unable to substitute symbol :1:, RC :2:. | A request failed to substitute text for a system symbol. | Contact your systems programmer.
ESY5789 - Unable to get UCB copy for :1:, RC :2:. | A request failed to get a UCB copy for the volume specified. | Contact your systems programmer.
ESY5798 - Task was not started under TSOS. | Entire System Server (npr) is not running under TSOS and does not have the required privileges to process the user requests. | Check the job control and make sure that all tasks of the Entire System Server (npr) run under TSOS. Perform a restart after changing the job control.
ESY5799 - Entire System Server internal error. | An internal error has occurred. | Please contact our support.

## System Messages ESY5800 - ESY5899

Message | Explanation | Action
--- | --- | ---
ESY5800 - Specified level is a dataset name. | The specified level name is a dataset name. | No action is required.
ESY5801 - Job not found. | The requested job was not found. | No action is required.
ESY5802 - GETMAIN for CSA area failed. | An attempt was made to access main storage, and GETMAIN for the CSA area failed. | Notify your systems programmer.
ESY5803 - Cannot access data. | An attempt was made to access main storage, and the data specified cannot be accessed. | No action is required.
ESY5804 - Request to access data has timed out. | Main storage was accessed, and SRB was scheduled to run in an address space. SRB must be completed within 10 seconds. | No action is required.
ESY5805 - Invalid TCB address. | An invalid TCB-ADDRESS was specified. | Specify valid TCB-ADDRESS.
ESY5806 - Permanent I/O error on catalog. | A permanent I/O error occurred while accessing the catalog. | This may be a hardware error. Contact data center personell.
ESY5807 - Invalid track address. | An invalid track address was specified. | Specify valid track address.
ESY5809 - Subsystem not active. | The related subsystem has not been started properly. Therefore, the requested function is not available in this run of ESY. The following views return this error code on BS2000: views SPOOL-QUEUE, SPOOL-FILES, WRITE-SPOOL if SPOOL=NONE is defined; views SEND-MESSAGE, CONSOLE if CONSOLE task is not running; views CONSOLE, EVENTING if EVENTING task is not running. | Contact your administrator to get the subsystem started for the next ESY run.
ESY5810 - Error detected in catalog, processing terminated. | An error in the catalog structure was detected. | Notify your systems programmer.
ESY5811 - Specified level is an empty index. | The level specified is an empty index. | No action is required.
ESY5820 - Unknown command. | A command which is not known to Entire System Server was entered. | Check spelling, syntax of command. Check to see whether command is a Natural command.
ESY5821 - Job no longer active. | An attempt was made to access a job which is no longer active. | No action required.
ESY5822 - Logical error on JES3 spool. | A logical error occurred while reading the JES3 spool dataset. | Try again. If the error persists, it may indicate a bad control block on the JES3 spool (which may be caused by a hardware error).
ESY5823 - Requested job in input queue. | An attempt was made to access output data of a job which is in the input queue. | Wait until job is processed.
ESY5824 - I/O error on JES3 spool. | A READ operation to JES3 spool failed to complete normally. | Probably a hardware failure. A JES3 warm start (with analysis) should be considered.
ESY5825 - JES3 command dataset is full. | A WRITE operation to the JES3 command dataset failed, because the dataset is full. | Wait until space becomes available.
ESY5826 - I/O error on JES3 command dataset. | A WRITE attempt to the JES3 command dataset failed. | This is probably a hardware error. If the error persists, it may be advisable to relocate the JES3 command dataset.
ESY5830 - JES interface is not active. | The JES interface is not active. | Check the JES parameter in the Entire System Server parameter file.
ESY5831 - Error during queue initialization. | An error occurred while reading JES control blocks. | This is probably a hardware error. Contact data center personnel.
ESY5832 - Error during queue open. | An error occurred during the opening of the JES spool dataset. | Check with your systems programmer.
ESY5833 - You are not allowed to alter this job. | An attempt was made to modify a job. The user is not authorized to modify the specified job. This error message is issued by the security system with which Entire System Server interfaces. | No action is required.
ESY5834 - Command failed, MGCRE RC = :1:. | A request failed to issue an internal JES or system command. | Check with systems programmer. Contact Customer support.
ESY5840 - VTAM operator ACB is not open. | The VTAM operator ACB was not opened successfully during initialization. | Either active VTAM support has not been requested by the system parameters, or an open error occurred during initialization. The job-log contains further information.
ESY5841 - Error in SENDCMD - RTNCD=:1: FDBK2=:2:. | A VTAM error occurred while sending a command. Note: A more detailed message is returned when field ERROR-TEXT is specified. | Check the command requested. The RTNCD and FDBK2 values are defined in the appropriate VTAM documentation.
ESY5842 - Invalid VTAM command. | An invalid VTAM command was requested. | No action is required.
ESY5845 - Printer is active for user :1:. | Another user is working with the printer. | Wait until printer is not busy anymore.
ESY5849 - Print failed. Fct=:1: FD=:2: S=:3:. | The print request failed. For further details, check the variable data of FUNCTION, FEEDBACK and STATUS. You may find the explanation of these fields in the VTAM documentation. | Please contact your systems programmer.
ESY5850 - Error :1: occurred while processing VTOC. | The specified error code occurred while processing the VTOC. | Contact Customer support.
ESY5851 - File not on volume. | The requested file does not exist on the specified volume. | No action is required.
ESY5852 - No password supplied / VSAM data space. | No password was specified before attempting to access a password-protected VSAM file. | Specify a password.
ESY5853 - Retention cycle unexpired / NEWNAME exists. | A VTOC-UPDATE RENAME function was attempted; however, the retention cycle is unexpired, and the NEWNAME still exists. | Specify a different NEWNAME, or wait until the retention cycle has expired.
ESY5854 - Permanent I/O error. | A permanent I/O error was detected. | This is probably a hardware error. Contact data center personnel.
ESY5855 - Volume not mounted. | The requested volume was not mounted. | Make sure that the volume is mounted before re-issuing the request.
ESY5856 - Operator unable to mount volume. | The operator is not able to mount the volume. | No action is required.
ESY5857 - File in use. | The file is in use. | Retry later.
ESY5858 - Not authorized. | A security violation was detected. | No action is required.
ESY5859 - File definition not deleted by RACF. | The file definition has not been deleted by RACF. | Execute RACF file deletion.
ESY5860 - Member under MSHP control or changed with MSHP bypass. | Member to be overwritten is under MSHP control or was changed with MSHP bypass. | Use MSHP=YES to indicate MSHP bypass required.
ESY5861 - Member contains SYSIPT data. | Member to be overwritten contains SYSIPT data. | Use INLINE-DATA=YES to confirm SYSIPT data required or INLINE-DATA=OFF to switch off the SYSIPT indicator.
ESY5870 - RECORD field not in search buffer. | RECORD must be specified for WRITE-FILE. | Specify RECORD value.
ESY5871 - MEMBER/MEMBER-TYPE not specified. | The member name and/or type was not specified. | Specify a member name and/or type.
ESY5872 - Record format not supported. | The record format of the desired dataset is not supported. | No action is required.
ESY5873 - RECORD-LENGTH missing. | The RECORD-LENGTH value is missing. | Specify RECORD-LENGTH value.
ESY5874 - RECORD-LENGTH > LRECL. | The specified RECORD-LENGTH value is greater than the LRECL of the dataset. | Specify valid RECORD-LENGTH value.
ESY5875 - Position of data field > RECORD-LENGTH. | Invalid parameter specified. | Check program and correct error.
ESY5876 - No 'NEW-' field for CHANGE request. | No NEW-CLASS, NEW-DESTINATION or NEW-USERID field was supplied for the CHANGE request. | Supply 'NEW-' value.
ESY5877 - VSAM (SHOWCAT) processing error. | A SHOWCAT error was detected when processing the requested VSAM catalog. |
ESY5878 - Volume defined as DYNAM/D pool name. | The requested volume is defined to Entire System Server as a CA-Dynam/D 'virtual' pool name. The requested function cannot be performed. |
ESY5881 - Error occurred while opening file. | An error occurred during OPEN. | Check the status of the dataset.
ESY5882 - Error occurred while closing file. | An error occurred during CLOSE. | Check the status of the dataset.
ESY5883 - Dataset is full. | The dataset is full. | Compress the PDS, or increase the dataset size.
ESY5886 - Event is in use. | An attempt was made to delete an event someone was waiting for. | Issue 'POST' request before deleting an event.
ESY5887 - Event is already defined. | An attempt was made to define an event which already exists. | No action is required.
ESY5888 - Event name must be specified. | An eventing request was issued without specifying the EVENT-NAME. | Specify an EVENT-NAME.
ESY5889 - Permanent I/O error while writing dataset. | An I/O error was detected during WRITE access. | This is probably a hardware error. Contact data center personnel.
ESY5890 - Event does not exist. | The specified event does not exist. | No action is required.
ESY5891 - Timeout waiting for event. | A timeout happened before the event was posted. | No action is required.
ESY5893 - Getmain failed. | There was not sufficient storage available to proceed with the request. | Notify systems programmer.
ESY5894 - Enable Eventing failed. | Internal eventing error occurred. | Contact technical support of Software AG.
ESY5895 - :1: must be specified. | Required value :1: was not specified. | Provide required value.
ESY5896 - Error occurred when sending e-mail. | Severe error occurred during e-mail processing. Further information is returned in field SYSTEM-MESSAGE to identify subfunction and response code. | Contact technical support of Software AG.
ESY5897 - Mailer response :1:. | Error :1: occurred during e-mail processing in Mailer function. E-mail was not delivered to recipient(s) if serious error occurred. | Contact Entire System Server Administrator. Mailer report may contain further error diagnostics.
ESY5899 - Permanent I/O error while reading dataset. | An I/O error was detected during READ access. | This is probably a hardware error. Contact data center personnel.

## System Messages ESY5900 - ESY5999

Message | Explanation | Action
--- | --- | ---
ESY5900 - Cannot allocate SYSOUT dataset. | Dynamic allocation of SYSOUT dataset failed. | Contact systems programmer.
ESY5901 - Cannot allocate internal reader. | Dynamic allocation of internal reader failed. | Contact systems programmer.
ESY5902 - Dynamic allocation failed. |  | Contact systems programmer.
ESY5903 - Dynamic allocation failed for temporary dataset. | Dynamic allocation for a temporary dataset failed. | Contact systems programmer.
ESY5904 - Edit not allowed (SCLM protection). | The selected PDS member has been protected by SCLM. Only browsing if this member is allowed, all update actions are denied. | Use SCLM dialog to free member.
ESY5906 - DESERV :1: error, R15=:2:, R0=:3: | An error occurred during execution of a DESERV macro. | Check the R15 and R0 values and if necessary Contact Software AG customer support.
ESY5907 - DSPSERV :1: error, R15=:2:, R0=:3: | An error occurred during execution of a DSPSERV macro. | Check the R15 and R0 values and if necessary Contact Software AG customer support.
ESY5908 - ALESERV :1: error, R15=:2:, R0=:3: | An error occurred during execution of an ALESERV macro. | Check the R15 and R0 values and if necessary Contact Software AG customer support.
ESY5909 - Syntax error in JCL command. | An error was detected when processing START-TIME on a SUBMIT request. | Fix error and resubmit.
ESY5921 - Entire System Server node table not linked. | Entire System Server node table not linked. | Contact systems programmer.
ESY5922 - Entire System Server node :1: not active. |  | Contact operator or contact systems programmer.
ESY5981 - Invalid value specified (BLKCTRL/BLKSIZE/LRECL). | Invalid value for BLOCK CONTROL, BLOCK SIZE or RECORD LENGTH specified. | Please correct error.
ESY5982 - Error during use of ISAM-key. | Possible reasons: - duplicate key detected for DUPEKY=NO; - key must be generated, but KEYLEN is greater than 8 bytes or no default KEYPOS; - key length of file is greater than 253 bytes; - key not found in ISAM-file; - no key supplied for UPDATE-INPLACE=YES; - invalid key sequence detected | Please check parameters or file attributes.
ESY5983 - :1: not supported by :2:. | Various functions are not supported in special modes. E.g. view EVENTING is only available in MULTI USER MODE for BS2000. Error text "SINGLE USER MODE not supported by EVENTING" occurs. | No action possible.
ESY5984 - Server is not authorized to access. | ESY Server Task is not authorized to access various objects with protection attributes, which not allows access for $TSOS. | No action possible.
ESY5985 - Access to tape file not allowed. | Access to tape file was requested, but parameter TAPES=NO is specified in ESY startup file. | Please contact your ESY Administrator.
ESY5986 - No or not enough space for :1:. | Various startup parameter sizes are exceeded. See variable text for details. | Please contact your ESY Administrator.
ESY5987 - Job Variable already exists. | An existing job variable cannot be allocated again. | Please check your input values.
ESY5988 - Invalid task type detected. | Task type must have a value between 1 and 7. | Correct program.
ESY5989 - Invalid ELEMENT specification. | Element name must be unique. | Correct element name.
ESY5990 - Field RECORD not found in format buffer. | An attempt was made to read a record without specifying the RECORD field. | Supply field RECORD in program.
ESY5991 - Unknown product. | An invalid PRODUCT value was specified. | Specify valid product code.
ESY5992 - Requested job variable not found. | The requested job variable is not cataloged. | No action required.
ESY5993 - Cannot open file. | An open request failed. | No action required.
ESY5994 - File not on volume. | The requested dataset is not on the specified volume. | No action is required.
ESY5995 - File not in catalog. | The dataset is not cataloged. | Specify VOLSER, or catalog dataset.
ESY5996 - Volume not online. | The specified volume is currently not available. | Contact operator or contact systems programmer.
ESY5997 - Dataset is not PDS or sequential. |  | No action is required.
ESY5998 - MEMBER not found. | The requested member was not found. | No action is required.
ESY5999 - Entire System Server node :1: not active. |  | Contact operator or contact systems programmer.

### On this page

- System Messages ESY3000 - ESY55xx
- System Messages ESY5600 - ESY5699
- System Messages ESY5700 - ESY5799
- System Messages ESY5800 - ESY5899
- System Messages ESY5900 - ESY5999