ARMT* - Adabas Review Interface Messages

#### Search Results

Search

# ARMT* - Adabas Review Interface Messages

### Overview of Messages

`ARMT01 | ARMT02 | ARMT03 | ARMT04 | ARMT05 | ARMT06 | ARMT07 | ARMT08 | ARMT09`

ARMT01 | dbid GETMAIN FAILURE, SIZE requested-getmain-size
Explanation | A request for storage in the Adabas nucleus failed.
Action | Either determine what is using so much storage in the Adabas nucleus and correct the problem; or increase the available storage.

ARMT02 | dbid ATTACH ADARST FAILURE, STRS nn
Explanation | The Adabas nucleus was unable to attach the subtask ADARST. STRS is the ADAIOR response code.
Action | Probably, the module ADARST is missing.

ARMT03 | dbid CLOG TOO BIG, CLOG NOT SENT
Explanation | When an ADABAS nucleus runs Adabas Review in hub mode, the CLOG inclusive CLOG extension and control information may be bigger than around 32K. This CLOG record is not sent to the Adabas Review hub. This message is only issued one time.
Action | One of the buffers may be too big. For instance, you may set LOGRB=NO.

ARMT04 | dbid ATTACH OF ADARST SUCCESSFUL
Explanation | The subtask ADARST was attached successfully. The database will send data to the Adabas Review hub.
Action | No action is required for this informational message.

ARMT05 | dbid DETACH OF ADARST SUCCESSFUL
Explanation | The subtask ADARST was detached successfully.
Action | Once you have corrected the error that led to detachment of ADARST, you can reactivate the subtask using the ADARUN parameter REVIEW=hubid. The successful ATTACH will be acknowledged with message ARMT04. A restart of the database is in this case not necessary. If the subtask abends a second time, it will be deactivated completely and message ARST10 will be given.

ARMT06 | dbid Review suspended, buffer unavailable. REVIEW parameter is set to NO.
Explanation | ADARMT is experiencing a temporary buffer shortage. The ADARUN parameter REVIEW is set to NO.
Action | To activate Review again, change the ADARUN REVIEW parameter.

ARMT07 | dbid Review resumed, nn CLOG records skipped
Explanation | Buffers have become available after the shortage noted by message ARMT06. The number of CLOG records skipped during the shortage is given in the message (nn).
Action | No action is required for this informational message.

ARMT08 | dbid Review suspended, subtask unable to initialize
Explanation | The subtask ADARST did not initialize. ADARST is detached and message ARMT05 appears. All Adabas Review processing from this nucleus is suspended.
Action | If you can correct the error that led to the initialization failure of ADARST, you can reactivate the subtask using the operator command REVIEW=hubid. The successful ATTACH will be acknowledged with message ARMT04. In this case, a restart of the database is not necessary. Notify your Software AG technical support representative if you are unable to resolve the initialization failure.

ARMT09 | dbid Review Trans-Port disabled after error
Explanation | Future records will be sent to the Hub using the command queue instead of Trans-Port. There should be additional messages in the Nucleus and Hub to identify the error.
Action | Correct the error. Reestablish Trans-Port by restarting the Nucleus or Review Hub.