ADAFRM JCL/JCS Requirements and Examples

#### Search Results

Search

# ADAFRM JCL/JCS Requirements and Examples

This section describes the job control information required to run the Delta Save functions of ADAFRM with BS2000/OSD, z/OS, z/VM, VSE/ESA and z/VSE systems, and shows examples of each of the job streams.

This document covers the following topics:

- z/OS

## z/OS

Data Set | DD Name | Storage | More Information
--- | --- | --- | ---
Delta Save images (DSIM) | DDDSIMR1 | disk | Required for DSIM... functions
ADAFRM parameters | DDKARTE |  |
ADARUN parameters | DDCARD |  | Adabas Operations
ADAFRM messages | DDDRUCK |  | Adabas Messages and Codes
ADARUN messages | DDPRINT |  | Adabas Messages and Codes

### Format DSIM Data Set (ADAFRM DSIMFRM)

    //FORMAT   EXEC  PGM=ADARUN
    //DDDSIMR1 DD  DSN=ADABAS.DB010.DSIMR1,DISP=(NEW,CATLG),
    //             VOL=SER=...,UNIT=...,SPACE=(CYL,20)
    //DDCARD   DD  *
    ADARUN    PROG=ADAFRM,...
    //DDKARTE  DD  *
    ADAFRM DSIMFRM SIZE=20,...
    //DDPRINT  DD  SYSOUT=*
    //DDDRUCK  DD  SYSOUT=*

### Reset DSIM Data Set (ADAFRM DSIMRESET)

    //FORMAT   EXEC  PGM=ADARUN
    //DDDSIMR1 DD  DSN=ADABAS.DB010.DSIMR1,DISP=OLD
    //DDCARD   DD  *
    ADARUN    PROG=ADAFRM, ...
    //DDKARTE  DD  *
    ADAFRM DSIMRESET FROMRABN=1,SIZE=1B
    //DDPRINT  DD  SYSOUT=*
    //DDDRUCK  DD  SYSOUT=*