ADAREP Utility

#### Search Results

Search

# ADAREP Utility

If a Delta Save logging (DLOG) area is defined in the database, the database report utility ADAREP additionally reports the Delta Save status. After the section about alternate RABNs, a Delta Save section is displayed with the following information:

- Delta Save status (disabled or enabled);

- percentage of the DLOG area used;

- number of full save operations since installation of the DLOG area;

- date and time of the last full save;

- number of Delta Save operations since the last full save;

- date and time of the last delta save;

- estimate of the number of database blocks that would be saved in a current Delta Save operation. The estimate may be higher or lower than the actual number of blocks.

- location, device type, block size, and number of unused blocks of the DLOG area.

If no DLOG area is defined, the Delta Save section is omitted.

This document covers the following topics:

- Delta Save Report Format

- Delta Save Checkpoints

- JCL/JCS Requirements and Examples

## Delta Save Report Format

The following is an example of the Delta Save section in an ADAREP database report:

      ***********************

      * DELTA SAVE FACILITY *                           yyyy-mm-dd  hh:mm:ss

      ***********************

      DELTA SAVE STATUS = ENABLED

      DLOG AREA USAGE   = 2%

      LAST FULL SAVE NUMBER        = 2

      DATE/TIME OF LAST FULL SAVE  = 1997-01-19 04:03:36

      LAST DELTA SAVE NUMBER       = 5

      DATE/TIME OF LAST DELTA SAVE = 1997-01-24 22:39:45

      ESTIMATED NUMBER OF CHANGED BLOCKS = CA. 1,700 BLOCKS

      D S F   L O G G I N G   A R E A

      LIST I DEV  BLOCK I  SPACE ALLOC.  I  FROM     TO   I  UNUSED SPACE  I

      TYPE I TYPE LNGTH I BLOCKS     CYL I  RABN    RABN  I BLOCKS     CYL I

           I            I                I                I                I

      -----I------------I----------------I----------------I----------------I

           I            I                I                I                I

      DSF  I 3390  2004 I    100       0 I  1340    1439  I    74        0 I

           I            I                I                I                I

      ----------------------------------------------------------------------

## Delta Save Checkpoints

The following additional checkpoints can be written by the Adabas nucleus or utilities and included in the ADAREP output when running with the Delta Save Facility:

Checkpoint | Originated | Description
--- | --- | ---
Type | Name | By
0B | SYNP | ADASAV | End of SAVE DELTA operation
0C | SYNP | ADASAV | End of RESTORE DELTA operation
0D | SYNP | ADASAV | End of MERGE operation
0E | SYNV | ADASAV | VOLSER entry for SAVE DELTA operation
0F | SYNV | ADASAV | VOLSER entry for MERGE operation (output volumes)
6A | SYNS | SYSAOS | DSF logging (DLOG) area installed
6B | SYNS | SYSAOS | DLOG area changed
6C | SYNS | SYSAOS | DLOG area removed

## JCL/JCS Requirements and Examples

This section describes the job control information required to run the ADAREP utility with BS2000/OSD, z/OS, z/VM, VSE/ESA and z/VSE systems, and shows examples of each of the job streams.

This section covers the following topics:

- z/OS

### z/OS

Data Set | DD Name | Storage | More Information
--- | --- | --- | ---
Associator | DDASSORn | disk |
Data Storage | DDDATARn | disk |
ADAREP parameters | DDKARTE |  |
ADARUN parameters | DDCARD |  | Adabas Operations
ADAREP messages | DDDRUCK |  | Adabas Messages and Codes
ADARUN messages | DDPRINT |  | Adabas Messages and Codes

#### Example

    //REP       EXEC PGM=ADARUN
    //STEPLIB   DD   DISP=SHR,DSN=ADABAS.Vvrs.LOADLIB
    //*
    //DDASSOR1  DD   DISP=SHR,DSN=EXAMPLE.ADA99.ASSOR1
    //DDDATAR1  DD   DISP=SHR,DSN=EXAMPLE.ADA99.DATAR1
    //SYSUDUMP  DD   SYSOUT=A
    //DDDRUCK   DD   SYSOUT=A
    //DDPRINT   DD   SYSOUT=A
    //DDCARD    DD   *
    ADARUN PROG=ADAREP,SVC=249,DEVICE=3390,DB=99
    //DDKARTE   DD   *
    ADAREP    CPLIST

### On this page

- Delta Save Report Format
- Delta Save Checkpoints
- JCL/JCS Requirements and Examples