Component Summary

#### Search Results

Search

# Component Summary

Component | Number
--- | ---
Entire Net-Work | One per operating system image
ADASVC/SVCCLU | One per operating system image
ADACOM | Zero, one, or more per sysplex; required for each operating system image that has cluster users but no cluster nuclei; optional but recommended for operating system images that have cluster nuclei.
PPT | One per cluster; located in the database Associator
Adabas DBIDs | One per cluster; a practically unlimited number per sysplex
sysplex cache structures | One per cluster; specified in each nucleus
sysplex lock structures | One per cluster; specified in each nucleus
XCF group names | One per cluster; specified in each nucleus
Adabas nuclei | Up to 32 per cluster