NETE* - zEnterprise Data Compression (zEDC) Support Messages

#### Search Results

Search

# NETE* - zEnterprise Data Compression (zEDC) Support Messages

### Overview of Messages

`NETE001I | NETE002E | NETE003E | NETE004E | NETE005E`

NETE001I | IBM zEDC compression services interface active
Explanation | Initialization of IBM’s system zEnterprise Data Compression (zEDC) services was successful.
Action | No action is required for this informational message.

NETE002E | IBM zEDC compression services interface failed
Explanation | Initialization of IBM’s System zEnterprise Data Compression (zEDC) services failed. Entire Net-Work was unable to load one or more zEDC support modules.
Action | Verify that the required zEDC modules are available for Entire Net-Work to load. If compression is not required, set the ZEDC LINK parameter to N.

NETE003E | Cannot active zEDC compression services. LPAR Capabilities down level
Explanation | Entire Net-Work's invocation of IBM's zEnterprise Data Compression (zEDC) services "FPZARZV" indicated that the LPAR does not support zEDC compression.
Action | Contact your IBM support specialist if you want to use zEDC.

NETE004E | Unable to LOAD IBM Compression Support Modules, Reason Code=nnnnnnnn
Explanation | The Entire Net-Work module "Netzedc" was unable to load IBM's zEnterprise Data Compression (zEDC) services "FPZ4*".
Action | Verify that Entire Net-Work has access to the IBM’s zEDC support modules FPZ4RZV,FPZ4PRB, FPZ4RMR, FPZ4DMR, FPZ4ABC and FPZ4URZ. If the problem persists, contact your Software AG technical support representative.

NETE005E | Attempting to initialize previously initialized zEDC support interface
Explanation | The Entire Net-Work module "Netzedc" detected a second zEDC initialization call. Only one initialization invocation is allowed.
Action | Contact your Software AG technical support representative for assistance.