Entire Net-Work Message Formats

#### Search Results

Search

# Entire Net-Work Message Formats

Each message is identified by a six- or seven-character alphanumeric identifier as described in the following table:

Message | Description
--- | ---
NETnnnn | Entire Net-Work control module messages.
NETBnnn | Expandable buffer pool messages.
NETInn | These Entire Net-Work system messages correspond to ADAIOR messages documented in the Adabas Messages and Codes manual. The Entire Net-Work messages begin with NETI; the corresponding ADAIOR messages begin with ADAI.
NETMnn | These Entire Net-Work system messages correspond to ADAMPM messages documented in the Adabas Messages and Codes manual. The Entire Net-Work messages begin with NETM; the corresponding ADAMPM messages begin with ADAM.
NETPnnn | TCPX line driver messages.
NETUnnn | Batch utility program messages.