Requirements and Restrictions

#### Search Results

Search

# Requirements and Restrictions

This document describes the requirements and restrictions of Entire Net-Work Administration.

- Adabas Components

- TCP/IP Transport Providers Supported

Note
Entire Net-Work 6.4 SP1 is compatible with Entire Net-Work 6.3 SP2 nodes.

## Adabas Components

Entire Net-Work 6.4 requires the Adabas 8 components supplied in Adabas Limited Load Library (WAL) and the SVC from Adabas 8.2.2 (or later). However, before Entire Net-Work can function correctly, the most recent fix data set must be concatenated in front of the standard WAL load library.

Be sure your enterprise is running with the most current fix solution for WAL supported by Entire Net-Work 6.3, when available for that platform.

Important
You should always use the most current Adabas load library or the Adabas limited library (WAL) as provided on the Entire Net-Work installation media, unless you have been specifically instructed otherwise by Software AG.

## TCP/IP Transport Providers Supported

Entire Net-Work 6.5 supports the following levels of TCP/IP transport providers:

Platform | TCP/IP Protocol Supported
--- | ---
z/OS | IBM TCP/IP for z/OS Version 1.10, 1.11, and 1.12.
z/VSE | IBM and Connectivity Systems TCP/IP z/VSE Version 4.2 and 4.3.
BS2000/OSD Sockets Subsystem | Sockets Version 2.0 and above. For Sockets 2.2 and above, the SOC6 subsystem will be used, otherwise the SOCKETS subsystem is used. When accessing via IPV6 addressing, a SOC6 subsystem with Sockets 2.5 is the minimum requirement.

### On this page

- Adabas Components
- TCP/IP Transport Providers Supported