UTIMER Utility

#### Search Results

Search

# UTIMER Utility

### Overview of Messages

`UTM0001 | UTM0002 | UTM0003 | UTM0004`

UTM0001 | System error loading UTMEX1. Inform your system group.
Explanation: | An error occurred while loading the exit UTMEX1.

UTM0002 | No region for UTMEX1. Inform your system group.
Explanation: | Increase the region size for UTIMRM with ULIB.

UTM0003 | Timer SD file in use. Please try later.
Explanation: | The timer utility uses a Com-plete SD file to store the requests for the timer monitor. This SD file is in use by another user.

UTM0004 | Timer SD too small. Inform your system group.
Explanation: | The timer SD file has not enough space to add this request.
System programmer info: | The default number of timer SD file records is 1000. It can be increased by a zap in UTIMER.