Terminal Access Method

#### Search Results

Search

# Terminal Access Method

### Overview of Messages

`TAM0001 | TAM0002 | TAM0003 | TAM0004 | TAM0005 | TAM0006 | TAM0007 | TAM0008 | TAM0009 | TAM0010 | TAM0011 | TAM0012 | TAM0013 | TAM0014 | TAM0015 | TAM0016 | TAM0017 | TAM0018 | TAM0019 | TAM0020 | TAM0021 | TAM0022 | TAM0023`

TAM0001 | No program active
Explanation: | This message is associated with the Com-plete terminal access method. It appears when Com-plete could not accept a terminal entry for one of the following reasons: The terminal operator entered NULL INPUT from a terminal that was not in conversation with a program. The terminal operator attempted to enter data for a program without first calling the program. The terminal operator attempted to call a program without preceding the request with an asterisk (*). The terminal operator entered '*EOJ' or '*CANCEL' from a terminal that was not in conversation with a program.
System action: | The terminal entry is ignored.
Terminal operator info: | Com-plete will not accept entries from a terminal unless one of these procedures is followed: To use a Com-plete application program or utility, call it by entering the '*program' or '*utility' (e.g. '*UDUMP') desired. To use a program that had ended, reenter the '*program-name' command.

TAM0002 | No more stacking slots
Explanation: | Continue with the execution of present transaction.

TAM0003 | $1 not found in library
Explanation: | This message is associated with the Com-plete terminal access method. It appears when Com-plete did not find the program $1 in its library of application programs.
System action: | The terminal entry is ignored.
Terminal operator info: | When attempting to initiate a program by entering '*program-name', the program must reside in the Com-plete library. If it does not, this message will appear. The most common cause of this error is incorrect entry of a program name. Reenter the request. If this message reappears, contact the application programmer responsible for the program.
Appl. programmer info: | Refer to the Com-plete User Utilities Manual for information about how to catalog a program.

TAM0004 | I/O error occurred during load for $1
Explanation: | This message is associated with the Com-plete terminal access method. It appears when a disk I/O error has occurred while Com-plete was hod. attempting to load a program from the Com-plete program library.
System action: | The terminal entry is ignored.
Terminal operator info: | This error was probably caused by a hardware failure. Notify the Com-plete system programmer.
System programmer info: | Move the entire library to another location.

TAM0005 | Invalid page number requested
Explanation: | This message is associated with Com-plete's terminal access method. It appears when the terminal operator specified a non-numeric character for a page number in a page display request.
System action: | The terminal entry is ignored.
Terminal operator info: | Page numbers in display requests may not contain non-numeric characters. For more information, refer to the Com-plete User Utilities Manual.

TAM0006 | Requested page not built by program
Explanation: | This message is associated with Com-plete's terminal access method. It appears when the page number requested by the terminal operator was higher than the highest page built by the program that created the page file.
System action: | The terminal entry is ignored.
Terminal operator info: | Reenter the paging request specifying a smaller number. To display the highest page in the page file, enter *UP/H. For more information, refer to the Com-plete User Utilities Manual.

TAM0007 | No pages built by program
Explanation: | This message is associated with Com-plete's terminal access method. It appears when the terminal operator has attempted to display a page when there were no pages built for the terminal in use.
System action: | The terminal entry is ignored.
Terminal operator info: | The program in use did not build a paging file. If the program is expected to have built a paging file, contact the application programmer responsible for the program in use when the error occurred. For more information, refer to the Com-plete User Utilities Manual.

TAM0008 | $1 is an invalid program name
Explanation: | This message appears when the terminal operator has attempted to call the program $1 and either or both of the following conditions prevented Com-plete from initiating conversation: The program name $1 contained characters other than A through Z or 0 through 9. The program name $1 began with a numeric character.
System action: | The terminal entry is ignored.
Terminal operator info: | Enter a valid program name.

TAM0009 | Program name specified was too long
Explanation: | This message is associated with the Com-plete terminal access method. It appears when the program name specified by the terminal operator contained more than six characters.
System action: | The terminal entry is ignored.
Terminal operator info: | Enter a valid program name.

TAM0010 | Permanent error on Tid $1 - Sense=$2, CSWSTAT=$3.
Explanation: | This message is associated with the Com-plete terminal access method. It appears when three successive I/O errors have occurred while Com-plete was attempting to read or write the terminal TID $1.
System action: | If the error occurred while Com-plete was attempting to read a terminal operator's response to a program, control is passed to the program at the point immediately following the read operation and the return code is set to indicate that an error occurred. If the error occurred while Com-plete was attempting to read a terminal that was not in conversation with a program, Com-plete attempts to write the TAM0001 message to the terminal. If the error occurred while Com-plete was performing a WRTD operation at the request of a user program, the TAM0012 message is written to the operator console. The user program's output is not written. If the error occurred while Com-plete was performing another type of write operation at the request of a user program, control is passed to the program at the point immediately following the write operation, and the return code is set to indicate that an error has occurred.
System programmer info: | The value $2 is the sense data associated with the hardware error. For information on how to evaluate this data, see the appropriate hardware manual for the device type that experienced the error. The value $3 is the status flag from the CSW associated with the error.
Computer operator info: | Seek the assistance of the Com-plete system programmer. Place the terminal TID $1 on IGNORE status until the problem can be determined.

TAM0011 | Permanent error on Tid $1.
Explanation: | This message is associated with the Com-plete terminal access method. It appears when three successive I/O errors have occurred while Com-plete was attempting to read or write to the terminal TID $1.
System action: | If the error occurred while Com-plete was attempting to read a terminal operator's response to a program, control is passed to the program at the point immediately following the read operation, and the return code is set to indicate that an error occurred. If the error occurred while Com-plete was attempting to read a terminal that was not in conversation with a program, Com-plete attempts to write the TAM0001 message to the terminal. If the error occurred while Com-plete was performing a WRTD operation at the request of a user program, the TAM0012 message is written to the operator console. The user program's output is not written. If the error occurred while Com-plete was performing another type of write operation at the request of a user program, control is passed to the program at the point immediately following the write operation, and the return code is set to indicate that an error has occurred.
System programmer info: | This message is accompanied by another Com-plete error message that supplies more information about the nature of the error and the appropriate action to be taken.
Computer operator info: | Seek the assistance of the Com-plete system programmer. Place the terminal TID $1 on IGNORE status until the problem can be determined.

TAM0012 | Permanent write error with DISP=DONE on Tid $1.
Explanation: | This message is associated with the Com-plete terminal access method. It appears when three successive I/O errors have occurred while Com-plete was attempting to write to the terminal TID $1 at the request of the user program.
System action: | The error is ignored. Com-plete was unable to return the error condition to the user program because the write operation had a disposition of DONE.
System programmer info: | This message is accompanied by another Com-plete error message that supplies more information about the nature of the error and the appropriate action to take.
Computer operator info: | Seek the assistance of the Com-plete system programmer.

TAM0013 | Use of application $1 has been suspended by an administrator
Explanation: | Start or continuation of the application was denied because its use has been suspended.
System programmer info: | The "suspended" flag for an application can be switched in ULIB.
Terminal operator info: | If you feel like the use of the application should not be suspended, contact your Com-plete system administrator.

TAM0014 | Tid $1 ignored due to intervention required
Explanation: | This message is associated with the Com-plete terminal access method. It appears when successive I/O errors have occurred while Com-plete was s attempting to write to the terminal TID $1 at the request of the user program.
System action: | The error is ignored. Com-plete was unable to return the error condition to the user program because the write operation had a disposition of DONE.
System programmer info: | This message is accompanied by other Com-plete error messages supplying more information about the nature of the error and the appropriate action to take.
Computer operator info: | Seek the assistance of the Com-plete system programmer.

TAM0015 | Autologoff: User=$1, Tid=$2 $3
Explanation: | Self-explanatory message.

TAM0016 | $1
Explanation: | This message is issued when an attached task attempts to issue a write or Com-plete attempts to write to the attached task 'terminal' for an abend or such like, and no attaching terminal can be identified for the attached task to which the message must be written. $1 is the text of the message that was to be sent. This generally will only occur for tasks attached via the operator command 'USER' or via the Com-plete startup parameter 'STARTUPPGM'. When the Com-plete 'Attach' function is used, the attacher can always be identified.

TAM0017 | Terminal operator requested *CANCEL
Explanation: | The terminal operator entered *CANCEL thus forcing an utility abend.

TAM0018 | No eligible thread for program $1
Explanation: | The program $1 was requested by the user, however, due to the size with which this program was catalogued, there was no thread large enough defined to the system in which to run the program.
Terminal operator info: | Report the error to your system administrator.
System programmer info: | This message indicates that either a program is catalogued too large and the catalog size must be reduced so that it can fit into one of the defined threads in the system, or one or more threads large enough to accomodate the program must be defined.

TAM0019 | Program $1, Logon required - Enter '*ULOG ON' to logon
Explanation: | The user requested that program $1 be started, however, system options have determined that the terminal user must logon to Com-plete before this program can be executed.
System programmer info: | This indicates that this program has not been catalogued with the option indicating that it can be run before logon. If the program should be available before logon to the system, change the catalog options with the ULIB utility.
Terminal operator info: | To logon to the system, enter '*ULOG ON' and you will be presented to with a logon menu. If you should be able to run program $1 without logging on, contact your system administrator.

TAM0020 | Access to program $1 disallowed
Explanation: | An attempt was made to run program $1, however, system definitions have disallowed access to this program from the userid currently logged on to the terminal.
Terminal operator info: | If you require access to program $1, contact your system administrator.
System programmer info: | This indicates that the user is a Com-pass user and does not have access to this program based on the Com-pass definition. Should access be required, the userid definition should be altered and the user must then logoff and logon again. If the program should be generally available, the catalog option for the program should be changed with the ULIB utility.

TAM0021 | Program $1 not executed, no eligible processor group
Explanation: | An attempt was made to run the program $1, however this failed as there was no eligible processor group available to run the program.
Terminal operator info: | If you should be in a position to run this program, contact your system administrator.
System programmer info: | This indicates that program $1 has been catalogued using ULIB to run on a particular group of processors. This group is either not active or quiescing.

TAM0022 | Program $1 not executed, system is quiescing
Explanation: | An attempt was made to run program $1 however, this was not accepted as a system quiesce has been requested by the system operator.
System programmer info: | It is possible for a program to be started while the system is in this state by changing the catalog options for the program in ULIB. Refer to the documentation on this utility for more information.

TAM0023 | Program $1 not executed, no storage for internal buffer
Explanation: | A request to run the program $1 failed because there was not enough storage to start the program.
Terminal operator info: | Report the error to your system administrator.
System programmer info: | This indicates that an internal error to get storage failed. There will have been a prior fixed buffer pool manager error which will indicate why the request to get storage failed.