Stopping the CONNX CICS/Adabas TCP/IP Listener
You can stop the CONNX CICS/Adabas TCP/IP listener program with the NX01 transaction from an authorized 3270 terminal session. The NX01 STOP command gracefully terminates the CONNX CICS/Adabas TCP/IP listener, and permits it to be restarted on the same or on a different TCP/IP port. To stop the CONNX CICS/Adabas TCP/IP Listener:
1. Verify that the CONNX CICS TCP/IP listener transaction/program (NX00/CNXRUN) is running by typing cemt inq ta. Press <Enter>.
2. Verification appears. Press the F3 key, and then press <Clear>.
3. Enter NX01 STOP.
Verification appears.
You can further verify that the CONNX CICS TCP/IP listener transaction/program (NX00/CNXRUN) is stopped by issuing a second CEMT INQ TA command, which shows that the NX00 task has been stopped. You can restart the CONNX CICS/Adabas TCP/IP Listener program on the same TCP/IP port, or you can change the TCP/IP port using the NX01 CNXRUNPORT command, and restart the listener on a different port.