Importing from SCT COBOL FD (File Definition) Files - MVS-OS/390
This procedure is site-specific for SCT customers using CONNX for VSAM with either CICS or Started Task. See Importing from VSAM COBOL FD Files (CICS) - MVS z/OS for information on how to verify FTP access.
Note:
See CONNX and SCT Import Rules for definitions of the SCT import rules.
1. Click the Import button in the CONNX CDD Windows Application window.
2. Select VSAM SCT COBOL FD files in the Import Type list box.
3. Type an SCT COBOL FD partitioned data set and member name in the Enter an SCT COBOL FD data set member text box and click the OK button.
Specify the fully qualified partitioned data set and member name for an SCT file, for example, to import the SCT AAFILE, enter: SCT.SISBASE.SOURCE(ACAARC)
4. From the list of available files, select each to display the properties, columns, and indexes.
5. Save the CDD by selecting the File menu and then clicking Save.
Partial (for example, AC*) or complete (*) wildcard characters may be used in place of a file name during import.
If CONNX detects more than one record layout when importing, multiple data dictionary entries are created.