Importing from VSAM COBOL FD files (CICS) - VSE
To import VSAM COBOL FD files:
1. Click the Import button in the CONNX Data Dictionary Manager window.
2. Select VSAM COBOL FD files in the Import Type list box.
3. Type a fully qualified library.sublib.member.type name in the Enter a COBOL FD data set member text box, for example cnxvvrr.copybook.customer.c
The COBOL copybook that you want to import must reside in a library.sublib and the library must be defined to the TCP/IP file system. This can be done via operating system console commands or via the IPINIT00 batch job. The following examples assume that the sample CONNX COBOL copybooks reside in VSAM-managed library CNXVVRR:
Via VSE console commands:
msg f7
AR 0015 1I40I READY
F7-0102 IPN300I Enter TCP/IP Command
102 def file,pub=CNXV8R8,dlbl=CNXV8R8,type=lib
F7 0100 IPN264I File defined, Dataset: CNXV8R8
Via batch JCL - Add the following control record to the IPINIT00 member as discussed above, submit the batch job, and stop/restart TCP/IP:
DEFINE FILE,PUBLIC='CNXV8R8', DLBL=CNXV8R8, TYPE=LIBRARY,READONLY=NO
4. After defining the CONNX library to TCP/IP, you can import from a COBOL copybook by specifying the fully-qualified library.sublib.member.type name, for example:
CNXVVRR.COPYBOOK.CUSTOMER.C
5. To verify the entries currently defined for FTP access to the VSE TCP/IP job, start an FTP session using the Windows command prompt, and enter the dir command.
A COBOL FD specification does not contain the CICS FCT (File Control Table) name; therefore, it must be specified on the Table Properties tab in the CONNX Data Dictionary Manager when the data is returned.
All of the record layouts in the specified file are imported. No additional logon information is required.
6. Type a CICS user name in the User Name text box.
The CICS user ID must be authorized for FTP access to the target host. The most common way to authorize a VSE userid for TCP/IP is to hardcode it in the TCP/IP initialization data set. For example, edit member IPINIT00 in the TCP/IP ICCF library and add the appropriate user ID and password:
DEFINE USER, ID=CONX, PASSWORD=CONNXVSE
and then submit job IPINIT00 to the POWER reader queue.
Additional security strategies are documented in the following manuals published by Connectivity Systems Incorporated: TCP/IP for VSE Commands Version 1 Release 4, TCP/IP for VSE Installation Guide Version 1 Release 4
7. Type a CICS password in the Password text box.
The TCPIP port number is set to 6500 by default, but can be configured via the CONNX NX01 CICS transaction.
8. Select a Destination Database for the imported tables.
9. Select each file imported file and follow these steps:
a. Click the Table Properties tab in the CONNX Data Dictionary Manager window.
b. Type the CICS FCT name for the file in the CICS File Name text box. For example, the CICS short file name for the CONNX VSAM KSDS sample customer file is CNXCSTK.
c. Tab out of the CICS File Name text box to display the CONNX Database Logon dialog box. Click the OK button.
d. Click the Table Indexes tab to display the key information for the imported CICS VSAM file.
If the Table Index information list box is empty, click the Refresh Indexes button. If the list box remains empty, no indexes are defined on the imported VSAM file.
e. Repeat steps a) through e) for each file for which there is imported metadata.
f. Click File -> Save.
For the CONNX sample files using the CNXVVRR.COPYBOOK library.sublibrary, select from this list of member names and CICS file names:

CNXVVRR.COPYBOOK library.sublibrary Member Names | CICS File Name
CUSTOMER.C | CNXCSTK
CUSTOMRE.C | CNXCSTE
CUSTOMRR.C | CNXCSTR
EQUIPMNE.C | CNXEQE
EQUIPMNR.C | CNXEQR
EQUIPMNT.C | CNXEQK
ORDER.C | CNXORK
ORDERE.C | CNXORE
ORDERR.C | CNXORR
PRODGRP.C | CNXPGK
PRODGRPE.C | CNXPGE
PRODGRPR.C | CNXPGR
PRODUCT.C | CNXPRDK
PRODUCTE.C | CNXPRDE
PRODUCTR.C | CNXPRDR

Note:
For your site, specify the COBOL copybook library.sublib.member.type and the corresponding CICS file name to import test or production metadata.