Blacklist Maintenance

#### Search Results

Search

# Blacklist Maintenance

This function is used to maintain a blacklist of Natural objects. In a blacklist, you can specify the Natural objects that are not to be loaded into the buffer pool; objects that are already loaded in the buffer pool are then deleted. If the BP cache is enabled, the Natural objects will also be deleted from the BP cache. The blacklist always applies to the buffer pool currently active.

In a blacklist, you can maintain individual Natural objects and/or libraries and object sets which contain multiple Natural objects. In an object set, you specify the objects not to be executed and add a single set (instead of multiple individual objects) to the blacklist. You can also combine both: maintain objects individually or by sets.

The source code of an object set is stored as a Natural source object of the type Text in the current Natural library and system file. The first line of an object set source contains the comment `**BBL**` (buffer pool blacklist).

For further information on the blacklist, see the relevant section in Natural Buffer Pool in the Operations documentation.

To invoke Blacklist Maintenance

- In the SYSBPM Main Menu, enter the following function code:

      B

  Oder:
  Enter the following SYSBPM direct command:

      BLACKLIST

  The Blacklist Maintenance menu appears.

The functions provided in the Blacklist Maintenance menu are explained in the following section. This section also provides information on additional blacklist maintenance functions.

- Maintain Blacklist

- List Object Sets

- Edit Object Set

- Add Object Set to Blacklist

- Delete Object Set from Blacklist

- Delete Object Set Source Object

- Additional Object Set Maintenance with Utilities

- Blacklist Maintenance in Batch Mode

## Maintain Blacklist

This function invokes the Maintain Blacklist screen where you can display and maintain all Natural objects currently available in the blacklist.

To invoke the Maintain Blacklist screen

- In the Blacklist Maintenance menu, enter the following function code:

      M

  Oder:
  Enter the following SYSBPM direct command:

      DISPLAY BLACKLIST

  The Maintain Blacklist screen appears with the current blacklist. Press PF7 to scroll one page backward and PF8 to scroll one page forward.

Depending on the mode set when calling the Maintain Blacklist function earlier during a SYSBPM session, the Maintain Blacklist screen appears in Display Mode (default when initializing SYSBPM) or Add Mode. Use PF9 to switch from one mode to the other.

This section covers the following topics:

- Adding Objects

- Modifying Objects

- Deleting Objects

### Adding Objects

To add objects to the blacklist

1. In the Blacklist Maintenance menu, enter the following function code:

       M

   Oder:
   Enter the following SYSBPM direct command:

       DISPLAY BLACKLIST

   The Maintain Blacklist screen appears.

2. If required, press PF9 to switch to Add Mode.

   A screen with empty input fields appears.

3. In the relevant selection fields, enter the name of the library where the objects are stored, the names of the objects and the corresponding database IDs (DBID) and file numbers (FNR). If DBID and FNR are left blank, they will be taken from the current system file FUSER or FNAT in libraries whose names start with SYS (except the library SYSTEM).

   If you need to clear the Add Mode screen, in the Command line, enter either of the following:

       CLE

   or

       CLEAR

4. Press PF5 to confirm the addition.

   Oder:
   In the Command line, enter either of the following:

       UP

   or

       UPDATE

   An appropriate message appears.

### Modifying Objects

To modify objects on the blacklist

1. In the Blacklist Maintenance menu, enter the following function code:

       M

   Oder:
   Enter the following SYSBPM direct command:

       DISPLAY BLACKLIST

   The Maintain Blacklist screen appears.

2. If required, press PF9 to switch to Display Mode and obtain the list of all objects currently contained in the blacklist.

3. In the relevant input field(s), replace the existing entries with new values.

4. Press PF5 to confirm the modification.

   Oder:
   In the Command line, enter either of the following:

       UP

   or

       UPDATE

   An appropriate message appears.

### Deleting Objects

To delete individual objects from the blacklist

1. In the Blacklist Maintenance menu, enter the following function code:

       M

   Oder:
   Enter the following SYSBPM direct command:

       DISPLAY BLACKLIST

   The Maintain Blacklist screen appears.

2. If required, press PF9 to switch to Display Mode and obtain a list of all objects currently on the blacklist.

3. In column C, next to the object(s) required, enter the following line command:

       DE

4. Press ENTER to confirm the deletion.

   An appropriate message appears.

To delete all objects from the blacklist

1. In the Blacklist Maintenance menu, enter the following function code:

       M

   Oder:
   Enter the following SYSBPM direct command:

       DISPLAY BLACKLIST

   The Maintain Blacklist screen appears.

2. Press PF2.

   The Confirm Delete window appears.

3. Confirm the deletion, by entering `Y` (Yes).

   Oder:
   Cancel the deletion, by entering `N` (No; this is the default) or by pressing PF3 without entering anything in the window.

4. Press ENTER to confirm the action.

   An appropriate message appears.

## List Object Sets

This function invokes the List Object Sets screen which displays a list of all existing object sets.

To invoke the List Object Sets screen

- In the Blacklist Maintenance menu, enter function code `L`, a library name and an object set name. Asterisk (*) notation is also allowed for an object set name.

  Oder:
  Enter the following SYSBPM direct command:

      LIST SET library-name set-name

  Asterisk (*) notation is also allowed for set-name.

  The List Object Sets screen appears with the specified set(s).

You can manipulate an object set from the List Object Sets screen by using any of the line commands provided to modify a set and add it to or delete it from the blacklist. For a list of possible line commands, enter a question mark (?) in the leftmost screen column (prefix information).

For a list of commands that can be entered in the command line of the List Object Sets screen, invoke the Help window by entering a question mark (?) in the command line. If required, press PF7 to scroll backward and PF8 to scroll forward in the window.

## Edit Object Set

This function invokes the Edit Object Set screen where you can create a new object set, add objects to an existing set or modify them, or delete objects from a set.

The editing functions provided on the Edit Object Set screen are a subset of the functions provided by the Software AG Editor described in the Editors documentation.

For a list of available line commands, enter a question mark (?) in the leftmost screen column (prefix information).

For a list of commands that can be entered in the command line of the Edit Object Set screen, invoke the Help window by entering a question mark (?) in the command line. If required, press PF7 to scroll backward and PF8 to scroll forward in the window.

This section covers the following topics:

- Creating Object Sets

- Modifying Object Sets

### Creating Object Sets

To create an object set

1. In the Blacklist Maintenance menu, enter function code `E` and a library name. Do not enter the name of an object set but clear the contents (if any) of the corresponding field.

   The Edit Object Set screen appears.

2. In the relevant input fields, enter the name of the library where the objects are stored, the names of the objects and the corresponding database IDs (DBID) and file numbers (FNR). If DBID and FNR are left blank, they will be taken from the current system file FUSER or FNAT in libraries whose names start with SYS (except the library SYSTEM).

3. To save the object set as a source object of the type Text, in the command line of the Edit Object Set screen, enter the following:

       SA set-name

### Modifying Object Sets

This section provides instructions for adding objects to an object set, modifying existing objects and deleting objects from an object set. Note that any of these object set modifications will not update the current blacklist.

To add a new object to an object set

1. In the Blacklist Maintenance menu, enter function code `E`, a library name and an object set name.

   Oder:
   On the List Object Sets screen, in the leftmost column, next to the object set required, enter the following line command:

       E

   Oder:
   Enter the following SYSBPM direct command:

       EDIT SET library-name set-name

   The Edit Object Set screen appears with the specified object set.

2. Complete the input fields by entering the name of the library where the objects are stored, the names of the objects and the corresponding database IDs (DBID) and file numbers (FNR). If DBID and FNR are left blank, they will be taken from the current system file FUSER or FNAT in libraries whose names start with SYS (except the library SYSTEM).

3. To save the modifications, in the command line of the Edit Object Set screen, enter the following:

       SA

To modify an object of an object set

1. In the Blacklist Maintenance menu, enter function code `E`, a library name and an object set name.

   Oder:
   On the List Object Sets screen, in the leftmost column, next to the object set(s) required, enter the following line command:

       E

   Oder:
   Enter the following SYSBPM direct command:

       EDIT SET library-name set-name

   The Edit Object Set screen appears with the specified object set.

2. In the relevant input field(s), replace the existing entries with new values.

3. To save the modifications, in the command line of the Edit Object Set screen, enter the following:

       SA

To delete an object from an object set

1. In the Blacklist Maintenance menu, enter function code `E`, a library name and an object set name.

   Oder:
   On the List Object Sets screen, in the leftmost column, next to the object set(s) required, enter the following line command:

       E

   Oder:
   Enter the following SYSBPM direct command:

       EDIT SET library-name set-name

   The Edit Object Set screen appears with the specified object set.

2. In the leftmost column, next to the object required, enter the following line command:

       D

   The specified object is removed from the object set.

3. To save the modification, in the command line of the Edit Object Set screen, enter the following:

       SA

## Add Object Set to Blacklist

This function is used to add all objects of an object set to the blacklist.

To add an object set to the blacklist

- In the Blacklist Maintenance menu, enter function code `A`, a library name and an object set name.

  Oder:
  On the List Object Sets screen, in the leftmost column, next to the object set(s) required, enter the following line command:

      AC

  Oder:
  On the Edit Object Set screen, in the command line, enter the following:

      AC

  Oder:
  Enter the following SYSBPM direct command:

      ADD SET library-name set-name

  A message appears confirming that the object set was added to the blacklist.

Anmerkung
The command `AC` denotes `ACTIVATE` which is the equivalent of Add Object Set to Blacklist.

## Delete Object Set from Blacklist

This function is used to delete all objects of an object set from the blacklist. Note that the Delete Object Set function will not delete the object set as a source object. The objects of the object set can be added to the blacklist again at any time, as described above. See also Delete Object Set Source Object.

To delete an object set from the blacklist

- In the Blacklist Maintenance menu, enter function code `D`, a library name and an object set name.

  Oder:
  On the List Object Sets screen, in the leftmost column, next to the object set(s) required, enter the following line command:

      DA

  Oder:
  On the Edit Object Set screen, in the command line, enter the following:

      DA

  Oder:
  Enter the following SYSBPM direct command:

      DELETE SET library-name set-name

  A message appears confirming that the object set was deleted from the blacklist.

Anmerkung
The command `DA` denotes `DEACTIVATE` which is the equivalent of Delete Object Set from Blacklist.

## Delete Object Set Source Object

To delete the source object of an object set

1. In the Blacklist Maintenance menu, enter function code `L`, a library name and an object set name.

   Oder:
   Enter the following SYSBPM direct command:

       LIST SET library-name list-name

   The List Object Sets screen appears.

2. In the leftmost column, next to the object set required, enter the following line command:

       D

   The DELETE window appears.

3. Confirm the deletion by entering the name of the object set.

   A confirmation message appears.

Anmerkung
Deleting the source object of an object set will not update the current blacklist.

## Additional Object Set Maintenance with Utilities

The Natural utilities SYSMAIN and Object Handler provide additional functions for maintaining object sets. Functions include transferring object sets between different Natural libraries and system files and/or different mainframe platforms and deleting or finding object sets in a different environment.

When using a Natural utility, an object set is treated like any other source object of the type Text.

For details, refer to the relevant sections in the Utilities documentation.

## Blacklist Maintenance in Batch Mode

SYSBPM blacklist maintenance functions can also be executed in batch mode as described in Batch Processing.

In addition, the Natural system library SYSBPM provides the command `BPMBLBAT` that further facilitates batch processing of the blacklist maintenance functions add and delete all objects.

Log on to the library SYSBPM and execute the `BPMBLBAT` command using the syntax indicated in the diagram below. The symbols used in the diagram are explained in the section System Command Syntax in the System Commands documentation.

`BPMBLBAT` |  | `FUNC=LOCK, BPNAME=`bp-name, (object-specification) |
`FUNC=RLS, BPNAME=`bp-name

This section covers the following topics:

- Explanation of Syntax

- Examples of Input

### Explanation of Syntax

The keywords and the object-specification clause indicated in the `BPMBLBAT` syntax diagram above are described in the following section. Examples of Input demonstrate the use of the keywords.

Syntax Item | Explanation
--- | ---
`FUNC=LOCK` | Adds object names to a blacklist as described in Adding Objects in the section Maintain Blacklist.
`FUNC=RLS` | Deletes a complete blacklist with all object names contained in the list. This functions corresponds to delete function described under To delete all objects from the blacklist in the section Maintain Blacklist. (In batch mode, you cannot delete single object names from a blacklist.)
`BPNAME` | The name of the buffer pool where the blacklist is loaded.
object-specification |
The keywords that apply to the object-specification clause (see the respective syntax below) are:
`LIB` | The name of the library where the objects are stored.
`DBID` `FNR` | The database ID (DBID) and the file number (FNR) where the objects are stored. If DBID and FNR are left blank, they will be taken from the current system file FUSER or FNAT in libraries whose names start with SYS (except the library SYSTEM).
object-name | The name(s) of the object(s) to be added to the blacklist: Enter each name in a separate line in the positions 1 to 8. To indicate the end of the input, in a separate line, enter a period (.)

#### Syntax of object-specification

Shown and explained below is the syntax that applies to object-specification:

`LIB=`lib-name, `DBID` dbid, `FNR` fnr [object-name]...

### Examples of Input

#### Example 1 - Adding Objects to a Blacklist

The example input below demonstrates how to add to a blacklist the objects `A`, `B` and `C` in the buffer pool `NATGBP`:

    /*Job
    .
    .
    .
    */Job

    LOGON SYSBPM
    BPMBLBAT
    FUNC=LOCK,BPNAME=NATGBP,LIB=SAGTEST,DBID=10,FNR=32
    A
    B
    C
    .
    FIN

#### Example 2 - Deleting a Blacklist:

The example input below demonstrates how to delete a blacklist in the buffer pool `NATGBP`:

    /*Job
    .
    .
    .
    */Job
    LOGON SYSBPM
    BPMBLBAT
    FUNC=RLS,BPNAME=NATGBP
    .
    FIN

### On this page

- Maintain Blacklist
- List Object Sets
- Edit Object Set
- Add Object Set to Blacklist
- Delete Object Set from Blacklist
- Delete Object Set Source Object
- Additional Object Set Maintenance with Utilities
- Blacklist Maintenance in Batch Mode