SD - Time Delay between Two Screens

#### Search Results

Search

# SD - Time Delay between Two Screens

This Natural profile parameter can be used to delay the time related to screen output display. This is the time delay between two screens during a non-conversational write operation (see the Natural terminal command `%N`).

Possible settings | `1 - 100` | The unit for the specified setting is a tenth of a second, which means that `SD=10` leads to a delay of one second.
`0`
Default setting | `0` |
Dynamic specification | no |
Specification within session | no |