CVMIN - Control Variable Modified at Input

#### Search Results

Search

# CVMIN - Control Variable Modified at Input

This Natural profile parameter determines whether or not an attribute control variable is assigned the status `MODIFIED` when the setting of the field to which the attribute control variable is attached is overwritten by an identical setting.

Possible settings | `ON` | If a field setting is overwritten by the same setting, the corresponding control variable will be assigned the status `MODIFIED`.
`OFF` | If a field setting is overwritten by the same setting, the corresponding control variable will not be assigned the status `MODIFIED`.
Default setting | `OFF` |
Dynamic specification | yes |
Specification within session | no |

Note
If an attribute control variable has been assigned the status `MODIFIED`, the `MODIFIED` option evaluates this as `TRUE`. This applies regardless of whether the input was entered manually, read from the stack or supplied in batch mode.