Sample File Definition

#### Search Results

Search

# Sample File Definition

The following file definition was used for generating the sample output for the following external object types:

- ADACMP, ADAWAN or ADAFDU definitions

- Adabas files

- ADAINV definitions

- ADASCR definitions

- Vista translator table

- DDM

- Assembler copy code

- C include Code

- COBOL copy code

- FORTRAN copy code

- PL/I include Code

Note
The file definition used for generating a DB2 table or an Adabas VSAM Bridge transparency table are given in the corresponding sections of this documentation.

    File ID ............ * GENERATION-EXAMPLE
    Type ............... Adabas, Simple file
    File number ........ 231                      Added 2007-05-31 at 13:30 by BOE
                                               Modified 2007-05-31 at 13:35 by HNO
                                        Fields modified 2007-05-31 at 13:37 by CHD
    ------------------------------------------------------------------------------

    File attributes
      Sequence field ..........
      Log. distribution type .. Simple file
      Adabas SQL usage ........ N

    Vista
      L-DBnr .................. 3
      L-Fnr ................... 241

    Abstract
      Example file for the
      Predict generation subsystem.
      ..

    File ID ............ * GENERATION-EXAMPLE
    ------------------------------------------------------------------------------

    Adabas attributes
      Required attributes                         Added 2007-05-31 at 13:30 by BOE
        Phys. file number ..... 231            Modified 2007-05-31 at 13:35 by CHD
        Min ISN ............... 1
        Max ISN ............... 3391

      Loading attributes                             Loading attributes
        Max recl ..............                        One AC extent .... N
        ISN reusage ........... N                      DS reusage ....... Y
        User ISN .............. N                      Mixed DS device .. N
        Ciphered .............. N                      Mirror ........... N
        LOWNERID ..............
        Refresh from program .. N
        Automatic allocation .. Y
        PLOG .................. Y
        ISN SIZE .............. 0 Adabas decides

     Adabas security definition
       Access level ... 2
       Update level ... 3

     Extend allocation
             Device    Padding factor     Cylinder    Blocks    Max 2. Alloc
       Asso  3390            10        UI             41
                                       NI             80
       Data  3390            10        DS   > 1       233

                      --------------- Generation ---------------
    Generation status              on      DBnr       Fnr   Warnings
    NATURAL DDM GENERATED     2007-05-31   180        171   NATURAL DDM GENERATED
    VERIFIC. RULE GENERATED   2007-05-31   180        171   VERIFIC. RULE GENERATED

     Cnt  Ty L Field ID                         F    Length   Occ D DB S
        1 GR 1 GROUP-1                                              AA
        2    2 ELE-N-9V5                        N      9.5          AB N
               Specifications for 3GL
                 Initialize with .... Z    Zero
               Field synonyms
                 BAL/Assembler ....... ELN9V5
                 FORTRAN ............. ELN9V5
               Verification name
                 GEN-CHECK-ZERO
        3 GR 2 GR-IN-GROUP                                          AC
               Field synonyms
                 BAL/Assembler ....... GR-IN-GR
        4    3 ELE-B-4                          B      4.0        D AD F
              Specifications for 3GL
                Init value ......... 00001111
              Condition name
                INIT-ELE-B-4
                : Condition value
                :   00001000
                COND-ELE-B-4-V-1
                : Condition value
                :   FFFFFFFF
              Verification name
                GEN-VER-EXAM
       5    3 ELE-PS-5V2                       PS     5.2          AE N
              Specifications for 3GL
                Initialize with .... Z    Zero
              Field synonyms
                BAL/Assembler ....... ELPS52
                FORTRAN ............. ELPS52
              Verification name
                GEN-CHECK-ZERO
       6 MU 3 MU-B-4                           B      4.0      5   AF N
       7 RE 3 MU-B-4
       8    4 MU-RED-B-7                       B      7.0
              Field synonyms
                BAL/Assembler ....... MURB7
                FORTRAN ............. MURB7
       9    4 MU-RED-US-13                     US    13.0
              Field synonyms
                BAL/Assembler ....... MURB13
                FORTRAN ............. MURB13
      10 RE 3 MU-B-4
      11    4 MU-RED-B-8                       B      8.0
              Condition name
                MU-RED-B-8-COND1
                : Condition value
                :   111111
              Field synonyms
                BAL/Assembler ....... MURB8
                FORTRAN ............. MURB8
      12    2 ELE-A-42                         A     42.0          AG N
              Specifications for 3GL
                Initialize with .... H    High-value
              Condition name
                COND-NAME-START
                : Condition value
                :   COND-START
                :  THRU
                :   COND-ZEND
                FILL-WITH-STRING
                : Condition value
                :   A
              Verification name
                GEN-CHECK-BLANK
                GEN-VER-EXAM
      13    2 ELE-F-8                          F      8.0          AH F
      14    2 ELE-B-3                          B      3.0          AI N
               Field synonyms
                FORTRAN ............. FOB3
      15 SB 1 SB-ELE-A-5                       A      5.0          AJ N
              Source field(s)                   Start    End       DB
              ELE-A-42                            10      14       AG(10-14)
              Field synonyms
                BAL/Assembler ....... SBB5
                FORTRAN ............. SBB5
      16 SP 1 SP-DE-A-24                       A     24.0        D S1 N
              Source field(s)                   Start    End       DB
              ELE-B-3                                              AI(1-3)
              ELE-A-42                            20      36       AG(20-36)
              ELE-PS-5V2                                           AE(1-4)
              Field synonyms
                BAL/Assembler ....... SPDA24
                FORTRAN ............. SPDA24
      17 PC 1 PC-OCC-7                                         7   AL
      18    2 PC-ELE-DE-NS-7V3                 NS     7.3        D AM N
              Field synonyms
                BAL/Assembler ....... PCNS7V3
      19 MC 2 PC-MC-PS-6V1                     PS     6.1     11 D AN N
              Field synonyms
                BAL/Assembler ....... PCMCPS
                FORTRAN ............. MCPS
              Verification name
                GEN-CHECK-ZERO
      20 GR 2 PC-GR                                                AO
      21    3 PC-ELE-I-2                       I      2.0          AP F
              Field synonyms
                BAL/Assembler ....... BALI2
                FORTRAN ............. FOI2
      22    3 PC-PS-20V7                       PS    20.7          AQ N
              Field synonyms
                BAL/Assembler ....... PCPS20V7
                FORTRAN ............. PS20V7
      23    2 PC-ELE-F-4                       F      4.0          AR F
              Field synonyms
                BAL/Assembler ....... BALF4
                FORTRAN ............. FOF4
      24    1 ELE-D                            D                   AS N
      25    1 ELE-T                            T                   AT N
      26    1 ELE-L                            L                   AU N
      27 HQ 1 HQ-DE-I-4                        I      4.0        D S2
              Source field(s)                                      DB
              PC-ELE-I-2                                           AP
              MU-B-4                                               AF

    *** End of report ***