Migrating to this Entire Net-Work Version

#### Search Results

Search

# Migrating to this Entire Net-Work Version

The architectural changes for this version of Entire Net-Work enhance the functionality already introduced in Entire Net-Work 7.2 and later releases and are described in Entire Net-Work 7.6 Release Notes. We also recommend you read the following sections:

- Architectural Changes Introduced in Entire Net-Work 7.2

- Planning Steps for Entire Net-Work 7

- Frequently Asked Questions for Entire Net-Work 7.2

To migrate from Entire Net-Work versions later than 7.2 to Entire Net-Work 7.6, you need to install 7.6 and then migrate your earlier Entire Net-Work nodes (Kernels) to Entire Net-Work 7.6 Kernel configuration definitions. For complete information, read Migrating Kernel Configurations from Prior Releases.

To migrate from earlier Entire Net-Work Client versions to Entire Net-Work Client 1.6, you need to install 1.6 and then migrate your earlier Entire Net-Work Client client configurations to Entire Net-Work Client 1.6 client configuration definitions. For complete information, read Migrating Entire Net-Work Client Configurations from Prior Releases.

| Warning: Once a Kernel configuration has been migrated to 7.6, it cannot be migrated back to any earlier version. If you really need to do so, contact your technical support representative for assistance. Once a client configuration has been migrated to 1.6, it cannot be migrated back to any earlier version; there is no procedure to do so.

The user exits you used in past releases are still valid and supported by Entire Net-Work 7.6. No user exit code changes are necessary, however, you must rebuild and recompile any existing user exits into the Entire Net-Work 7.6 installation library so they will be recognized by Entire Net-Work 7.6.

Note
When you install Entire Net-Work 7.6 on a Windows system running an older version of Entire Net-Work, the older Entire Net-Work installation is automatically uninstalled. However, on Linux systems, the older Entire Net-Work installation must be removed manually.